Adams Car Assembly (Adams 2017)
!Adams Car suspension assembly
!nastrelene hardpointy na prve simulacie
!END OF MODEL COMMENTS
!
!-------------------------------- SYSTEM UNITS ---------------------------------
!
UNITS/
, FORCE = NEWTON
, MASS = KILOGRAM
, LENGTH = MILLIMETER
, TIME = SECOND
!
!----------------------------------- PARTS -------------------------------------
!
!----------------------------------- Ground ------------------------------------
!
!                            adams_view_name='ground'
PART/1
, GROUND
!
!                            adams_view_name='origo'
MARKER/1
, PART = 1
!
!Dummy for communicators
!                          adams_view_name='_cv_marker'
MARKER/2
, PART = 1
!
!                        adams_view_name='jxl_joint_j_2'
MARKER/3
, PART = 1
, QP = -0.0025116527, -837.8781412, -649.8024417
!
!                       adams_view_name='jfl_actuator_j_1'
MARKER/4
, PART = 1
, QP = -0.0025116527, -837.8781412, -649.8024417
, REULER = 0D, 180D, 0D
!
!                     adams_view_name='rel_reboundstop_j_1'
MARKER/5
, PART = 1
, QP = -0.0025116527, -837.8781412, -329.8024417
!
!                       adams_view_name='jml_actuator_j_2'
MARKER/6
, PART = 1
, QP = -0.0025116527, -837.8781412, -649.8024417
!
!                       adams_view_name='jfl_actuator_j_2'
MARKER/7
, PART = 1
, QP = -0.0025116527, -837.8781412, -649.8024417
!
!                        adams_view_name='jxr_joint_j_2'
MARKER/8
, PART = 1
, QP = -0.0025116527, 837.8781412, -649.8024417
!
!                       adams_view_name='jfr_actuator_j_1'
MARKER/9
, PART = 1
, QP = -0.0025116527, 837.8781412, -649.8024417
, REULER = 0D, 180D, 0D
!
!                     adams_view_name='rer_reboundstop_j_1'
MARKER/10
, PART = 1
, QP = -0.0025116527, 837.8781412, -329.8024417
!
!                       adams_view_name='jmr_actuator_j_2'
MARKER/11
, PART = 1
, QP = -0.0025116527, 837.8781412, -649.8024417
!
!                       adams_view_name='jfr_actuator_j_2'
MARKER/12
, PART = 1
, QP = -0.0025116527, 837.8781412, -649.8024417
!
!                        adams_view_name='jxl_joint_j_3'
MARKER/13
, PART = 1
, QP = 30, -321, 0
, REULER = 0D, 90D, 0D
!
!                        adams_view_name='jxr_joint_j_3'
MARKER/14
, PART = 1
, QP = 30, 321, 0
, REULER = 180D, 90D, 180D
!
!                        adams_view_name='jxs_joint_j_8'
MARKER/15
, PART = 1
, QP = 17, 0, -94.5
!
!                       adams_view_name='bxl_bushing_j_3'
MARKER/16
, PART = 1
, QP = -400, -450, -120
!
!                       adams_view_name='bxr_bushing_j_3'
MARKER/17
, PART = 1
, QP = -400, 450, -120
!
!                       adams_view_name='bxl_bushing_j_4'
MARKER/18
, PART = 1
, QP = 400, -450, -120
!
!                       adams_view_name='bxr_bushing_j_4'
MARKER/19
, PART = 1
, QP = 400, 450, -120
!
!                       adams_view_name='bxl_bushgeom_j_3'
MARKER/20
, PART = 1
, QP = -400, -450, -130
!
!                       adams_view_name='bxr_bushgeom_j_3'
MARKER/21
, PART = 1
, QP = -400, 450, -130
!
!                       adams_view_name='bxl_bushgeom_j_4'
MARKER/22
, PART = 1
, QP = 400, -450, -130
!
!                       adams_view_name='bxr_bushgeom_j_4'
MARKER/23
, PART = 1
, QP = 400, 450, -130
!
!                        adams_view_name='jxl_joint_j_12'
MARKER/24
, PART = 1
, QP = 7.167, -465.435, 511.534
, REULER = 260.759132D, 180D, 0D
!
!                        adams_view_name='nsl_spring_i_1'
MARKER/26
, PART = 1
, QP = 7.167, -465.435, 511.534
!
!                        adams_view_name='jxr_joint_j_12'
MARKER/28
, PART = 1
, QP = 7.167, 465.435, 511.534
, REULER = 99.24086798D, 180D, 0D
!
!                        adams_view_name='nsr_spring_i_1'
MARKER/30
, PART = 1
, QP = 7.167, 465.435, 511.534
!
!                        adams_view_name='jxl_joint_j_15'
MARKER/32
, PART = 1
, QP = -9.75, -440, 383.5
, REULER = 270D, 87.10787264D, 90D
!
!                        adams_view_name='jxr_joint_j_15'
MARKER/37
, PART = 1
, QP = -9.75, 440, 383.5
, REULER = 270D, 87.10787264D, 90D
!
!                        adams_view_name='jxs_joint_j_11'
MARKER/42
, PART = 1
, QP = 975, -350, 800
, REULER = 90D, 58.31363231D, 90D
!
!                        adams_view_name='jxs_joint_j_13'
MARKER/43
, PART = 1
, QP = 889.906389, -350, 747.4730796
, REULER = 90D, 58.31363231D, 0D
!
!                        adams_view_name='sws_switch_j_1'
MARKER/44
, PART = 1
, QP = -70, 0, -20
!
!                   adams_view_name='steering_column_housing'
GRAPHICS/79
, CYLINDER
, CM = 43
, LENGTH = -237.9732128
, RADIUS = 35
!
!                          adams_view_name='_cv_csolid'
GRAPHICS/83
, ELLIPSOID
, CM = 2
, XSCALE = 100
, YSCALE = 100
, ZSCALE = 100
!
!                        adams_view_name='testrig_origo'
MARKER/46
, PART = 1
!
!Dummy for communicators
!                      adams_view_name='testrig__cv_marker'
MARKER/47
, PART = 1
!
!                    adams_view_name='testrig_cfl_spin_axis'
MARKER/48
, PART = 1
, QP = 0, -835, 0
, REULER = 359.95D, 89.5D, 0D
!
!                    adams_view_name='testrig_cfr_spin_axis'
MARKER/49
, PART = 1
, QP = 0, 835, 0
, REULER = 180.05D, 89.5D, 180D
!
!               adams_view_name='testrig_cfl_wheel_contact_point'
MARKER/52
, PART = 1
, QP = -0.0025116527, -837.8781412, -329.8024417
, REULER = 89.95D, 0D, 0D
!
!               adams_view_name='testrig_cfr_wheel_contact_point'
MARKER/53
, PART = 1
, QP = -0.0025116527, 837.8781412, -329.8024417
, REULER = 90.05D, 0D, 0D
!
!                     adams_view_name='testrig_cfl_jack_ref'
MARKER/54
, PART = 1
, QP = -0.0025116527, -837.8781412, -649.8024417
!
!                     adams_view_name='testrig_cfr_jack_ref'
MARKER/55
, PART = 1
, QP = -0.0025116527, 837.8781412, -649.8024417
!
!Global Reference Frame for Parts
!              adams_view_name='testrig_cfs_global_part_reference'
MARKER/58
, PART = 1
!
!              adams_view_name='testrig_cfs_steering_input_slider'
MARKER/59
, PART = 1
, QP = 200, 0, 0
!
!                    adams_view_name='testrig_jxs_joint_j_1'
MARKER/60
, PART = 1
, QP = 200, 0, 0
!
!                    adams_view_name='testrig_jxs_joint_j_2'
MARKER/61
, PART = 1
, QP = 200, 0, 0
!
!Origo's y-axis
!                       adams_view_name='testrig_origo_y'
MARKER/62
, PART = 1
, REULER = 180D, 90D, 180D
!
!                    adams_view_name='testrig_jxs_joint_j_3'
MARKER/63
, PART = 1
, QP = 200, -200, 0
!
!                    adams_view_name='testrig_jxs_joint_j_4'
MARKER/64
, PART = 1
, QP = 200, 200, 0
!
!               adams_view_name='testrig_cfl_differential_output'
MARKER/65
, PART = 1
, QP = 30, -321, 0
, REULER = 0D, 90D, 0D
!
!               adams_view_name='testrig_cfr_differential_output'
MARKER/66
, PART = 1
, QP = 30, 321, 0
, REULER = 180D, 90D, 180D
!
!                  adams_view_name='FRT_SUSP_cfl_lca_outer_ref'
MARKER/181
, PART = 1
, QP = -14.416, -656.659835, -99.82
!
!                  adams_view_name='FRT_SUSP_cfr_lca_outer_ref'
MARKER/182
, PART = 1
, QP = -14.416, 656.659835, -99.82
!
!                 adams_view_name='FRT_SUSP_cfl_hub_compliance'
MARKER/183
, PART = 1
, QP = 0, -835, 0
, REULER = 359.95D, 89.5D, 0D
!
!                 adams_view_name='FRT_SUSP_cfr_hub_compliance'
MARKER/184
, PART = 1
, QP = 0, 835, 0
, REULER = 180.05D, 89.5D, 180D
!
!                  adams_view_name='FRT_SUSP_afr_aforce_meaj_2'
MARKER/185
, PART = 1
!
!                  adams_view_name='FRT_SUSP_afl_aforce_meaj_2'
MARKER/186
, PART = 1
!
!                    adams_view_name='FRT_SUSP_cfl_lca_outer'
MARKER/187
, PART = 1
, QP = -14.416, -791.843, -99.82
, REULER = 180D, 90D, 180D
!
!                    adams_view_name='FRT_SUSP_cfr_lca_outer'
MARKER/188
, PART = 1
, QP = -14.416, 791.843, -99.82
, REULER = 0D, 90D, 0D
!
!                  adams_view_name='FRT_SUSP_cfl_tierod_middle'
MARKER/189
, PART = 1
, QP = -122.635, -602.75, -41.635
, REULER = 353.2905617D, 90.33422447D, 92.8387371D
!
!                  adams_view_name='FRT_SUSP_cfr_tierod_middle'
MARKER/190
, PART = 1
, QP = -122.635, 602.75, -41.635
, REULER = 186.7094383D, 90.33422447D, 87.1612629D
!
!                        adams_view_name='FRT_SUSP_origo'
MARKER/191
, PART = 1
!
!                  adams_view_name='FRT_SUSP_cfl_wheel_center'
MARKER/192
, PART = 1
, QP = 0, -835, 0
, REULER = 359.95D, 89.5D, 0D
!
!                  adams_view_name='FRT_SUSP_cfr_wheel_center'
MARKER/193
, PART = 1
, QP = 0, 835, 0
, REULER = 180.05D, 89.5D, 180D
!
!                  adams_view_name='FRT_SUSP_cfl_lwr_strut_ext'
MARKER/194
, PART = 1
, QP = -24, -657, -149.8
!
!                  adams_view_name='FRT_SUSP_cfr_lwr_strut_ext'
MARKER/195
, PART = 1
, QP = -24, 657, -149.8
!
!                  adams_view_name='FRT_SUSP_cfl_top_mount_ext'
MARKER/196
, PART = 1
, QP = 7.167, -465.435, 561.534
!
!                  adams_view_name='FRT_SUSP_cfr_top_mount_ext'
MARKER/197
, PART = 1
, QP = 7.167, 465.435, 561.534
!
!                 adams_view_name='FRT_SUSP_cfs_subframe_fixed'
MARKER/198
, PART = 1
, QP = 17, 0, -94.5
!
!Dummy for communicators
!                     adams_view_name='FRT_SUSP__cv_marker'
MARKER/204
, PART = 1
!
!Attachment point of ARM to suspension, position is defined in ARB subsystem
!                   adams_view_name='FRT_SUSP_cfr_ARB_pickup'
MARKER/207
, PART = 1
, QP = -50, 700, 350
!
!Attachment point of ARM to suspension, position is defined in ARB subsystem
!                   adams_view_name='FRT_SUSP_cfl_ARB_pickup'
MARKER/208
, PART = 1
, QP = -50, -700, 350
!
!                 adams_view_name='FRT_SUSP_cfr_lwr_spring_seat'
MARKER/209
, PART = 1
, QP = -8.4165, 561.2175, 205.867
!
!                 adams_view_name='FRT_SUSP_cfl_lwr_spring_seat'
MARKER/210
, PART = 1
, QP = -8.4165, -561.2175, 205.867
!
!                 adams_view_name='FRT_SUSP_cfr_drive_shaft_otr'
MARKER/211
, PART = 1
, QP = 0.0654473465, 760.0028843, -0.6544901624
, REULER = 180.05D, 89.5D, 174.2893334D
!
!                 adams_view_name='FRT_SUSP_cfl_drive_shaft_otr'
MARKER/212
, PART = 1
, QP = 0.0654473465, -760.0028843, -0.6544901624
, REULER = 359.95D, 89.5D, 5.71066658D
!
!                 adams_view_name='FRT_SUSP_cfr_drive_shaft_inr'
MARKER/213
, PART = 1
, QP = 30, 321, 0
, REULER = 0D, 90D, 181.2525175D
!
!                 adams_view_name='FRT_SUSP_cfl_drive_shaft_inr'
MARKER/214
, PART = 1
, QP = 30, -321, 0
, REULER = 180D, 90D, 358.7474825D
!
!               adams_view_name='FRT_SUSP_cfl_upright_spindle_inr'
MARKER/217
, PART = 1
, QP = 0.0654473465, -760.0028843, -0.6544901624
, REULER = 359.95D, 89.5D, 0D
!
!               adams_view_name='FRT_SUSP_cfr_upright_spindle_inr'
MARKER/218
, PART = 1
, QP = 0.0654473465, 760.0028843, -0.6544901624
, REULER = 180.05D, 89.5D, 180D
!
!                adams_view_name='FRT_SUSP_cfl_lca_front_middle'
MARKER/219
, PART = 1
, QP = -108.708, -590.9215, -102.41
!
!                adams_view_name='FRT_SUSP_cfr_lca_front_middle'
MARKER/220
, PART = 1
, QP = -108.708, 590.9215, -102.41
!
!                 adams_view_name='FRT_SUSP_cfl_lca_rear_middle'
MARKER/221
, PART = 1
, QP = 111.292, -590.9215, -91.91
!
!                 adams_view_name='FRT_SUSP_cfr_lca_rear_middle'
MARKER/222
, PART = 1
, QP = 111.292, 590.9215, -91.91
!
!                  adams_view_name='FRT_SUSP_afl_aforce_meaj_1'
MARKER/223
, PART = 1
!
!                  adams_view_name='FRT_SUSP_afr_aforce_meaj_1'
MARKER/224
, PART = 1
!
!                  adams_view_name='FRT_SUSP_cfl_lwr_strut_loc'
MARKER/225
, PART = 1
, QP = -24, -657, -99.8
!
!                  adams_view_name='FRT_SUSP_cfr_lwr_strut_loc'
MARKER/226
, PART = 1
, QP = -24, 657, -99.8
!
!                   adams_view_name='MDI_FRONT_STEERING_origo'
MARKER/494
, PART = 1
!
!         adams_view_name='MDI_FRONT_STEERING_cfs_steering_wheel_center'
MARKER/495
, PART = 1
, QP = 975, -350, 800
, REULER = 270D, 121.6863677D, 90D
!
!             adams_view_name='MDI_FRONT_STEERING_cfs_pinion_pivot'
MARKER/496
, PART = 1
, QP = -70, -300, -20
, REULER = 83.92754359D, 59.35741874D, 273.1036171D
!
!              adams_view_name='MDI_FRONT_STEERING_cfs_rack_mount'
MARKER/497
, PART = 1
, QP = -70, 0, -20
, REULER = 180D, 90D, 180D
!
!Dummy for communicators
!                adams_view_name='MDI_FRONT_STEERING__cv_marker'
MARKER/500
, PART = 1
!
!        adams_view_name='MDI_FRONT_STEERING_cfs_steering_column_to_body'
MARKER/501
, PART = 1
, QP = 889.906389, -350, 747.4730796
, REULER = 270D, 121.6863677D, 90D
!
!------------------------------------ Part -------------------------------------
!
!Dummy for communicators
!                           adams_view_name='_cv_part'
PART/2
, CM = 45
, IP = 0, 0, 0
!
!Dummy for communicators
!                            adams_view_name='marker'
MARKER/45
, PART = 2
!
!------------------------------------ Part -------------------------------------
!
!                      adams_view_name='testrig.whl_wheel'
PART/4
, QG = 0, -835, 0
, REULER = 359.95D, 89.5D, 0D
, MASS = 20
, CM = 74
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/74
, PART = 4
!
!                            adams_view_name='tire_i'
MARKER/75
, PART = 4
, REULER = 180D, 90D, 0D
!
!                           adams_view_name='geo_ctr'
MARKER/76
, PART = 4
, QP = 0, 0, -20.778345
!
!                           adams_view_name='geo_inr'
MARKER/77
, PART = 4
, QP = 0, 0, -103.891725
, REULER = 0D, 180D, 0D
!
!                           adams_view_name='geo_otr'
MARKER/78
, PART = 4
, QP = 0, 0, 103.891725
!
!                        adams_view_name='jxl_joint_i_1'
MARKER/79
, PART = 4
!
!                       adams_view_name='jml_actuator_i_1'
MARKER/80
, PART = 4
!
!                          adams_view_name='wheel_hub'
GRAPHICS/5
, CYLINDER
, CM = 76
, LENGTH = 41.55669
, RADIUS = 192.941775
!
!                          adams_view_name='wheel_rim'
GRAPHICS/6
, CYLINDER
, CM = 77
, LENGTH = -207.78345
, RADIUS = 192.941775
, SEG = 0
!
!                          adams_view_name='tire_tread'
GRAPHICS/7
, CYLINDER
, CM = 77
, LENGTH = -207.78345
, RADIUS = 329.815
, SEG = 0
!
!                         adams_view_name='wheel_inner1'
GRAPHICS/101
, FRUSTUM
, CM = 77
, LENGTH = 0
, SIDES = 20
, TOP = 192.941775
, BOTTOM = 225.923275
, SEG = 0
!
!                         adams_view_name='wheel_outer1'
GRAPHICS/102
, FRUSTUM
, CM = 78
, LENGTH = 0
, SIDES = 20
, TOP = 192.941775
, BOTTOM = 225.923275
, SEG = 0
!
!                        adams_view_name='tire_sidewall1'
GRAPHICS/103
, FRUSTUM
, CM = 77
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 225.923275
, SEG = 0
!
!                        adams_view_name='tire_sidewall2'
GRAPHICS/104
, FRUSTUM
, CM = 77
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 329.815
, SEG = 0
!
!                        adams_view_name='tire_sidewall3'
GRAPHICS/105
, FRUSTUM
, CM = 78
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 225.923275
, SEG = 0
!
!                        adams_view_name='tire_sidewall4'
GRAPHICS/106
, FRUSTUM
, CM = 78
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 329.815
, SEG = 0
!
!------------------------------------ Part -------------------------------------
!
!                      adams_view_name='testrig.whr_wheel'
PART/5
, QG = 0, 835, 0
, REULER = 180.05D, 89.5D, 180D
, MASS = 20
, CM = 81
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/81
, PART = 5
!
!                            adams_view_name='tire_i'
MARKER/82
, PART = 5
, REULER = 0D, 90D, 180D
!
!                           adams_view_name='geo_ctr'
MARKER/83
, PART = 5
, QP = 0, 0, -20.778345
!
!                           adams_view_name='geo_inr'
MARKER/84
, PART = 5
, QP = 0, 0, -103.891725
, REULER = 0D, 180D, 0D
!
!                           adams_view_name='geo_otr'
MARKER/85
, PART = 5
, QP = 0, 0, 103.891725
!
!                        adams_view_name='jxr_joint_i_1'
MARKER/86
, PART = 5
!
!                       adams_view_name='jmr_actuator_i_1'
MARKER/87
, PART = 5
, REULER = 0D, 180D, 0D
!
!                          adams_view_name='wheel_hub'
GRAPHICS/8
, CYLINDER
, CM = 83
, LENGTH = 41.55669
, RADIUS = 192.941775
!
!                          adams_view_name='wheel_rim'
GRAPHICS/9
, CYLINDER
, CM = 84
, LENGTH = -207.78345
, RADIUS = 192.941775
, SEG = 0
!
!                          adams_view_name='tire_tread'
GRAPHICS/10
, CYLINDER
, CM = 84
, LENGTH = -207.78345
, RADIUS = 329.815
, SEG = 0
!
!                         adams_view_name='wheel_inner1'
GRAPHICS/107
, FRUSTUM
, CM = 84
, LENGTH = 0
, SIDES = 20
, TOP = 192.941775
, BOTTOM = 225.923275
, SEG = 0
!
!                         adams_view_name='wheel_outer1'
GRAPHICS/108
, FRUSTUM
, CM = 85
, LENGTH = 0
, SIDES = 20
, TOP = 192.941775
, BOTTOM = 225.923275
, SEG = 0
!
!                        adams_view_name='tire_sidewall1'
GRAPHICS/109
, FRUSTUM
, CM = 84
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 225.923275
, SEG = 0
!
!                        adams_view_name='tire_sidewall2'
GRAPHICS/110
, FRUSTUM
, CM = 84
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 329.815
, SEG = 0
!
!                        adams_view_name='tire_sidewall3'
GRAPHICS/111
, FRUSTUM
, CM = 85
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 225.923275
, SEG = 0
!
!                        adams_view_name='tire_sidewall4'
GRAPHICS/112
, FRUSTUM
, CM = 85
, LENGTH = 25.97293125
, SIDES = 20
, TOP = 277.8691375
, BOTTOM = 329.815
, SEG = 0
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!                      adams_view_name='testrig.gel_table'
PART/8
, QG = -0.0025116527, -837.8781412, -329.8024417
, MASS = 1
, CM = 91
, IM = 92
, IP = 1, 1, 1
!
!                        adams_view_name='til_tire_ref_1'
MARKER/90
, PART = 8
!
!                              adams_view_name='cm'
MARKER/91
, PART = 8
!
!                        adams_view_name='inertia_frame'
MARKER/92
, PART = 8
!
!                          adams_view_name='mal_geomar'
MARKER/93
, PART = 8
, REULER = 89.95D, 0D, 0D
!
!                        adams_view_name='jxl_joint_i_4'
MARKER/94
, PART = 8
, REULER = 90D, 90D, 0D
!
!                        adams_view_name='jxl_joint_i_5'
MARKER/95
, PART = 8
!
!                        adams_view_name='jxs_joint_i_6'
MARKER/96
, PART = 8
!
!                        adams_view_name='jxs_joint_j_5'
MARKER/97
, PART = 8
, QP = 0, 1675.756282, 0
!
!                       adams_view_name='cfl_table_origo'
MARKER/98
, PART = 8
!
!                   adams_view_name='cfs_road_reference_frame'
MARKER/99
, PART = 8
, QP = 0, 837.8781412, 0
!
!                         adams_view_name='til_tire_j_1'
MARKER/100
, PART = 8
, FLOATING
!
!                        adams_view_name='til_tire_ref_2'
MARKER/101
, PART = 8
, QP = -0.2617893861, -299.9884627, 2.61796065
!
!                         adams_view_name='til_tire_j_2'
MARKER/102
, PART = 8
, FLOATING
!
!                          adams_view_name='table_geo'
GRAPHICS/11
, CYLINDER
, CM = 93
, LENGTH = -20
, RADIUS = 263.852
!
!------------------------------------ Part -------------------------------------
!
!                      adams_view_name='testrig.ger_table'
PART/9
, QG = -0.0025116527, 837.8781412, -329.8024417
, MASS = 1
, CM = 104
, IM = 105
, IP = 1, 1, 1
!
!                        adams_view_name='tir_tire_ref_1'
MARKER/103
, PART = 9
!
!                              adams_view_name='cm'
MARKER/104
, PART = 9
!
!                        adams_view_name='inertia_frame'
MARKER/105
, PART = 9
!
!                          adams_view_name='mar_geomar'
MARKER/106
, PART = 9
, REULER = 90.05D, 0D, 0D
!
!                        adams_view_name='jxr_joint_i_4'
MARKER/107
, PART = 9
, REULER = 90D, 90D, 180D
!
!                        adams_view_name='jxr_joint_i_5'
MARKER/108
, PART = 9
!
!                        adams_view_name='jxs_joint_i_5'
MARKER/109
, PART = 9
!
!                       adams_view_name='cfr_table_origo'
MARKER/110
, PART = 9
!
!                   adams_view_name='cfs_road_reference_frame'
MARKER/111
, PART = 9
, QP = 0, -837.8781412, 0
!
!                        adams_view_name='jxs_joint_j_6'
MARKER/112
, PART = 9
, QP = 0, -1675.756282, 0
!
!                         adams_view_name='tir_tire_j_1'
MARKER/113
, PART = 9
, FLOATING
!
!                        adams_view_name='tir_tire_ref_2'
MARKER/114
, PART = 9
, QP = -0.2617893861, 299.9884627, 2.61796065
!
!                         adams_view_name='tir_tire_j_2'
MARKER/115
, PART = 9
, FLOATING
!
!                          adams_view_name='table_geo'
GRAPHICS/12
, CYLINDER
, CM = 106
, LENGTH = -20
, RADIUS = 263.852
!
!------------------------------------ Part -------------------------------------
!
!                       adams_view_name='testrig.gel_jack'
PART/10
, QG = -0.0025116527, -837.8781412, -649.8024417
, MASS = 1
, CM = 116
, IM = 117
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/116
, PART = 10
!
!                        adams_view_name='inertia_frame'
MARKER/117
, PART = 10
!
!                           adams_view_name='gracyl_1'
MARKER/118
, PART = 10
!
!                        adams_view_name='jxl_joint_i_2'
MARKER/119
, PART = 10
!
!                       adams_view_name='jfl_actuator_i_1'
MARKER/120
, PART = 10
!
!                        adams_view_name='jxl_joint_j_4'
MARKER/121
, PART = 10
, QP = 0, 0, 320
, REULER = 90D, 90D, 0D
!
!                        adams_view_name='jxl_joint_j_5'
MARKER/122
, PART = 10
, QP = 0, 0, 320
!
!                     adams_view_name='rel_reboundstop_i_1'
MARKER/123
, PART = 10
!
!                       adams_view_name='jml_actuator_i_2'
MARKER/124
, PART = 10
!
!                       adams_view_name='jfl_actuator_i_2'
MARKER/125
, PART = 10
!
!                       adams_view_name='gracyl_jack_geo'
GRAPHICS/13
, CYLINDER
, CM = 118
, LENGTH = 300
, SIDES = 15
, RADIUS = 98.11338
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!                       adams_view_name='testrig.ger_jack'
PART/11
, QG = -0.0025116527, 837.8781412, -649.8024417
, MASS = 1
, CM = 126
, IM = 127
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/126
, PART = 11
!
!                        adams_view_name='inertia_frame'
MARKER/127
, PART = 11
!
!                           adams_view_name='gracyl_2'
MARKER/128
, PART = 11
!
!                        adams_view_name='jxr_joint_i_2'
MARKER/129
, PART = 11
!
!                       adams_view_name='jfr_actuator_i_1'
MARKER/130
, PART = 11
!
!                        adams_view_name='jxr_joint_j_4'
MARKER/131
, PART = 11
, QP = 0, 0, 320
, REULER = 90D, 90D, 180D
!
!                        adams_view_name='jxr_joint_j_5'
MARKER/132
, PART = 11
, QP = 0, 0, 320
!
!                     adams_view_name='rer_reboundstop_i_1'
MARKER/133
, PART = 11
!
!                       adams_view_name='jmr_actuator_i_2'
MARKER/134
, PART = 11
!
!                       adams_view_name='jfr_actuator_i_2'
MARKER/135
, PART = 11
!
!                       adams_view_name='gracyl_jack_geo'
GRAPHICS/14
, CYLINDER
, CM = 128
, LENGTH = 300
, SIDES = 15
, RADIUS = 98.11338
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!Steering Input Controlled by Loadcase Input
!              adams_view_name='testrig.ges_steering_input_slider'
PART/15
, CM = 139
, IP = 0, 0, 0
!
!                              adams_view_name='cm'
MARKER/139
, PART = 15
, QP = 200, 0, 0
!
!                        adams_view_name='jxs_joint_i_1'
MARKER/140
, PART = 15
, QP = 200, 0, 0
!
!                       adams_view_name='jfs_actuator_i_1'
MARKER/141
, PART = 15
, QP = 200, 0, 0
!
!------------------------------------ Part -------------------------------------
!
!Steering Input Part Used for Compliance Matrix Calculations
!                  adams_view_name='testrig.ges_steering_part'
PART/16
, CM = 142
, IP = 0, 0, 0
!
!                              adams_view_name='cm'
MARKER/142
, PART = 16
, QP = 200, 0, 0
!
!                        adams_view_name='jxs_joint_i_2'
MARKER/143
, PART = 16
, QP = 200, 0, 0
!
!                       adams_view_name='jfs_actuator_j_1'
MARKER/144
, PART = 16
, QP = 200, 0, 0
, REULER = 0D, 180D, 0D
!
!------------------------------------ Part -------------------------------------
!
!Steering Input Controlled by Loadcase Input
!            adams_view_name='testrig.ges_steering_input_translation'
PART/17
, CM = 145
, IP = 0, 0, 0
!
!                              adams_view_name='cm'
MARKER/145
, PART = 17
, QP = 200, 0, 0
!
!                        adams_view_name='jxs_joint_i_3'
MARKER/146
, PART = 17
, QP = 200, -200, 0
!
!------------------------------------ Part -------------------------------------
!
!Steering Input Controlled by Loadcase Input
!             adams_view_name='testrig.ges_steering_input_rotation'
PART/18
, CM = 147
, IP = 0, 0, 0
!
!                              adams_view_name='cm'
MARKER/147
, PART = 18
, QP = 200, 0, 0
!
!                        adams_view_name='jxs_joint_i_4'
MARKER/148
, PART = 18
, QP = 200, 200, 0
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='testrig.gel_diff_output'
PART/19
, QG = 30, -321, 0
, REULER = 0D, 90D, 0D
, MASS = 2
, CM = 149
, IM = 150
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/149
, PART = 19
!
!                        adams_view_name='inertia_frame'
MARKER/150
, PART = 19
!
!                        adams_view_name='jxl_joint_i_3'
MARKER/151
, PART = 19
!
!                           adams_view_name='gracyl_3'
MARKER/152
, PART = 19
!
!                        adams_view_name='jxl_joint_j_17'
MARKER/153
, PART = 19
, REULER = 181.2525175D, 180D, 0D
!
!                      adams_view_name='gracyl_diff_output'
GRAPHICS/15
, CYLINDER
, CM = 152
, LENGTH = 40
, SIDES = 15
, RADIUS = 50
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='testrig.ger_diff_output'
PART/20
, QG = 30, 321, 0
, REULER = 180D, 90D, 180D
, MASS = 2
, CM = 154
, IM = 155
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/154
, PART = 20
!
!                        adams_view_name='inertia_frame'
MARKER/155
, PART = 20
!
!                        adams_view_name='jxr_joint_i_3'
MARKER/156
, PART = 20
!
!                           adams_view_name='gracyl_4'
MARKER/157
, PART = 20
!
!                        adams_view_name='jxr_joint_j_17'
MARKER/158
, PART = 20
, REULER = 178.7474825D, 180D, 0D
!
!                      adams_view_name='gracyl_diff_output'
GRAPHICS/16
, CYLINDER
, CM = 157
, LENGTH = 40
, SIDES = 15
, RADIUS = 50
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!               adams_view_name='FRT_SUSP.gel_lower_control_arm2'
PART/26
, QG = -14.416, -791.843, -99.82
, REULER = 180D, 90D, 180D
, MASS = 1
, CM = 227
, IM = 228
, IP = 100, 100, 100
!
!                              adams_view_name='cm'
MARKER/227
, PART = 26
!
!                        adams_view_name='inertia_frame'
MARKER/228
, PART = 26
!
!                        adams_view_name='jxl_joint_j_2'
MARKER/229
, PART = 26
!
!                        adams_view_name='afl_aforce_j_2'
MARKER/230
, PART = 26
, QP = 0, 0, 135.183165
, REULER = 180D, 180D, 0D
!
!                           adams_view_name='gracyl_7'
MARKER/231
, PART = 26
, QP = 0, 0, -20
!
!                        adams_view_name='jxl_joint_j_9'
MARKER/232
, PART = 26
, REULER = 0D, 90D, 0D
!
!                            adams_view_name='kp1_1'
MARKER/233
, PART = 26
, REULER = 0D, 90D, 0D
!
!                       adams_view_name='gracyl_lca2_pin'
GRAPHICS/23
, CYLINDER
, CM = 231
, LENGTH = 40
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!               adams_view_name='FRT_SUSP.ger_lower_control_arm2'
PART/27
, QG = -14.416, 791.843, -99.82
, REULER = 0D, 90D, 0D
, MASS = 1
, CM = 234
, IM = 235
, IP = 100, 100, 100
!
!                              adams_view_name='cm'
MARKER/234
, PART = 27
!
!                        adams_view_name='inertia_frame'
MARKER/235
, PART = 27
!
!                        adams_view_name='jxr_joint_j_2'
MARKER/236
, PART = 27
!
!                        adams_view_name='afr_aforce_j_2'
MARKER/237
, PART = 27
, QP = 0, 0, 135.183165
, REULER = 180D, 180D, 0D
!
!                           adams_view_name='gracyl_8'
MARKER/238
, PART = 27
, QP = 0, 0, -20
!
!                        adams_view_name='jxr_joint_j_9'
MARKER/239
, PART = 27
, REULER = 180D, 90D, 180D
!
!                            adams_view_name='kp1_2'
MARKER/240
, PART = 27
, REULER = 180D, 90D, 180D
!
!                       adams_view_name='gracyl_lca2_pin'
GRAPHICS/24
, CYLINDER
, CM = 238
, LENGTH = 40
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!                  adams_view_name='FRT_SUSP.gel_tierod_inner'
PART/28
, QG = -122.635, -602.75, -41.635
, REULER = 353.2905617D, 90.33422447D, 92.8387371D
, MASS = 1
, CM = 241
, IM = 242
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/241
, PART = 28
!
!                        adams_view_name='inertia_frame'
MARKER/242
, PART = 28
!
!                          adams_view_name='gralin_23'
MARKER/243
, PART = 28
, QP = 0, 0, -210.001763
!
!                        adams_view_name='jxl_joint_j_1'
MARKER/244
, PART = 28
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='afl_aforce_i_1'
MARKER/245
, PART = 28
, QP = 0, 0, -210.001763
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='jxl_joint_i_11'
MARKER/246
, PART = 28
, QP = 0, 0, -210.001763
, REULER = 90D, 0D, 0D
!
!                          adams_view_name='graell_11'
MARKER/247
, PART = 28
, QP = 0, 0, -210.001763
, REULER = 87.1612629D, 90.33422447D, 186.7094383D
!
!                     adams_view_name='gralin_tierod_inner'
GRAPHICS/25
, CYLINDER
, CM = 243
, LENGTH = 210.001763
, SIDES = 15
, RADIUS = 12
, SEG = 15
!
!                     adams_view_name='graell_tierod_inner'
GRAPHICS/85
, ELLIPSOID
, CM = 247
, XSCALE = 36
, YSCALE = 36
, ZSCALE = 36
!
!------------------------------------ Part -------------------------------------
!
!                  adams_view_name='FRT_SUSP.ger_tierod_inner'
PART/29
, QG = -122.635, 602.75, -41.635
, REULER = 186.7094383D, 90.33422447D, 87.1612629D
, MASS = 1
, CM = 248
, IM = 249
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/248
, PART = 29
!
!                        adams_view_name='inertia_frame'
MARKER/249
, PART = 29
!
!                          adams_view_name='gralin_24'
MARKER/250
, PART = 29
, QP = 0, 0, -210.001763
!
!                        adams_view_name='jxr_joint_j_1'
MARKER/251
, PART = 29
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='afr_aforce_i_1'
MARKER/252
, PART = 29
, QP = 0, 0, -210.001763
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='jxr_joint_i_11'
MARKER/253
, PART = 29
, QP = 0, 0, -210.001763
, REULER = 270D, 0D, 0D
!
!                          adams_view_name='graell_12'
MARKER/254
, PART = 29
, QP = 0, 0, -210.001763
, REULER = 92.8387371D, 90.33422447D, 353.2905617D
!
!                     adams_view_name='gralin_tierod_inner'
GRAPHICS/26
, CYLINDER
, CM = 250
, LENGTH = 210.001763
, SIDES = 15
, RADIUS = 12
, SEG = 15
!
!                     adams_view_name='graell_tierod_inner'
GRAPHICS/86
, ELLIPSOID
, CM = 254
, XSCALE = 36
, YSCALE = 36
, ZSCALE = 36
!
!------------------------------------ Part -------------------------------------
!
!                  adams_view_name='FRT_SUSP.gel_tierod_outer'
PART/30
, QG = -122.635, -602.75, -41.635
, REULER = 353.2905617D, 90.33422447D, 92.8387371D
, MASS = 1
, CM = 255
, IM = 256
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/255
, PART = 30
!
!                        adams_view_name='inertia_frame'
MARKER/256
, PART = 30
!
!                          adams_view_name='gralin_25'
MARKER/257
, PART = 30
!
!                        adams_view_name='jxl_joint_i_1'
MARKER/258
, PART = 30
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='afl_aforce_j_1'
MARKER/259
, PART = 30
, QP = 0, 0, 210.001763
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='jxl_joint_i_10'
MARKER/260
, PART = 30
, QP = 0, 0, 210.001763
, REULER = 87.1612629D, 90.33422447D, 186.7094383D
!
!                           adams_view_name='graell_9'
MARKER/261
, PART = 30
, QP = 0, 0, 210.001763
, REULER = 87.1612629D, 90.33422447D, 186.7094383D
!
!                     adams_view_name='gralin_tierod_outer'
GRAPHICS/27
, CYLINDER
, CM = 257
, LENGTH = 210.001763
, SIDES = 15
, RADIUS = 10
, SEG = 15
!
!                     adams_view_name='graell_tierod_outer'
GRAPHICS/87
, ELLIPSOID
, CM = 261
, XSCALE = 30
, YSCALE = 30
, ZSCALE = 30
!
!------------------------------------ Part -------------------------------------
!
!                  adams_view_name='FRT_SUSP.ger_tierod_outer'
PART/31
, QG = -122.635, 602.75, -41.635
, REULER = 186.7094383D, 90.33422447D, 87.1612629D
, MASS = 1
, CM = 262
, IM = 263
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/262
, PART = 31
!
!                        adams_view_name='inertia_frame'
MARKER/263
, PART = 31
!
!                          adams_view_name='gralin_26'
MARKER/264
, PART = 31
!
!                        adams_view_name='jxr_joint_i_1'
MARKER/265
, PART = 31
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='jxr_joint_i_10'
MARKER/266
, PART = 31
, QP = 0, 0, 210.001763
, REULER = 92.8387371D, 90.33422447D, 353.2905617D
!
!                        adams_view_name='afr_aforce_j_1'
MARKER/267
, PART = 31
, QP = 0, 0, 210.001763
, REULER = 180D, 180D, 0D
!
!                          adams_view_name='graell_10'
MARKER/268
, PART = 31
, QP = 0, 0, 210.001763
, REULER = 92.8387371D, 90.33422447D, 353.2905617D
!
!                     adams_view_name='gralin_tierod_outer'
GRAPHICS/28
, CYLINDER
, CM = 264
, LENGTH = 210.001763
, SIDES = 15
, RADIUS = 10
, SEG = 15
!
!                     adams_view_name='graell_tierod_outer'
GRAPHICS/88
, ELLIPSOID
, CM = 268
, XSCALE = 30
, YSCALE = 30
, ZSCALE = 30
!
!------------------------------------ Part -------------------------------------
!
!                adams_view_name='FRT_SUSP.gel_lower_control_arm'
PART/32
, QG = 6.528, -523.9476667, -96.27333333
, REULER = 355.529721D, 90.75618744D, 182.6816001D
, MASS = 6.557425487
, CM = 271
, IM = 276
, IP = 71240.6575, 1.716880578E+05, 1.019588854E+05, 0, -14438.81923, 0
!
!                        adams_view_name='jxl_joint_i_2'
MARKER/269
, PART = 32
, QP = 0, 0, 268.7361896
, REULER = 96.90019934D, 175.4663422D, 279.6113141D
!
!                        adams_view_name='afl_aforce_i_2'
MARKER/270
, PART = 32
, QP = 0, 0, 268.7361896
, REULER = 276.9001993D, 4.533657844D, 80.38868592D
!
!                              adams_view_name='cm'
MARKER/271
, PART = 32
, QP = 5.382811275, 0, 54.21567563
, REULER = 90D, 21.61550496D, 270D
!
!                        adams_view_name='jxl_joint_i_8'
MARKER/272
, PART = 32
, QP = 0, 0, -134.3680948
, REULER = 90D, 85.49904437D, 180.544115D
!
!                        adams_view_name='swl_switch_j_2'
MARKER/273
, PART = 32
, QP = 21.59901551, -450.1124293, 174.0172705
, REULER = 357.3183999D, 90.75618744D, 184.470279D
!
!                        adams_view_name='jxl_joint_j_16'
MARKER/274
, PART = 32
, QP = 20.1244094, 0.8036765999, 135.0617704
, REULER = 357.3183999D, 90.75618744D, 265.2294111D
!
!                        adams_view_name='inertia_frame'
MARKER/276
, PART = 32
, QP = 5.382811275, 0, 54.21567563
!
!                           adams_view_name='gralin_5'
MARKER/278
, PART = 32
, QP = 219.5711788, 0, -117.0837833
, REULER = 270D, 29.64432007D, 90D
!
!                           adams_view_name='gralin_7'
MARKER/279
, PART = 32
, QP = -219.5711788, 0, -151.6524063
, REULER = 90D, 27.5783025D, 270D
!
!                           adams_view_name='graell_5'
MARKER/280
, PART = 32
, QP = 0, 0, 268.7361896
, REULER = 357.3183999D, 90.75618744D, 184.470279D
!
!                          adams_view_name='gralin_19'
MARKER/285
, PART = 32
, QP = 109.7855894, 0, 75.82620313
, REULER = 269.4864439D, 56.54990893D, 90.28308273D
!
!                          adams_view_name='gralin_21'
MARKER/286
, PART = 32
, QP = -109.7855894, 0, 58.54189167
, REULER = 90.3544507D, 59.50144822D, 269.8201087D
!
!                         adams_view_name='coomarker_1'
MARKER/287
, PART = 32
, QP = 20.1244094, 0.8036765999, 135.0617704
, REULER = 357.3183999D, 90.75618744D, 184.470279D
!
!                  adams_view_name='grarev_lca_case_MARKER_562'
MARKER/562
, PART = 32
, QP = -18.34691741, 1.143346234, 247.2400648
!
!                     adams_view_name='i_graphic_MARKER_575'
MARKER/575
, PART = 32
, QP = 234.5249192, 0, -115.9066475
!
!                     adams_view_name='i_graphic_MARKER_577'
MARKER/577
, PART = 32
, QP = -204.6174385, 0, -150.4752704
!
!                       adams_view_name='gralin_lca_front'
GRAPHICS/29
, CYLINDER
, CM = 278
, LENGTH = 443.9240409
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                       adams_view_name='gralin_lca_rear'
GRAPHICS/30
, CYLINDER
, CM = 279
, LENGTH = 474.2763689
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                  adams_view_name='gralin_lca_damper_mount_1'
GRAPHICS/31
, CYLINDER
, CM = 285
, LENGTH = 107.4645315
, SIDES = 15
, RADIUS = 10
, SEG = 15
!
!                  adams_view_name='gralin_lca_damper_mount_2'
GRAPHICS/32
, CYLINDER
, CM = 286
, LENGTH = 150.7731592
, SIDES = 15
, RADIUS = 10
, SEG = 15
!
!                  adams_view_name='graell_upright_lower_ball'
GRAPHICS/89
, ELLIPSOID
, CM = 280
, XSCALE = 30
, YSCALE = 30
, ZSCALE = 30
!
!                  adams_view_name='grarev_lca_case_GCURVE_163'
GRAPHICS/163
, CURVE
, CID = 1
, CRM = 562
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_280'
GRAPHICS/280
, CURVE
, CID = 14
, CRM = 575
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_298'
GRAPHICS/298
, CURVE
, CID = 16
, CRM = 577
, SEG = 500
!
!                       adams_view_name='grarev_lca_case'
GRAPHICS/134
, REVOLUTION
, CRM = 269
, SIDES = 20
, GID = 163
!
!------------------------------------ Part -------------------------------------
!
!                adams_view_name='FRT_SUSP.ger_lower_control_arm'
PART/33
, QG = 6.528, 523.9476667, -96.27333333
, REULER = 184.470279D, 90.75618744D, 357.3183999D
, MASS = 6.557425487
, CM = 290
, IM = 295
, IP = 71240.6575, 1.716880578E+05, 1.019588854E+05, 0, -14438.81923, 0
!
!                        adams_view_name='jxr_joint_i_2'
MARKER/288
, PART = 33
, QP = 0, 0, 268.7361896
, REULER = 83.09980066D, 175.4663422D, 260.3886859D
!
!                        adams_view_name='afr_aforce_i_2'
MARKER/289
, PART = 33
, QP = 0, 0, 268.7361896
, REULER = 263.0998007D, 4.533657844D, 99.61131408D
!
!                              adams_view_name='cm'
MARKER/290
, PART = 33
, QP = 5.382811275, 0, 54.21567563
, REULER = 90D, 21.61550496D, 270D
!
!                        adams_view_name='jxr_joint_i_8'
MARKER/291
, PART = 33
, QP = 0, 0, -134.3680948
, REULER = 90D, 85.49904437D, 359.455885D
!
!                        adams_view_name='swr_switch_j_2'
MARKER/292
, PART = 33
, QP = 21.59901551, 450.1124293, 174.0172705
, REULER = 182.6816001D, 90.75618744D, 355.529721D
!
!                        adams_view_name='jxr_joint_j_16'
MARKER/293
, PART = 33
, QP = 20.1244094, -0.8036765999, 135.0617704
, REULER = 182.6816001D, 90.75618744D, 274.7705889D
!
!                        adams_view_name='inertia_frame'
MARKER/295
, PART = 33
, QP = 5.382811275, 0, 54.21567563
!
!                           adams_view_name='gralin_6'
MARKER/297
, PART = 33
, QP = 219.5711788, 0, -117.0837833
, REULER = 270D, 29.64432007D, 90D
!
!                           adams_view_name='gralin_8'
MARKER/298
, PART = 33
, QP = -219.5711788, 0, -151.6524063
, REULER = 90D, 27.5783025D, 270D
!
!                           adams_view_name='graell_6'
MARKER/299
, PART = 33
, QP = 0, 0, 268.7361896
, REULER = 182.6816001D, 90.75618744D, 355.529721D
!
!                          adams_view_name='gralin_20'
MARKER/304
, PART = 33
, QP = 109.7855894, 0, 75.82620313
, REULER = 270.5135561D, 56.54990893D, 89.71691727D
!
!                          adams_view_name='gralin_22'
MARKER/305
, PART = 33
, QP = -109.7855894, 0, 58.54189167
, REULER = 89.6455493D, 59.50144822D, 270.1798913D
!
!                         adams_view_name='coomarker_2'
MARKER/306
, PART = 33
, QP = 20.1244094, -0.8036765999, 135.0617704
, REULER = 182.6816001D, 90.75618744D, 355.529721D
!
!                  adams_view_name='grarev_lca_case_MARKER_563'
MARKER/563
, PART = 33
, QP = -18.34691741, -1.143346234, 247.2400648
!
!                     adams_view_name='i_graphic_MARKER_576'
MARKER/576
, PART = 33
, QP = 234.5249192, 0, -115.9066475
!
!                     adams_view_name='i_graphic_MARKER_578'
MARKER/578
, PART = 33
, QP = -204.6174385, 0, -150.4752704
!
!                       adams_view_name='gralin_lca_front'
GRAPHICS/33
, CYLINDER
, CM = 297
, LENGTH = 443.9240409
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                       adams_view_name='gralin_lca_rear'
GRAPHICS/34
, CYLINDER
, CM = 298
, LENGTH = 474.2763689
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                  adams_view_name='gralin_lca_damper_mount_1'
GRAPHICS/35
, CYLINDER
, CM = 304
, LENGTH = 107.4645315
, SIDES = 15
, RADIUS = 10
, SEG = 15
!
!                  adams_view_name='gralin_lca_damper_mount_2'
GRAPHICS/36
, CYLINDER
, CM = 305
, LENGTH = 150.7731592
, SIDES = 15
, RADIUS = 10
, SEG = 15
!
!                  adams_view_name='graell_upright_lower_ball'
GRAPHICS/90
, ELLIPSOID
, CM = 299
, XSCALE = 30
, YSCALE = 30
, ZSCALE = 30
!
!                  adams_view_name='grarev_lca_case_GCURVE_172'
GRAPHICS/172
, CURVE
, CID = 2
, CRM = 563
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_289'
GRAPHICS/289
, CURVE
, CID = 15
, CRM = 576
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_307'
GRAPHICS/307
, CURVE
, CID = 17
, CRM = 578
, SEG = 500
!
!                       adams_view_name='grarev_lca_case'
GRAPHICS/135
, REVOLUTION
, CRM = 288
, SIDES = 20
, GID = 172
!
!------------------------------------ Part -------------------------------------
!
!                     adams_view_name='FRT_SUSP.gel_upright'
PART/34
, QG = 0, -835, 0
, MASS = 3.638219793
, CM = 308
, IM = 313
, IP = 40802.73904, 42306.34705, 8340.065416
!
!                      adams_view_name='afl_aforce_meai_2'
MARKER/307
, PART = 34
, REULER = 359.95D, 89.5D, 0D
!
!                              adams_view_name='cm'
MARKER/308
, PART = 34
, QP = 24.71102106, 50.44175889, 11.69602966
, REULER = 155.9386081D, 12.80550552D, 205.3244685D
!
!                        adams_view_name='jxl_joint_i_9'
MARKER/309
, PART = 34
, QP = -14.416, 43.157, -99.82
!
!                        adams_view_name='jxl_joint_j_10'
MARKER/310
, PART = 34
, QP = -147.17, 23.69, -42.86
!
!                        adams_view_name='jxl_joint_j_13'
MARKER/311
, PART = 34
, QP = 36.54, 109.51, 433.66
!
!                        adams_view_name='swl_switch_j_1'
MARKER/312
, PART = 34
, QP = -50, 135, 350
!
!                        adams_view_name='inertia_frame'
MARKER/313
, PART = 34
, QP = 24.71102106, 50.44175889, 11.69602966
!
!                        adams_view_name='jxl_joint_j_20'
MARKER/314
, PART = 34
, REULER = 359.95D, 89.5D, 0D
!
!                          adams_view_name='gralin_13'
MARKER/315
, PART = 34
, QP = 36.54, 109.51, 433.66
, REULER = 313.4170901D, 173.404822D, 133.2272072D
!
!                          adams_view_name='gralin_15'
MARKER/316
, PART = 34
, QP = -14.416, 43.157, -99.82
, REULER = 155.5431202D, 19.42926976D, 205.7471894D
!
!                          adams_view_name='gralin_17'
MARKER/317
, PART = 34
, QP = -147.17, 23.69, -42.86
, REULER = 109.211906D, 74.8536422D, 264.7975553D
!
!                           adams_view_name='gracyl_5'
MARKER/318
, PART = 34
, QP = 0.0654473465, 74.99711567, -0.6544901624
, REULER = 359.95D, 89.5D, 0D
!
!                      adams_view_name='afl_aforce_meai_1'
MARKER/319
, PART = 34
, REULER = 359.95D, 89.5D, 0D
!
!                       adams_view_name='mal_wheel_center'
MARKER/320
, PART = 34
, REULER = 359.95D, 89.5D, 0D
!
!                       adams_view_name='mal_kingpin_axis'
MARKER/321
, PART = 34
, QP = -14.416, 43.157, -99.82
, REULER = 142.4774233D, 8.912651367D, 217.8593182D
!
!                       adams_view_name='bxl_bushing_j_1'
MARKER/322
, PART = 34
, REULER = 359.95D, 89.5D, 0D
!
!                       adams_view_name='bxl_bushgeom_j_1'
MARKER/323
, PART = 34
, QP = 0.0087263129, 9.999615423, -0.087265355
, REULER = 359.95D, 89.5D, 0D
!
!                        adams_view_name='jxl_joint_j_3'
MARKER/324
, PART = 34
!
!                       adams_view_name='mal_spindle_lock'
MARKER/325
, PART = 34
, REULER = 179.95D, 0.5D, 180D
!
!                      adams_view_name='gralin_upright_upr'
GRAPHICS/37
, CYLINDER
, CM = 315
, LENGTH = 437.2077407
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                      adams_view_name='gralin_upright_lwr'
GRAPHICS/38
, CYLINDER
, CM = 316
, LENGTH = 105.1537143
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                   adams_view_name='gralin_upright_steer_arm'
GRAPHICS/39
, CYLINDER
, CM = 317
, LENGTH = 161.5301895
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                    adams_view_name='gracyl_upright_spindle'
GRAPHICS/40
, CYLINDER
, CM = 318
, LENGTH = 75
, SIDES = 15
, RADIUS = 20
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!                     adams_view_name='FRT_SUSP.ger_upright'
PART/35
, QG = 0, 835, 0
, MASS = 3.638219793
, CM = 327
, IM = 332
, IP = 40802.73904, 42306.34705, 8340.065416
!
!                      adams_view_name='afr_aforce_meai_2'
MARKER/326
, PART = 35
, REULER = 180.05D, 89.5D, 180D
!
!                              adams_view_name='cm'
MARKER/327
, PART = 35
, QP = 24.71102106, -50.44175889, 11.69602966
, REULER = 24.51111563D, 12.64736633D, 334.2918363D
!
!                        adams_view_name='jxr_joint_i_9'
MARKER/328
, PART = 35
, QP = -14.416, -43.157, -99.82
!
!                        adams_view_name='jxr_joint_j_10'
MARKER/329
, PART = 35
, QP = -147.17, -23.69, -42.86
!
!                        adams_view_name='jxr_joint_j_13'
MARKER/330
, PART = 35
, QP = 36.54, -109.51, 433.66
!
!                        adams_view_name='swr_switch_j_1'
MARKER/331
, PART = 35
, QP = -50, -135, 350
!
!                        adams_view_name='inertia_frame'
MARKER/332
, PART = 35
, QP = 24.71102106, -50.44175889, 11.69602966
!
!                        adams_view_name='jxr_joint_j_20'
MARKER/333
, PART = 35
, REULER = 180.05D, 89.5D, 180D
!
!                          adams_view_name='gralin_14'
MARKER/334
, PART = 35
, QP = 36.54, -109.51, 433.66
, REULER = 226.5829099D, 173.404822D, 46.77279277D
!
!                          adams_view_name='gralin_16'
MARKER/335
, PART = 35
, QP = -14.416, -43.157, -99.82
, REULER = 24.45687975D, 19.42926976D, 334.2528106D
!
!                          adams_view_name='gralin_18'
MARKER/336
, PART = 35
, QP = -147.17, -23.69, -42.86
, REULER = 70.78809398D, 74.8536422D, 275.2024447D
!
!                           adams_view_name='gracyl_6'
MARKER/337
, PART = 35
, QP = 0.0654473465, -74.99711567, -0.6544901624
, REULER = 180.05D, 89.5D, 180D
!
!                      adams_view_name='afr_aforce_meai_1'
MARKER/338
, PART = 35
, REULER = 180.05D, 89.5D, 180D
!
!                       adams_view_name='mar_wheel_center'
MARKER/339
, PART = 35
, REULER = 180.05D, 89.5D, 180D
!
!                       adams_view_name='mar_kingpin_axis'
MARKER/340
, PART = 35
, QP = -14.416, -43.157, -99.82
, REULER = 37.52257667D, 8.912651367D, 322.1406818D
!
!                       adams_view_name='bxr_bushing_j_1'
MARKER/341
, PART = 35
, REULER = 180.05D, 89.5D, 180D
!
!                       adams_view_name='bxr_bushgeom_j_1'
MARKER/342
, PART = 35
, QP = 0.0087263129, -9.999615423, -0.087265355
, REULER = 180.05D, 89.5D, 180D
!
!                        adams_view_name='jxr_joint_j_3'
MARKER/343
, PART = 35
!
!                       adams_view_name='mar_spindle_lock'
MARKER/344
, PART = 35
, REULER = 0.05D, 0.5D, 0D
!
!                      adams_view_name='gralin_upright_upr'
GRAPHICS/41
, CYLINDER
, CM = 334
, LENGTH = 437.2077407
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                      adams_view_name='gralin_upright_lwr'
GRAPHICS/42
, CYLINDER
, CM = 335
, LENGTH = 105.1537143
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                   adams_view_name='gralin_upright_steer_arm'
GRAPHICS/43
, CYLINDER
, CM = 336
, LENGTH = 161.5301895
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                    adams_view_name='gracyl_upright_spindle'
GRAPHICS/44
, CYLINDER
, CM = 337
, LENGTH = 75
, SIDES = 15
, RADIUS = 20
, SEG = 15
!
!                  adams_view_name='jorsph_lca_balljoint_1_g1'
GRAPHICS/91
, ELLIPSOID
, CM = 328
, XSCALE = 15
, YSCALE = 15
, ZSCALE = 15
!
!------------------------------------ Part -------------------------------------
!
!                    adams_view_name='FRT_SUSP.ges_subframe'
PART/36
, MASS = 50
, CM = 345
, IM = 351
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/345
, PART = 36
, QP = 0, 0, 150
!
!                        adams_view_name='jxs_joint_i_8'
MARKER/346
, PART = 36
, QP = 17, 0, -94.5
!
!                       adams_view_name='bxl_bushing_i_3'
MARKER/347
, PART = 36
, QP = -400, -450, -120
!
!                       adams_view_name='bxr_bushing_i_3'
MARKER/348
, PART = 36
, QP = -400, 450, -120
!
!                       adams_view_name='bxl_bushing_i_4'
MARKER/349
, PART = 36
, QP = 400, -450, -120
!
!                       adams_view_name='bxr_bushing_i_4'
MARKER/350
, PART = 36
, QP = 400, 450, -120
!
!                        adams_view_name='inertia_frame'
MARKER/351
, PART = 36
, QP = 0, 0, 150
!
!                          adams_view_name='graout_15'
MARKER/352
, PART = 36
, QP = -400, -450, -120
!
!                          adams_view_name='graout_16'
MARKER/353
, PART = 36
, QP = -203, -390, -105
!
!                          adams_view_name='graout_17'
MARKER/354
, PART = 36
, QP = 237, -390, -84
!
!                          adams_view_name='graout_18'
MARKER/355
, PART = 36
, QP = 400, -450, -120
!
!                          adams_view_name='graout_19'
MARKER/356
, PART = 36
, QP = 237, 390, -84
!
!                          adams_view_name='graout_20'
MARKER/357
, PART = 36
, QP = 400, 450, -120
!
!                          adams_view_name='graout_21'
MARKER/358
, PART = 36
, QP = -203, 390, -105
!
!                          adams_view_name='graout_22'
MARKER/359
, PART = 36
, QP = -400, 450, -120
!
!                       adams_view_name='bxl_bushgeom_i_3'
MARKER/360
, PART = 36
, QP = -400, -450, -130
, REULER = 270D, 0D, 0D
!
!                       adams_view_name='bxr_bushgeom_i_3'
MARKER/361
, PART = 36
, QP = -400, 450, -130
, REULER = 270D, 0D, 0D
!
!                       adams_view_name='bxl_bushgeom_i_4'
MARKER/362
, PART = 36
, QP = 400, -450, -130
, REULER = 270D, 0D, 0D
!
!                       adams_view_name='bxr_bushgeom_i_4'
MARKER/363
, PART = 36
, QP = 400, 450, -130
, REULER = 270D, 0D, 0D
!
!                        adams_view_name='jxl_joint_j_8'
MARKER/364
, PART = 36
, QP = 17, -390, -94.5
, REULER = 270D, 92.73249777D, 90D
!
!                        adams_view_name='jxr_joint_j_8'
MARKER/365
, PART = 36
, QP = 17, 390, -94.5
, REULER = 270D, 92.73249777D, 90D
!
!                        adams_view_name='sws_switch_j_2'
MARKER/374
, PART = 36
, QP = -70, 0, -20
!
!                     adams_view_name='i_graphic_MARKER_564'
MARKER/564
, PART = 36
, QP = -400, 450, -120
!
!                     adams_view_name='i_graphic_MARKER_565'
MARKER/565
, PART = 36
, QP = 400, -450, -120
!
!                     adams_view_name='i_graphic_MARKER_566'
MARKER/566
, PART = 36
, QP = 400, 450, -120
!
!                     adams_view_name='i_graphic_MARKER_579'
MARKER/579
, PART = 36
, QP = -400, -450, -120
!
!                   adams_view_name='graout_subframe_graphic'
GRAPHICS/133
, OUTLINE = 352, 353, 354, 355, 354, 356, 357, 356, 358, 353, 358, 359
!
!                     adams_view_name='i_graphic_GCURVE_181'
GRAPHICS/181
, CURVE
, CID = 3
, CRM = 564
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_190'
GRAPHICS/190
, CURVE
, CID = 4
, CRM = 565
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_199'
GRAPHICS/199
, CURVE
, CID = 5
, CRM = 566
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_316'
GRAPHICS/316
, CURVE
, CID = 18
, CRM = 579
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.gel_upper_strut'
PART/37
, QG = -3.42978, -530.5671, 303.68044
, REULER = 170.759132D, 17.61339003D, 189.6869719D
, MASS = 5
, CM = 375
, IM = 381
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/375
, PART = 37
!
!                        adams_view_name='jxl_joint_i_12'
MARKER/376
, PART = 37
, QP = 0, 0, 218.0770153
, REULER = 260.3130281D, 180D, 0D
!
!                        adams_view_name='jxl_joint_j_14'
MARKER/378
, PART = 37
, QP = 0, 0, -102.6244778
, REULER = 359.1276501D, 0D, 0D
!
!                       adams_view_name='bul_bumpstop_i_1'
MARKER/379
, PART = 37
, QP = 0, 0, 218.0770153
!
!                        adams_view_name='dal_damper_i_1'
MARKER/380
, PART = 37
, QP = 0, 0, 218.0770153
!
!                        adams_view_name='inertia_frame'
MARKER/381
, PART = 37
!
!                     adams_view_name='i_graphic_MARKER_567'
MARKER/567
, PART = 37
, QP = 0, 0, 218.0770153
!
!                     adams_view_name='i_graphic_GCURVE_208'
GRAPHICS/208
, CURVE
, CID = 6
, CRM = 567
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.ger_upper_strut'
PART/38
, QG = -3.42978, 530.5671, 303.68044
, REULER = 9.240867979D, 17.61339003D, 350.3130281D
, MASS = 5
, CM = 383
, IM = 389
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/383
, PART = 38
, REULER = 201.8014095D, 167.8438549D, 22.25314003D
!
!                        adams_view_name='jxr_joint_i_12'
MARKER/384
, PART = 38
, QP = 0, 0, 218.0770153
, REULER = 99.68697193D, 180D, 0D
!
!                        adams_view_name='jxr_joint_j_14'
MARKER/386
, PART = 38
, QP = 0, 0, -102.6244778
, REULER = 0.8723498878D, 0D, 0D
!
!                       adams_view_name='bur_bumpstop_i_1'
MARKER/387
, PART = 38
, QP = 0, 0, 218.0770153
!
!                        adams_view_name='dar_damper_i_1'
MARKER/388
, PART = 38
, QP = 0, 0, 218.0770153
!
!                        adams_view_name='inertia_frame'
MARKER/389
, PART = 38
!
!                     adams_view_name='i_graphic_MARKER_568'
MARKER/568
, PART = 38
, QP = 0, 0, 218.0770153
!
!                     adams_view_name='i_graphic_GCURVE_217'
GRAPHICS/217
, CURVE
, CID = 7
, CRM = 568
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!                adams_view_name='FRT_SUSP.gel_upper_control_arm'
PART/44
, QG = 5.68, -535.1633333, 400.22
, REULER = 9.209916656D, 80.16089628D, 175.5323137D
, MASS = 4.639404499
, CM = 396
, IM = 402
, IP = 24198.899, 31232.70325, 7386.36179, 0, 2611.808106, 0
!
!                              adams_view_name='cm'
MARKER/396
, PART = 44
, QP = -2.237217684, 0, 25.01031649
, REULER = 90D, 8.629949053D, 270D
!
!                        adams_view_name='jxl_joint_i_13'
MARKER/397
, PART = 44
, QP = 0, 0, 195.6906059
, REULER = 4.467686255D, 80.16089628D, 170.7900833D
!
!                        adams_view_name='jxl_joint_i_15'
MARKER/398
, PART = 44
, QP = 0, 0, -97.84530296
, REULER = 90D, 98.56174143D, 169.5933046D
!
!                            adams_view_name='kp2_1'
MARKER/401
, PART = 44
, QP = 0, 0, 195.6906059
, REULER = 4.467686255D, 80.16089628D, 170.7900833D
!
!                        adams_view_name='inertia_frame'
MARKER/402
, PART = 44
, QP = -2.237217684, 0, 25.01031649
!
!                           adams_view_name='gralin_9'
MARKER/405
, PART = 44
, QP = 166.5872061, 0, -122.9254798
, REULER = 270D, 27.60264681D, 90D
!
!                          adams_view_name='gralin_11'
MARKER/406
, PART = 44
, QP = -166.5872061, 0, -72.76512613
, REULER = 90D, 31.82120788D, 270D
!
!                           adams_view_name='graell_7'
MARKER/407
, PART = 44
, QP = 0, 0, 195.6906059
, REULER = 4.467686255D, 80.16089628D, 170.7900833D
!
!                     adams_view_name='i_graphic_MARKER_569'
MARKER/569
, PART = 44
, QP = 181.4200462, 0, -125.158606
!
!                     adams_view_name='i_graphic_MARKER_571'
MARKER/571
, PART = 44
, QP = -181.4200462, 0, -70.53199993
!
!                       adams_view_name='gralin_uca_front'
GRAPHICS/45
, CYLINDER
, CM = 405
, LENGTH = 359.537908
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                       adams_view_name='gralin_uca_rear'
GRAPHICS/46
, CYLINDER
, CM = 406
, LENGTH = 315.9426804
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                   adams_view_name='graell_upright_upr_ball'
GRAPHICS/92
, ELLIPSOID
, CM = 407
, XSCALE = 30
, YSCALE = 30
, ZSCALE = 30
!
!                     adams_view_name='i_graphic_GCURVE_226'
GRAPHICS/226
, CURVE
, CID = 8
, CRM = 569
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_244'
GRAPHICS/244
, CURVE
, CID = 10
, CRM = 571
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                adams_view_name='FRT_SUSP.ger_upper_control_arm'
PART/45
, QG = 5.68, 535.1633333, 400.22
, REULER = 170.7900833D, 80.16089628D, 4.467686255D
, MASS = 4.639404499
, CM = 408
, IM = 414
, IP = 24198.899, 31232.70325, 7386.36179, 0, 2611.808106, 0
!
!                              adams_view_name='cm'
MARKER/408
, PART = 45
, QP = -2.237217684, 0, 25.01031649
, REULER = 90D, 8.629949053D, 270D
!
!                        adams_view_name='jxr_joint_i_13'
MARKER/409
, PART = 45
, QP = 0, 0, 195.6906059
, REULER = 175.5323137D, 80.16089628D, 9.209916656D
!
!                        adams_view_name='jxr_joint_i_15'
MARKER/410
, PART = 45
, QP = 0, 0, -97.84530296
, REULER = 90D, 98.56174143D, 10.40669542D
!
!                            adams_view_name='kp2_2'
MARKER/413
, PART = 45
, QP = 0, 0, 195.6906059
, REULER = 175.5323137D, 80.16089628D, 9.209916656D
!
!                        adams_view_name='inertia_frame'
MARKER/414
, PART = 45
, QP = -2.237217684, 0, 25.01031649
!
!                          adams_view_name='gralin_10'
MARKER/417
, PART = 45
, QP = 166.5872061, 0, -122.9254798
, REULER = 270D, 27.60264681D, 90D
!
!                          adams_view_name='gralin_12'
MARKER/418
, PART = 45
, QP = -166.5872061, 0, -72.76512613
, REULER = 90D, 31.82120788D, 270D
!
!                           adams_view_name='graell_8'
MARKER/419
, PART = 45
, QP = 0, 0, 195.6906059
, REULER = 175.5323137D, 80.16089628D, 9.209916656D
!
!                     adams_view_name='i_graphic_MARKER_570'
MARKER/570
, PART = 45
, QP = 181.4200462, 0, -125.158606
!
!                     adams_view_name='i_graphic_MARKER_572'
MARKER/572
, PART = 45
, QP = -181.4200462, 0, -70.53199993
!
!                       adams_view_name='gralin_uca_front'
GRAPHICS/47
, CYLINDER
, CM = 417
, LENGTH = 359.537908
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                       adams_view_name='gralin_uca_rear'
GRAPHICS/48
, CYLINDER
, CM = 418
, LENGTH = 315.9426804
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                   adams_view_name='graell_upright_upr_ball'
GRAPHICS/93
, ELLIPSOID
, CM = 419
, XSCALE = 30
, YSCALE = 30
, ZSCALE = 30
!
!                     adams_view_name='i_graphic_GCURVE_235'
GRAPHICS/235
, CURVE
, CID = 9
, CRM = 570
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_253'
GRAPHICS/253
, CURVE
, CID = 11
, CRM = 572
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.gel_lower_strut'
PART/46
, QG = -13.71489, -593.78355, 101.94022
, REULER = 170.759132D, 17.61339003D, 189.6869719D
, MASS = 5
, CM = 420
, IM = 427
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/420
, PART = 46
, REULER = 338.1985905D, 167.8438549D, 157.74686D
!
!                        adams_view_name='jxl_joint_i_14'
MARKER/421
, PART = 46
, QP = 0, 0, 109.0385076
, REULER = 359.1276501D, 0D, 0D
!
!                       adams_view_name='bul_bumpstop_j_1'
MARKER/422
, PART = 46
, QP = 2.545791236, 14.91391016, -259.3189843
!
!                        adams_view_name='jxl_joint_i_16'
MARKER/423
, PART = 46
, QP = 0, 0, -211.6629854
, REULER = 80.31302807D, 0D, 0D
!
!                        adams_view_name='dal_damper_j_1'
MARKER/425
, PART = 46
, QP = 0, 0, -211.6629854
!
!                        adams_view_name='nsl_spring_j_1'
MARKER/426
, PART = 46
, QP = 0, 0, 109.0385076
!
!                        adams_view_name='inertia_frame'
MARKER/427
, PART = 46
!
!                     adams_view_name='i_graphic_MARKER_573'
MARKER/573
, PART = 46
, QP = -19.90280217, 0.5881866657, -213.5424807
!
!                     adams_view_name='i_graphic_GCURVE_262'
GRAPHICS/262
, CURVE
, CID = 12
, CRM = 573
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.ger_lower_strut'
PART/47
, QG = -13.71489, 593.78355, 101.94022
, REULER = 9.240867979D, 17.61339003D, 350.3130281D
, MASS = 5
, CM = 429
, IM = 436
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/429
, PART = 47
, REULER = 201.8014095D, 167.8438549D, 22.25314003D
!
!                        adams_view_name='jxr_joint_i_14'
MARKER/430
, PART = 47
, QP = 0, 0, 109.0385076
, REULER = 0.8723498878D, 0D, 0D
!
!                       adams_view_name='bur_bumpstop_j_1'
MARKER/431
, PART = 47
, QP = 2.545791236, -14.91391016, -259.3189843
!
!                        adams_view_name='jxr_joint_i_16'
MARKER/432
, PART = 47
, QP = 0, 0, -211.6629854
, REULER = 279.6869719D, 0D, 0D
!
!                        adams_view_name='dar_damper_j_1'
MARKER/434
, PART = 47
, QP = 0, 0, -211.6629854
!
!                        adams_view_name='nsr_spring_j_1'
MARKER/435
, PART = 47
, QP = 0, 0, 109.0385076
!
!                        adams_view_name='inertia_frame'
MARKER/436
, PART = 47
!
!                     adams_view_name='i_graphic_MARKER_574'
MARKER/574
, PART = 47
, QP = -19.90280217, -0.5881866657, -213.5424807
!
!                     adams_view_name='i_graphic_GCURVE_271'
GRAPHICS/271
, CURVE
, CID = 13
, CRM = 574
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.swl_ARB_pickup'
PART/50
, QG = -50, -700, 350
!
!                           adams_view_name='switch_i'
MARKER/440
, PART = 50
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.swr_ARB_pickup'
PART/51
, QG = -50, 700, 350
!
!                           adams_view_name='switch_i'
MARKER/441
, PART = 51
!
!------------------------------------ Part -------------------------------------
!
!                     adams_view_name='FRT_SUSP.gel_spindle'
PART/52
, QG = 0, -835, 0
, REULER = 359.95D, 89.5D, 0D
, MASS = 1.102840393
, CM = 445
, IM = 446
, IP = 477.8975037, 477.8975037, 496.2781769
!
!                       adams_view_name='bxl_bushing_i_9'
MARKER/442
, PART = 52
!
!                       adams_view_name='bxl_bushgeom_i_9'
MARKER/443
, PART = 52
, QP = 0, 0, -10
, REULER = 270D, 0D, 0D
!
!                        adams_view_name='jxl_joint_i_3'
MARKER/444
, PART = 52
, REULER = 180D, 89.5D, 180.05D
!
!                              adams_view_name='cm'
MARKER/445
, PART = 52
, QP = 0, 0, 15
!
!                        adams_view_name='inertia_frame'
MARKER/446
, PART = 52
, QP = 0, 0, 15
!
!                           adams_view_name='gracyl_1'
MARKER/447
, PART = 52
, QP = 0, 0, -75
, REULER = 5.71066658D, 0D, 0D
!
!                        adams_view_name='jxl_joint_j_19'
MARKER/448
, PART = 52
, QP = 0, 0, -75
, REULER = 8.631142389D, 0D, 0D
!
!                        adams_view_name='jxl_joint_i_20'
MARKER/449
, PART = 52
!
!                        adams_view_name='jxl_joint_j_1'
MARKER/450
, PART = 52
!
!                       adams_view_name='jml_actuator_j_1'
MARKER/451
, PART = 52
!
!                       adams_view_name='mal_spindle_lock'
MARKER/452
, PART = 52
, REULER = 90D, 90D, 0D
!
!                     adams_view_name='i_graphic_MARKER_580'
MARKER/580
, PART = 52
!
!                adams_view_name='gracyl_cv_jt_housing_extension'
GRAPHICS/49
, CYLINDER
, CM = 447
, LENGTH = 50
, SIDES = 15
, RADIUS = 30
, SEG = 15
!
!                     adams_view_name='i_graphic_GCURVE_325'
GRAPHICS/325
, CURVE
, CID = 19
, CRM = 580
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                     adams_view_name='FRT_SUSP.ger_spindle'
PART/53
, QG = 0, 835, 0
, REULER = 180.05D, 89.5D, 180D
, MASS = 1.102840393
, CM = 458
, IM = 459
, IP = 477.8975037, 477.8975037, 496.2781769
!
!                       adams_view_name='bxr_bushing_i_9'
MARKER/455
, PART = 53
!
!                       adams_view_name='bxr_bushgeom_i_9'
MARKER/456
, PART = 53
, QP = 0, 0, -10
, REULER = 270D, 0D, 0D
!
!                        adams_view_name='jxr_joint_i_3'
MARKER/457
, PART = 53
, REULER = 0D, 89.5D, 359.95D
!
!                              adams_view_name='cm'
MARKER/458
, PART = 53
, QP = 0, 0, 15
!
!                        adams_view_name='inertia_frame'
MARKER/459
, PART = 53
, QP = 0, 0, 15
!
!                           adams_view_name='gracyl_2'
MARKER/460
, PART = 53
, QP = 0, 0, -75
, REULER = 354.2893334D, 0D, 0D
!
!                        adams_view_name='jxr_joint_j_19'
MARKER/461
, PART = 53
, QP = 0, 0, -75
, REULER = 351.3688576D, 0D, 0D
!
!                        adams_view_name='jxr_joint_i_20'
MARKER/462
, PART = 53
!
!                        adams_view_name='jxr_joint_j_1'
MARKER/463
, PART = 53
!
!                       adams_view_name='jmr_actuator_j_1'
MARKER/464
, PART = 53
, REULER = 0D, 180D, 0D
!
!                       adams_view_name='mar_spindle_lock'
MARKER/465
, PART = 53
, REULER = 90D, 90D, 180D
!
!                     adams_view_name='i_graphic_MARKER_581'
MARKER/581
, PART = 53
!
!                adams_view_name='gracyl_cv_jt_housing_extension'
GRAPHICS/50
, CYLINDER
, CM = 460
, LENGTH = 50
, SIDES = 15
, RADIUS = 30
, SEG = 15
!
!                     adams_view_name='i_graphic_GCURVE_334'
GRAPHICS/334
, CURVE
, CID = 20
, CRM = 581
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.gel_drive_shaft'
PART/54
, QG = 30, -321, 0
, REULER = 176.0991766D, 89.91477819D, 171.3549137D
, MASS = 4.217452941
, CM = 468
, IM = 469
, IP = 1.659890656E+05, 1.659890656E+05, 692.8258537
!
!                              adams_view_name='cm'
MARKER/468
, PART = 54
, QP = 0, 0, -365.6817015
!
!                        adams_view_name='inertia_frame'
MARKER/469
, PART = 54
, QP = 0, 0, -365.6817015
!
!                           adams_view_name='gralin_3'
MARKER/470
, PART = 54
, QP = 0, 0, -440.0227701
!
!                           adams_view_name='graell_1'
MARKER/471
, PART = 54
, QP = 0, 0, -440.0227701
!
!                        adams_view_name='jxl_joint_j_18'
MARKER/472
, PART = 54
, REULER = 187.395471D, 180D, 0D
!
!                        adams_view_name='jxl_joint_i_19'
MARKER/473
, PART = 54
, QP = 0, 0, -440.0227701
!
!                      adams_view_name='gralin_drive_shaft'
GRAPHICS/51
, CYLINDER
, CM = 470
, LENGTH = 440.0227701
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                    adams_view_name='graell_otr_cv_housing'
GRAPHICS/94
, ELLIPSOID
, CM = 471
, XSCALE = 60
, YSCALE = 60
, ZSCALE = 60
!
!------------------------------------ Part -------------------------------------
!
!                   adams_view_name='FRT_SUSP.ger_drive_shaft'
PART/55
, QG = 30, 321, 0
, REULER = 3.900823428D, 89.91477819D, 8.645086317D
, MASS = 4.217452941
, CM = 474
, IM = 475
, IP = 1.659890656E+05, 1.659890656E+05, 692.8258537
!
!                              adams_view_name='cm'
MARKER/474
, PART = 55
, QP = 0, 0, -365.6817015
!
!                        adams_view_name='inertia_frame'
MARKER/475
, PART = 55
, QP = 0, 0, -365.6817015
!
!                           adams_view_name='gralin_4'
MARKER/476
, PART = 55
, QP = 0, 0, -440.0227701
!
!                           adams_view_name='graell_2'
MARKER/477
, PART = 55
, QP = 0, 0, -440.0227701
!
!                        adams_view_name='jxr_joint_j_18'
MARKER/478
, PART = 55
, REULER = 172.604529D, 180D, 0D
!
!                        adams_view_name='jxr_joint_i_19'
MARKER/479
, PART = 55
, QP = 0, 0, -440.0227701
!
!                      adams_view_name='gralin_drive_shaft'
GRAPHICS/52
, CYLINDER
, CM = 476
, LENGTH = 440.0227701
, SIDES = 15
, RADIUS = 15
, SEG = 15
!
!                    adams_view_name='graell_otr_cv_housing'
GRAPHICS/95
, ELLIPSOID
, CM = 477
, XSCALE = 60
, YSCALE = 60
, ZSCALE = 60
!
!------------------------------------ Part -------------------------------------
!
!                     adams_view_name='FRT_SUSP.gel_tripot'
PART/56
, QG = 30, -321, 0
, REULER = 180D, 90D, 358.7474825D
, MASS = 1.985112708
, CM = 480
, IM = 481
, IP = 1101.860091, 1101.860091, 813.8962101
!
!                              adams_view_name='cm'
MARKER/480
, PART = 56
, QP = 0, 0, 13.88888889
!
!                        adams_view_name='inertia_frame'
MARKER/481
, PART = 56
, QP = 0, 0, 13.88888889
!
!                           adams_view_name='gracyl_3'
MARKER/482
, PART = 56
!
!                           adams_view_name='graell_3'
MARKER/483
, PART = 56
!
!                        adams_view_name='jxl_joint_i_17'
MARKER/484
, PART = 56
!
!                        adams_view_name='jxl_joint_i_18'
MARKER/485
, PART = 56
!
!               adams_view_name='gracyl_tripot_housing_extention'
GRAPHICS/53
, CYLINDER
, CM = 482
, LENGTH = 50
, SIDES = 15
, RADIUS = 30
, SEG = 15
!
!                    adams_view_name='graell_tripot_housing'
GRAPHICS/96
, ELLIPSOID
, CM = 483
, XSCALE = 60
, YSCALE = 60
, ZSCALE = 60
!
!------------------------------------ Part -------------------------------------
!
!                     adams_view_name='FRT_SUSP.ger_tripot'
PART/57
, QG = 30, 321, 0
, REULER = 0D, 90D, 181.2525175D
, MASS = 1.985112708
, CM = 486
, IM = 487
, IP = 1101.860091, 1101.860091, 813.8962101
!
!                              adams_view_name='cm'
MARKER/486
, PART = 57
, QP = 0, 0, 13.88888889
!
!                        adams_view_name='inertia_frame'
MARKER/487
, PART = 57
, QP = 0, 0, 13.88888889
!
!                           adams_view_name='gracyl_4'
MARKER/488
, PART = 57
!
!                           adams_view_name='graell_4'
MARKER/489
, PART = 57
!
!                        adams_view_name='jxr_joint_i_17'
MARKER/490
, PART = 57
!
!                        adams_view_name='jxr_joint_i_18'
MARKER/491
, PART = 57
!
!               adams_view_name='gracyl_tripot_housing_extention'
GRAPHICS/54
, CYLINDER
, CM = 488
, LENGTH = 50
, SIDES = 15
, RADIUS = 30
, SEG = 15
!
!                    adams_view_name='graell_tripot_housing'
GRAPHICS/97
, ELLIPSOID
, CM = 489
, XSCALE = 60
, YSCALE = 60
, ZSCALE = 60
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!            adams_view_name='MDI_FRONT_STEERING.ges_steering_shaft'
PART/61
, QG = 165, -325, 120
, REULER = 83.92754359D, 59.35741874D, 273.1036171D
, MASS = 1.973672875
, CM = 504
, IM = 509
, IP = 20933.9283, 20933.9283, 223.3589429
!
!                           adams_view_name='gralin_1'
MARKER/503
, PART = 61
, QP = 0, 0, -274.6816339
!
!                              adams_view_name='cm'
MARKER/504
, PART = 61
!
!                        adams_view_name='jxs_joint_j_9'
MARKER/505
, PART = 61
, QP = 0, 0, 274.6816339
, REULER = 170.6136819D, 0D, 0D
!
!                adams_view_name='josrev_steering_input_shaft_1'
MARKER/506
, PART = 61
, QP = 0, 0, -274.6816339
!
!                        adams_view_name='jxs_joint_i_14'
MARKER/507
, PART = 61
, QP = 0, 0, -274.6816339
, REULER = 86.89638293D, 0D, 0D
!
!                       adams_view_name='bxs_bushing_i_1'
MARKER/508
, PART = 61
, QP = 0, 0, -274.6816339
!
!                        adams_view_name='inertia_frame'
MARKER/509
, PART = 61
!
!                       adams_view_name='bxs_bushgeom_i_1'
MARKER/510
, PART = 61
, QP = 0, 0, -287.1816339
, REULER = 270D, 0D, 0D
!
!                     adams_view_name='i_graphic_MARKER_585'
MARKER/585
, PART = 61
, QP = 0, 0, -277.1816339
!
!                    adams_view_name='gralin_steering_shaft'
GRAPHICS/73
, CYLINDER
, CM = 503
, LENGTH = 549.3632678
, SIDES = 15
, RADIUS = 15.04454593
, SEG = 15
!
!                     adams_view_name='i_graphic_GCURVE_346'
GRAPHICS/346
, CURVE
, CID = 24
, CRM = 585
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!                 adams_view_name='MDI_FRONT_STEERING.ges_rack'
PART/62
, QG = -70, 0, -20
, REULER = 0D, 90D, 0D
, MASS = 1.888888889
, CM = 512
, IM = 514
, IP = 1.137696706E+05, 1.137696706E+05, 85.63745492
!
!                           adams_view_name='gralin_2'
MARKER/511
, PART = 62
, QP = 0, 0, -390
!
!                              adams_view_name='cm'
MARKER/512
, PART = 62
!
!                        adams_view_name='jxs_joint_i_10'
MARKER/513
, PART = 62
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='inertia_frame'
MARKER/514
, PART = 62
!
!                    adams_view_name='steering_assist_vforce'
MARKER/515
, PART = 62
, REULER = 0D, 180D, 0D
!
!                        adams_view_name='jxl_joint_j_11'
MARKER/516
, PART = 62
, QP = -28.1, -20.41, 394.19
, REULER = 182.8583287D, 180D, 0D
!
!                        adams_view_name='jxr_joint_j_11'
MARKER/517
, PART = 62
, QP = -28.1, -20.41, -394.19
, REULER = 182.8583287D, 0D, 0D
!
!                         adams_view_name='gralin_rack'
GRAPHICS/74
, CYLINDER
, CM = 511
, LENGTH = 780
, SIDES = 15
, RADIUS = 9.522339643
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!            adams_view_name='MDI_FRONT_STEERING.ges_steering_wheel'
PART/63
, QG = 975, -350, 800
, REULER = 270D, 121.6863677D, 90D
, MASS = 2
, CM = 518
, IM = 521
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/518
, PART = 63
!
!                      adams_view_name='graphics_location'
MARKER/519
, PART = 63
, REULER = 180D, 0D, 0D
!
!                        adams_view_name='jxs_joint_i_11'
MARKER/520
, PART = 63
, REULER = 0D, 180D, 0D
!
!                        adams_view_name='inertia_frame'
MARKER/521
, PART = 63
!
!                       adams_view_name='jfs_actuator_i_1'
MARKER/522
, PART = 63
, REULER = 0D, 180D, 0D
!
!                adams_view_name='steering_wheel_rim_MARKER_582'
MARKER/582
, PART = 63
, QP = 3.846095791, 170, -13.46133527
!
!                             adams_view_name='hub'
GRAPHICS/75
, CYLINDER
, CM = 519
, LENGTH = 5
, SIDES = 3
, RADIUS = 170
, SEG = 3
!
!                adams_view_name='steering_wheel_rim_GCURVE_343'
GRAPHICS/343
, CURVE
, CID = 21
, CRM = 582
, SEG = 500
!
!                      adams_view_name='steering_wheel_rim'
GRAPHICS/154
, REVOLUTION
, CRM = 519
, SIDES = 30
, GID = 343
!
!------------------------------------ Part -------------------------------------
!
!                adams_view_name='MDI_FRONT_STEERING.ges_pinion'
PART/64
, QG = -70, -300, -20
, REULER = 83.92754359D, 59.35741874D, 273.1036171D
, MASS = 0.5
, CM = 523
, IM = 527
, IP = 1, 1, 1
!
!                              adams_view_name='cm'
MARKER/523
, PART = 64
, REULER = 90D, 45D, 270D
!
!                       adams_view_name='josrev_pinion_1'
MARKER/524
, PART = 64
!
!                        adams_view_name='jxs_joint_i_12'
MARKER/525
, PART = 64
, REULER = 266.8963829D, 180D, 0D
!
!                       adams_view_name='bxs_bushing_j_1'
MARKER/526
, PART = 64
!
!                        adams_view_name='inertia_frame'
MARKER/527
, PART = 64
!
!                       adams_view_name='bxs_bushgeom_j_1'
MARKER/528
, PART = 64
, QP = 0, 0, -12.5
!
!------------------------------------ Part -------------------------------------
!
!             adams_view_name='MDI_FRONT_STEERING.ges_rack_housing'
PART/65
, QG = -70, 0, -20
, REULER = 0D, 90D, 0D
, MASS = 4
, CM = 530
, IM = 537
, IP = 2.13537352E+05, 2.13537352E+05, 408.0372852
!
!                           adams_view_name='gralin_3'
MARKER/529
, PART = 65
, QP = 0, 0, -390
!
!                              adams_view_name='cm'
MARKER/530
, PART = 65
!
!                        adams_view_name='jxs_joint_j_10'
MARKER/531
, PART = 65
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='jxs_joint_j_12'
MARKER/532
, PART = 65
, QP = 0, 0, 300
, REULER = 300.7841465D, 95.22197079D, 93.10361707D
!
!                        adams_view_name='jxs_joint_j_14'
MARKER/533
, PART = 65
, QP = 0, 0, 300
, REULER = 120.7841465D, 84.77802921D, 266.8963829D
!
!                        adams_view_name='jxs_joint_i_15'
MARKER/534
, PART = 65
, REULER = 0D, 180D, 0D
!
!                       adams_view_name='bxl_bushing_i_1'
MARKER/535
, PART = 65
, QP = 0, 0, 390
, REULER = 0D, 180D, 0D
!
!                       adams_view_name='bxr_bushing_i_1'
MARKER/536
, PART = 65
, QP = 0, 0, -390
!
!                        adams_view_name='inertia_frame'
MARKER/537
, PART = 65
!
!                       adams_view_name='bxl_bushgeom_i_1'
MARKER/538
, PART = 65
, QP = 0, 0, 402.5
, REULER = 90D, 180D, 0D
!
!                       adams_view_name='bxr_bushgeom_i_1'
MARKER/539
, PART = 65
, QP = 0, 0, -402.5
, REULER = 270D, 0D, 0D
!
!                             adams_view_name='FMA'
MARKER/540
, PART = 65
, FLOATING
!
!                     adams_view_name='i_graphic_MARKER_583'
MARKER/583
, PART = 65
, QP = 0, 0, 392.5
!
!                     adams_view_name='i_graphic_MARKER_584'
MARKER/584
, PART = 65
, QP = 0, 0, -392.5
!
!                     adams_view_name='gralin_rack_housing'
GRAPHICS/76
, CYLINDER
, CM = 529
, LENGTH = 780
, SIDES = 15
, RADIUS = 14.28350946
, SEG = 15
!
!                     adams_view_name='i_graphic_GCURVE_344'
GRAPHICS/344
, CURVE
, CID = 22
, CRM = 583
, SEG = 500
!
!                     adams_view_name='i_graphic_GCURVE_345'
GRAPHICS/345
, CURVE
, CID = 23
, CRM = 584
, SEG = 500
!
!------------------------------------ Part -------------------------------------
!
!            adams_view_name='MDI_FRONT_STEERING.ges_steering_column'
PART/66
, QG = 772.5, -350, 675
, REULER = 270D, 121.6863677D, 90D
, MASS = 2.268238449
, CM = 542
, IM = 545
, IP = 32340.84222, 32340.84222, 254.2615078
!
!                           adams_view_name='gralin_4'
MARKER/541
, PART = 66
, QP = 0, 0, -237.9732128
!
!                              adams_view_name='cm'
MARKER/542
, PART = 66
!
!                        adams_view_name='jxs_joint_i_8'
MARKER/543
, PART = 66
, QP = 0, 0, 237.9732128
, REULER = 180D, 180D, 0D
!
!                        adams_view_name='jxs_joint_i_13'
MARKER/544
, PART = 66
, QP = 0, 0, -137.9732128
, REULER = 90D, 180D, 0D
!
!                        adams_view_name='inertia_frame'
MARKER/545
, PART = 66
!
!                    adams_view_name='gralin_steering_column'
GRAPHICS/77
, CYLINDER
, CM = 541
, LENGTH = 475.9464256
, SIDES = 15
, RADIUS = 14.97307338
, SEG = 15
!
!------------------------------------ Part -------------------------------------
!
!          adams_view_name='MDI_FRONT_STEERING.ges_intermediate_shaft'
PART/67
, QG = 485, -350, 405
, REULER = 90D, 30.37912601D, 270D
, MASS = 1.18711026
, CM = 547
, IM = 550
, IP = 4597.976307, 4597.976307, 134.344296
!
!                           adams_view_name='gralin_5'
MARKER/546
, PART = 67
, QP = 0, 0, -168.0773631
!
!                              adams_view_name='cm'
MARKER/547
, PART = 67
!
!                        adams_view_name='jxs_joint_j_8'
MARKER/548
, PART = 67
, QP = 0, 0, 168.0773631
!
!                        adams_view_name='jxs_joint_i_9'
MARKER/549
, PART = 67
, QP = 0, 0, -168.0773631
, REULER = 169.2702549D, 0D, 0D
!
!                        adams_view_name='inertia_frame'
MARKER/550
, PART = 67
!
!                          adams_view_name='graell_13'
MARKER/551
, PART = 67
, QP = 0, 0, 168.0773631
, REULER = 270D, 30.37912601D, 90D
!
!                          adams_view_name='graell_14'
MARKER/552
, PART = 67
, QP = 0, 0, -168.0773631
, REULER = 270D, 30.37912601D, 90D
!
!                  adams_view_name='gralin_intermediate_shaft'
GRAPHICS/78
, CYLINDER
, CM = 546
, LENGTH = 336.1547263
, SIDES = 15
, RADIUS = 15.04454593
, SEG = 15
!
!                        adams_view_name='graell_column'
GRAPHICS/99
, ELLIPSOID
, CM = 551
, XSCALE = 30.08909186
, YSCALE = 30.08909186
, ZSCALE = 30.08909186
!
!                      adams_view_name='graell_intermdiate'
GRAPHICS/100
, ELLIPSOID
, CM = 552
, XSCALE = 30.08909186
, YSCALE = 30.08909186
, ZSCALE = 30.08909186
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!------------------------------------ Part -------------------------------------
!
!           adams_view_name='MDI_FRONT_STEERING.sws_rack_house_mount'
PART/71
, QG = -70, 0, -20
!
!                           adams_view_name='switch_i'
MARKER/556
, PART = 71
!
!                        adams_view_name='jxs_joint_j_15'
MARKER/557
, PART = 71
, REULER = 180D, 90D, 180D
!
!                       adams_view_name='bxl_bushing_j_1'
MARKER/558
, PART = 71
, QP = 0, -390, 0
, REULER = 180D, 90D, 180D
!
!                       adams_view_name='bxr_bushing_j_1'
MARKER/559
, PART = 71
, QP = 0, 390, 0
, REULER = 0D, 90D, 0D
!
!                       adams_view_name='bxl_bushgeom_j_1'
MARKER/560
, PART = 71
, QP = 0, -402.5, 0
, REULER = 180D, 90D, 180D
!
!                       adams_view_name='bxr_bushgeom_j_1'
MARKER/561
, PART = 71
, QP = 0, 402.5, 0
, REULER = 0D, 90D, 0D
!
!------------------------------ DYNAMIC GRAPHICS -------------------------------
!
!                         adams_view_name='testrig.left'
GRAPHICS/1
, FORCE
, ETYPE = GFORCE
, EID = 1
, EMARKER = 75
!
!                        adams_view_name='testrig.right'
GRAPHICS/2
, FORCE
, ETYPE = GFORCE
, EID = 2
, EMARKER = 82
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.j_graphic'
GRAPHICS/55
, CYLINDER
, CM = 21
, LENGTH = 20
, SIDES = 12
, RADIUS = 30
, SEG = 12
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.j_graphic'
GRAPHICS/56
, CYLINDER
, CM = 22
, LENGTH = 20
, SIDES = 12
, RADIUS = 30
, SEG = 12
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.j_graphic'
GRAPHICS/57
, CYLINDER
, CM = 23
, LENGTH = 20
, SIDES = 12
, RADIUS = 30
, SEG = 12
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.j_graphic'
GRAPHICS/70
, CYLINDER
, CM = 20
, LENGTH = 20
, SIDES = 12
, RADIUS = 30
, SEG = 12
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.j_graphic'
GRAPHICS/80
, CYLINDER
, CM = 560
, LENGTH = 25
, SIDES = 12
, RADIUS = 20
, SEG = 12
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.j_graphic'
GRAPHICS/81
, CYLINDER
, CM = 561
, LENGTH = 25
, SIDES = 12
, RADIUS = 20
, SEG = 12
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.j_graphic'
GRAPHICS/82
, CYLINDER
, CM = 528
, LENGTH = 25
, SIDES = 12
, RADIUS = 20
, SEG = 12
!
!               adams_view_name='testrig.rer_retract_stop.graphic'
GRAPHICS/125
, SPDP
, I = 133
, J = 10
, COILS = 0
, DB = 57.6
, DC = 64
, LB = 510
, LC = 2
, LD = 10
!
!               adams_view_name='testrig.rel_retract_stop.graphic'
GRAPHICS/126
, SPDP
, I = 123
, J = 5
, COILS = 0
, DB = 57.6
, DC = 64
, LB = 510
, LC = 2
, LD = 10
!
!               adams_view_name='FRT_SUSP.nsl_ride_spring.graphic'
GRAPHICS/127
, SPDP
, I = 26
, J = 426
, COILS = 5
, DA = 125.0735823
, DB = 125.0735823
, DC = 125.0735823
, LC = -6.414029862
, LD = -6.414029862
!
!               adams_view_name='FRT_SUSP.nsr_ride_spring.graphic'
GRAPHICS/128
, SPDP
, I = 30
, J = 435
, COILS = 5
, DA = 125.0735823
, DB = 125.0735823
, DC = 125.0735823
, LC = -6.414029862
, LD = -6.414029862
!
!               adams_view_name='FRT_SUSP.dal_ride_damper.graphic'
GRAPHICS/129
, SPDP
, I = 380
, J = 425
, COILS = 0
, DB = 76.96835834
, DC = 61.57468667
, LC = 384.8417917
, LD = 384.8417917
!
!               adams_view_name='FRT_SUSP.dar_ride_damper.graphic'
GRAPHICS/130
, SPDP
, I = 388
, J = 434
, COILS = 0
, DB = 76.96835834
, DC = 61.57468667
, LC = 384.8417917
, LD = 384.8417917
!
!               adams_view_name='FRT_SUSP.bul_jounce_stop.graphic'
GRAPHICS/131
, SPDP
, I = 379
, J = 422
, COILS = 0
, DB = 110.2760105
, DC = 99.24840941
, LB = 661.7250653
, LC = 2
, LD = 10
!
!               adams_view_name='FRT_SUSP.bur_jounce_stop.graphic'
GRAPHICS/132
, SPDP
, I = 387
, J = 431
, COILS = 0
, DB = 110.2760105
, DC = 99.24840941
, LB = 661.7250653
, LC = 2
, LD = 10
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.i_graphic'
GRAPHICS/136
, REVOLUTION
, CRM = 361
, SIDES = 2
, GID = 181
, RANGLE = 180D
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.i_graphic'
GRAPHICS/137
, REVOLUTION
, CRM = 362
, SIDES = 2
, GID = 190
, RANGLE = 180D
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.i_graphic'
GRAPHICS/138
, REVOLUTION
, CRM = 363
, SIDES = 2
, GID = 199
, RANGLE = 180D
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.i_graphic'
GRAPHICS/151
, REVOLUTION
, CRM = 360
, SIDES = 2
, GID = 316
, RANGLE = 180D
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.i_graphic'
GRAPHICS/155
, REVOLUTION
, CRM = 538
, SIDES = 2
, GID = 344
, RANGLE = 180D
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.i_graphic'
GRAPHICS/156
, REVOLUTION
, CRM = 539
, SIDES = 2
, GID = 345
, RANGLE = 180D
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.i_graphic'
GRAPHICS/157
, REVOLUTION
, CRM = 510
, SIDES = 2
, GID = 346
, RANGLE = 180D
!
!-------------------------------- CONSTRAINTS ----------------------------------
!
!Dummy for communicators
!                     adams_view_name='_cv_joint_for_motion'
JOINT/1
, CYLINDRICAL
, I = 45
, J = 2
!
!                 adams_view_name='testrig.jorrev_wheel_bearing'
JOINT/4
, REVOLUTE
, I = 86
, J = 463
!
!                 adams_view_name='testrig.jolrev_wheel_bearing'
JOINT/5
, REVOLUTE
, I = 79
, J = 450
!
!                 adams_view_name='testrig.joltra_vertical_jack'
JOINT/8
, TRANSLATIONAL
, I = 119
, J = 3
!
!                 adams_view_name='testrig.jortra_vertical_jack'
JOINT/9
, TRANSLATIONAL
, I = 129
, J = 8
!
!Steering Input Joint for Motion Control
!             adams_view_name='testrig.jostra_steering_input_slider'
JOINT/10
, TRANSLATIONAL
, I = 140
, J = 60
!
!Steering Part Constraint for Coupling to Steering Subsystem
!                 adams_view_name='testrig.jostra_steering_part'
JOINT/11
, TRANSLATIONAL
, I = 143
, J = 61
!
!          adams_view_name='testrig.jostra_steering_input_translation'
JOINT/12
, TRANSLATIONAL
, I = 146
, J = 63
!
!            adams_view_name='testrig.jostra_steering_input_rotation'
JOINT/13
, TRANSLATIONAL
, I = 148
, J = 64
!
!                  adams_view_name='testrig.jolrev_diff_output'
JOINT/14
, REVOLUTE
, I = 151
, J = 13
!
!                  adams_view_name='testrig.jorrev_diff_output'
JOINT/15
, REVOLUTE
, I = 156
, J = 14
!
!                  adams_view_name='testrig.jorfix_table_fixed'
JOINT/19
, FIXED
, I = 108
, J = 132
!
!                  adams_view_name='testrig.jolfix_table_fixed'
JOINT/20
, FIXED
, I = 95
, J = 122
!
!                  adams_view_name='FRT_SUSP.joltra_lca_split'
JOINT/25
, TRANSLATIONAL
, I = 269
, J = 229
!
!                  adams_view_name='FRT_SUSP.jortra_lca_split'
JOINT/26
, TRANSLATIONAL
, I = 288
, J = 236
!
!                 adams_view_name='FRT_SUSP.joltra_tierod_split'
JOINT/27
, TRANSLATIONAL
, I = 258
, J = 244
!
!                 adams_view_name='FRT_SUSP.jortra_tierod_split'
JOINT/28
, TRANSLATIONAL
, I = 265
, J = 251
!
!                     adams_view_name='FRT_SUSP.jklrev_lca'
JOINT/29
, REVOLUTE
, I = 272
, J = 364
!
!                     adams_view_name='FRT_SUSP.jkrrev_lca'
JOINT/30
, REVOLUTE
, I = 291
, J = 365
!
!                adams_view_name='FRT_SUSP.jolsph_lca_balljoint'
JOINT/31
, SPHERICAL
, I = 309
, J = 232
!
!                adams_view_name='FRT_SUSP.jorsph_lca_balljoint'
JOINT/32
, SPHERICAL
, I = 328
, J = 239
!
!                 adams_view_name='FRT_SUSP.jolsph_tierod_outer'
JOINT/33
, SPHERICAL
, I = 260
, J = 310
!
!                 adams_view_name='FRT_SUSP.jorsph_tierod_outer'
JOINT/34
, SPHERICAL
, I = 266
, J = 329
!
!                 adams_view_name='FRT_SUSP.jolcon_tierod_inner'
JOINT/37
, CONVEL
, I = 246
, J = 516
!
!                 adams_view_name='FRT_SUSP.jorcon_tierod_inner'
JOINT/38
, CONVEL
, I = 253
, J = 517
!
!             adams_view_name='FRT_SUSP.jklhoo_top_mount_kinematic'
JOINT/43
, HOOKE
, I = 376
, J = 24
!
!             adams_view_name='FRT_SUSP.jkrhoo_top_mount_kinematic'
JOINT/44
, HOOKE
, I = 384
, J = 28
!
!                adams_view_name='FRT_SUSP.jolsph_uca_balljoint'
JOINT/45
, SPHERICAL
, I = 397
, J = 311
!
!                adams_view_name='FRT_SUSP.jorsph_uca_balljoint'
JOINT/46
, SPHERICAL
, I = 409
, J = 330
!
!                adams_view_name='FRT_SUSP.jolcyl_lwr_upr_strut'
JOINT/47
, CYLINDRICAL
, I = 421
, J = 378
!
!                adams_view_name='FRT_SUSP.jorcyl_lwr_upr_strut'
JOINT/48
, CYLINDRICAL
, I = 430
, J = 386
!
!                     adams_view_name='FRT_SUSP.jklrev_uca'
JOINT/51
, REVOLUTE
, I = 398
, J = 32
!
!                     adams_view_name='FRT_SUSP.jkrrev_uca'
JOINT/52
, REVOLUTE
, I = 410
, J = 37
!
!                     adams_view_name='FRT_SUSP.swl_fixed_1'
JOINT/53
, FIXED
, I = 440
, J = 312
!
!                     adams_view_name='FRT_SUSP.swr_fixed_1'
JOINT/54
, FIXED
, I = 441
, J = 331
!
!             adams_view_name='FRT_SUSP.jklhoo_lwr_strut_kinematic'
JOINT/55
, HOOKE
, I = 423
, J = 274
!
!             adams_view_name='FRT_SUSP.jkrhoo_lwr_strut_kinematic'
JOINT/56
, HOOKE
, I = 432
, J = 293
!
!            adams_view_name='FRT_SUSP.joltra_tripot_to_differential'
JOINT/59
, TRANSLATIONAL
, I = 484
, J = 153
!
!            adams_view_name='FRT_SUSP.jortra_tripot_to_differential'
JOINT/60
, TRANSLATIONAL
, I = 490
, J = 158
!
!               adams_view_name='FRT_SUSP.jolcon_drive_sft_int_jt'
JOINT/61
, CONVEL
, I = 485
, J = 472
!
!               adams_view_name='FRT_SUSP.jorcon_drive_sft_int_jt'
JOINT/62
, CONVEL
, I = 491
, J = 478
!
!                adams_view_name='FRT_SUSP.jolcon_drive_sft_otr'
JOINT/63
, CONVEL
, I = 473
, J = 448
!
!                adams_view_name='FRT_SUSP.jorcon_drive_sft_otr'
JOINT/64
, CONVEL
, I = 479
, J = 461
!
!               adams_view_name='FRT_SUSP.jolrev_spindle_upright'
JOINT/65
, REVOLUTE
, I = 449
, J = 314
!
!               adams_view_name='FRT_SUSP.jorrev_spindle_upright'
JOINT/66
, REVOLUTE
, I = 462
, J = 333
!
!        adams_view_name='MDI_FRONT_STEERING.joshoo_column_intermediate'
JOINT/69
, HOOKE
, I = 543
, J = 548
!
!      adams_view_name='MDI_FRONT_STEERING.joshoo_intermediate_shaftinput'
JOINT/70
, HOOKE
, I = 549
, J = 505
!
!        adams_view_name='MDI_FRONT_STEERING.jostra_rack_to_rackhousing'
JOINT/71
, TRANSLATIONAL
, I = 513
, J = 531
!
!           adams_view_name='MDI_FRONT_STEERING.josrev_steering_wheel'
JOINT/74
, REVOLUTE
, I = 520
, J = 42
!
!               adams_view_name='MDI_FRONT_STEERING.josrev_pinion'
JOINT/75
, REVOLUTE
, I = 525
, J = 532
!
!      adams_view_name='MDI_FRONT_STEERING.joscyl_steering_column_to_body'
JOINT/76
, CYLINDRICAL
, I = 544
, J = 43
!
!        adams_view_name='MDI_FRONT_STEERING.josrev_steering_input_shaft'
JOINT/77
, REVOLUTE
, I = 507
, J = 533
!
!                adams_view_name='MDI_FRONT_STEERING.sws_fixed_1'
JOINT/79
, FIXED
, I = 556
, J = 44
!
!Dummy for communicators
!                          adams_view_name='_cv_joint'
JPRIM/1
, INPLANE
, I = 45
, J = 2
!
!Active when steering_input=length
!              adams_view_name='testrig.steering_input_driver_tra'
JPRIM/3
, INPLANE
, I = 146
, J = 143
!
!                  adams_view_name='testrig.spindle_lock_left'
JPRIM/7
, PERPENDICULAR
, I = 452
, J = 325
!
!                  adams_view_name='testrig.spindle_lock_right'
JPRIM/8
, PERPENDICULAR
, I = 465
, J = 344
!
!Couples the test rig to the rotational steering part from the steering subsystem 
!          adams_view_name='testrig.steering_input_coupler_rotational'
COUPLER/1
, JOINTS = 13, 74
, TYPE = T:R
, SCALES = 1, -1
!
!Couples the test rig to the translational steering part from the steering subsystem
!         adams_view_name='testrig.steering_input_coupler_translational'
COUPLER/2
, JOINTS = 12, 71
, TYPE = T:T
, SCALES = 1, -1
!
!     adams_view_name='MDI_FRONT_STEERING.grsred_steering_wheel_column_lock'
COUPLER/4
, JOINTS = 74, 76
, TYPE = R:R
, SCALES = -1, 1
!
!           adams_view_name='MDI_FRONT_STEERING.grsred_pinion_to_rack'
COUPLER/5
, JOINTS = 75, 71
, TYPE = R:T
, SCALES = 1, 0.1745329252
!
!Dummy for communicators
!                          adams_view_name='_cv_motion'
MOTION/1
, ROTATIONAL
, JOINT = 1
, FUNCTION = 0
!
!Steering Motion Driven From Loadcase Spline
!                    adams_view_name='testrig.steering_input'
MOTION/2
, TRANSLATIONAL
, JOINT = 10
, FUNCTION = AKISPL(19,time,2)
!
!               adams_view_name='testrig.jml_bearing_lock.motion'
MOTION/3
, I = 80
, J = 451
, B3
, FUNCTION = 0.0
!
!               adams_view_name='testrig.jmr_bearing_lock.motion'
MOTION/4
, I = 87
, J = 464
, B3
, FUNCTION = 0.0
!
!             adams_view_name='FRT_SUSP.afl_camber_adjuster.motion'
MOTION/9
, I = 270
, J = 230
, Z
, FUNCTION = 135.183165+0.0
!
!             adams_view_name='FRT_SUSP.afr_camber_adjuster.motion'
MOTION/10
, I = 289
, J = 237
, Z
, FUNCTION = 135.183165+0.0
!
!               adams_view_name='FRT_SUSP.afl_toe_adjuster.motion'
MOTION/11
, I = 245
, J = 259
, Z
, FUNCTION = 420.0035259+0.0
!
!               adams_view_name='FRT_SUSP.afr_toe_adjuster.motion'
MOTION/12
, I = 252
, J = 267
, Z
, FUNCTION = 420.0035259+0.0
!
!----------------------------------- FORCES ------------------------------------
!
!              adams_view_name='FRT_SUSP.bgr_subframe_front.field'
FIELD/2
, I = 348
, J = 17
, FORMULATION = LINEAR
, LENGTH_TOL = 1.0E-05
, FUNCTION = USER(910, 2, 60, 61, 62, 63, 64, 65)\
, ROUTINE = abgFDM::fie910
!
!               adams_view_name='FRT_SUSP.bgl_subframe_rear.field'
FIELD/3
, I = 349
, J = 18
, FORMULATION = LINEAR
, LENGTH_TOL = 1.0E-05
, FUNCTION = USER(910, 2, 84, 85, 86, 87, 88, 89)\
, ROUTINE = abgFDM::fie910
!
!               adams_view_name='FRT_SUSP.bgr_subframe_rear.field'
FIELD/4
, I = 350
, J = 19
, FORMULATION = LINEAR
, LENGTH_TOL = 1.0E-05
, FUNCTION = USER(910, 2, 108, 109, 110, 111, 112, 113)\
, ROUTINE = abgFDM::fie910
!
!              adams_view_name='FRT_SUSP.bgl_subframe_front.field'
FIELD/17
, I = 347
, J = 16
, FORMULATION = LINEAR
, LENGTH_TOL = 1.0E-05
, FUNCTION = USER(910, 2, 420, 421, 422, 423, 424, 425)\
, ROUTINE = abgFDM::fie910
!
!      adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.field'
FIELD/20
, I = 535
, J = 558
, FORMULATION = LINEAR
, LENGTH_TOL = 1.0E-05
, FUNCTION = USER(910, 2, 496, 497, 498, 499, 500, 501)\
, ROUTINE = abgFDM::fie910
!
!      adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.field'
FIELD/21
, I = 536
, J = 559
, FORMULATION = LINEAR
, LENGTH_TOL = 1.0E-05
, FUNCTION = USER(910, 2, 520, 521, 522, 523, 524, 525)\
, ROUTINE = abgFDM::fie910
!
!           adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.field'
FIELD/22
, I = 508
, J = 526
, FORMULATION = LINEAR
, LENGTH_TOL = 1.0E-05
, FUNCTION = USER(910, 2, 544, 545, 546, 547, 548, 549)\
, ROUTINE = abgFDM::fie910
!
!                 adams_view_name='testrig.jfl_jack_force.force'
SFORCE/1
, TRANSLATIONAL
, I = 120
, J = 120
, ACTIONONLY
, FUNCTION = DIF(2)
!
!                adams_view_name='testrig.jfl_jack_force.force_j'
SFORCE/2
, TRANSLATIONAL
, I = 4
, J = 4
, ACTIONONLY
, FUNCTION = DIF(2)
!
!                 adams_view_name='testrig.jfr_jack_force.force'
SFORCE/3
, TRANSLATIONAL
, I = 130
, J = 130
, ACTIONONLY
, FUNCTION = DIF(3)
!
!                adams_view_name='testrig.jfr_jack_force.force_j'
SFORCE/4
, TRANSLATIONAL
, I = 9
, J = 9
, ACTIONONLY
, FUNCTION = DIF(3)
!
!                adams_view_name='testrig.rer_retract_stop.force'
SFORCE/5
, TRANSLATIONAL
, I = 133
, J = 10
, FUNCTION = -1.0*1.0*AKISPL(max(0,dm(133,10)-520.0),0,5)
!
!                adams_view_name='testrig.rel_retract_stop.force'
SFORCE/6
, TRANSLATIONAL
, I = 123
, J = 5
, FUNCTION = -1.0*1.0*AKISPL(max(0,dm(123,5)-520.0),0,7)
!
!               adams_view_name='testrig.jfs_steering_input.force'
SFORCE/11
, TRANSLATIONAL
, I = 141
, J = 141
, ACTIONONLY
, FUNCTION = DIF(4)
!
!              adams_view_name='testrig.jfs_steering_input.force_j'
SFORCE/12
, TRANSLATIONAL
, I = 144
, J = 144
, ACTIONONLY
, FUNCTION = DIF(4)
!
!                adams_view_name='FRT_SUSP.nsl_ride_spring.force'
SFORCE/13
, TRANSLATIONAL
, I = 26
, J = 426
, FUNCTION = 1.0*akispl(380.6514931-dm(26,426),0,279)
!
!                adams_view_name='FRT_SUSP.nsr_ride_spring.force'
SFORCE/14
, TRANSLATIONAL
, I = 30
, J = 435
, FUNCTION = 1.0*akispl(380.6514931-dm(30,435),0,280)
!
!                adams_view_name='FRT_SUSP.dal_ride_damper.force'
SFORCE/15
, TRANSLATIONAL
, I = 380
, J = 425
, FUNCTION = step(vr(380,425), -1e-4, 1.0, 1e-4, 1.0)*akispl(vr(380,425),0,281)
!
!                adams_view_name='FRT_SUSP.dar_ride_damper.force'
SFORCE/16
, TRANSLATIONAL
, I = 388
, J = 434
, FUNCTION = step(vr(388,434), -1e-4, 1.0, 1e-4, 1.0)*akispl(vr(388,434),0,283)
!
!                adams_view_name='FRT_SUSP.bul_jounce_stop.force'
SFORCE/21
, TRANSLATIONAL
, I = 379
, J = 422
, FUNCTION = 1.0*AKISPL(max(0,671.7250653-dm(379,422)),0,339)
!
!                adams_view_name='FRT_SUSP.bur_jounce_stop.force'
SFORCE/22
, TRANSLATIONAL
, I = 387
, J = 431
, FUNCTION = 1.0*AKISPL(max(0,671.7250653-dm(387,431)),0,341)
!
!          adams_view_name='MDI_FRONT_STEERING.steering_assist_vforce'
VFORCE/1
, I = 515
, JFLOAT = 540
, RM = 515
, FX = 0\
, FY = 0\
, FZ = 490.87*AKISPL(AZ(508,526)*57.29577951,0,343)
!
!                   adams_view_name='testrig.til_wheel.force'
GFORCE/1
, I = 75
, JFLOAT = 100
, RM = 90
, FUNCTION = USER(900, 1, 11)\
, ROUTINE = abgTire::gfo900
!
!                   adams_view_name='testrig.tir_wheel.force'
GFORCE/2
, I = 82
, JFLOAT = 113
, RM = 103
, FUNCTION = USER(900, 2, 12)\
, ROUTINE = abgTire::gfo900
!
!------------------------------ DATA STRUCTURES --------------------------------
!
!                        adams_view_name='assembly_name'
STRING/1
, STRING =double_wishbone
!
!                         adams_view_name='file_prefix'
STRING/2
, STRING =STEER_steering
!
!Memory for Adams Car minor role for solver
!                  adams_view_name='testrig.minor_role_string'
STRING/3
, STRING =any
!
!                   adams_view_name='testrig.simulation_type'
STRING/4
, STRING =SUSPENSION
!
!                  adams_view_name='testrig.til_wheel.tpf_file'
STRING/5
, STRING =RIGID_WHEEL
!
!                  adams_view_name='testrig.til_wheel.rpf_file'
STRING/6
, STRING =BEDPLATE
!
!                  adams_view_name='testrig.til_wheel.contact'
STRING/7
, STRING =SUSPENSION
!
!              adams_view_name='testrig.til_wheel.simulation_type'
STRING/8
, STRING =SUSPENSION
!
!                  adams_view_name='testrig.tir_wheel.tpf_file'
STRING/9
, STRING =RIGID_WHEEL
!
!                  adams_view_name='testrig.tir_wheel.rpf_file'
STRING/10
, STRING =BEDPLATE
!
!                  adams_view_name='testrig.tir_wheel.contact'
STRING/11
, STRING =SUSPENSION
!
!              adams_view_name='testrig.tir_wheel.simulation_type'
STRING/12
, STRING =SUSPENSION
!
!           adams_view_name='testrig.jml_bearing_lock.str_application'
STRING/13
, STRING =wheel_lock
!
!           adams_view_name='testrig.jml_bearing_lock.str_identifier'
STRING/14
, STRING =wheel_bearing_lock
!
!              adams_view_name='testrig.jml_bearing_lock.str_unit'
STRING/15
, STRING =angle
!
!           adams_view_name='testrig.jmr_bearing_lock.str_application'
STRING/16
, STRING =wheel_lock
!
!           adams_view_name='testrig.jmr_bearing_lock.str_identifier'
STRING/17
, STRING =wheel_bearing_lock
!
!              adams_view_name='testrig.jmr_bearing_lock.str_unit'
STRING/18
, STRING =angle
!
!            adams_view_name='testrig.jfl_jack_force.str_application'
STRING/19
, STRING =wheel_travel
!
!            adams_view_name='testrig.jfl_jack_force.str_identifier'
STRING/20
, STRING =jack_force
!
!               adams_view_name='testrig.jfl_jack_force.str_unit'
STRING/21
, STRING =force
!
!            adams_view_name='testrig.jfr_jack_force.str_application'
STRING/22
, STRING =wheel_travel
!
!            adams_view_name='testrig.jfr_jack_force.str_identifier'
STRING/23
, STRING =jack_force
!
!               adams_view_name='testrig.jfr_jack_force.str_unit'
STRING/24
, STRING =force
!
!          adams_view_name='testrig.jfs_steering_input.str_application'
STRING/37
, STRING =demand
!
!          adams_view_name='testrig.jfs_steering_input.str_identifier'
STRING/38
, STRING =steering
!
!             adams_view_name='testrig.jfs_steering_input.str_unit'
STRING/39
, STRING =force
!
!                  adams_view_name='FRT_SUSP.minor_role_string'
STRING/54
, STRING =front
!
!          adams_view_name='FRT_SUSP.afl_camber_adjuster.type_astring'
STRING/55
, STRING =camber
!
!          adams_view_name='FRT_SUSP.afr_camber_adjuster.type_astring'
STRING/56
, STRING =camber
!
!            adams_view_name='FRT_SUSP.afl_toe_adjuster.type_astring'
STRING/57
, STRING =toe
!
!            adams_view_name='FRT_SUSP.afr_toe_adjuster.type_astring'
STRING/58
, STRING =toe
!
!             adams_view_name='MDI_FRONT_STEERING.minor_role_string'
STRING/59
, STRING =front
!
!                         adams_view_name='plugin_list'
STRING/60
, STRING =acar:aexplore
!
!This spline is used to store the data from a loadcase file with x values being the
!component or column numbers and z values being the loadcase number (mapped to time)
!                   adams_view_name='testrig.loadcase_spline'
SPLINE/2
, X = 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19
, Y = 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0
, Y = 1, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -70
, Y = 2, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -69
, Y = 3, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -68
, Y = 4, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -67
, Y = 5, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -66
, Y = 6, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -65
, Y = 7, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -64
, Y = 8, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -63
, Y = 9, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -62
, Y = 10, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -61
, Y = 11, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -60
, Y = 12, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -59
, Y = 13, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -58
, Y = 14, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -57
, Y = 15, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -56
, Y = 16, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -55
, Y = 17, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -54
, Y = 18, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -53
, Y = 19, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -52
, Y = 20, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -51
, Y = 21, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -50
, Y = 22, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -49
, Y = 23, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -48
, Y = 24, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -47
, Y = 25, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -46
, Y = 26, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -45
, Y = 27, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -44
, Y = 28, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -43
, Y = 29, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -42
, Y = 30, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -41
, Y = 31, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -40
, Y = 32, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -39
, Y = 33, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -38
, Y = 34, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -37
, Y = 35, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -36
, Y = 36, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -35
, Y = 37, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -34
, Y = 38, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -33
, Y = 39, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -32
, Y = 40, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -31
, Y = 41, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -30
, Y = 42, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -29
, Y = 43, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -28
, Y = 44, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -27
, Y = 45, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -26
, Y = 46, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -25
, Y = 47, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -24
, Y = 48, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -23
, Y = 49, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -22
, Y = 50, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -21
, Y = 51, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -20
, Y = 52, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -19
, Y = 53, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -18
, Y = 54, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -17
, Y = 55, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -16
, Y = 56, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -15
, Y = 57, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -14
, Y = 58, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -13
, Y = 59, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -12
, Y = 60, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -11
, Y = 61, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -10
, Y = 62, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -9
, Y = 63, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -8
, Y = 64, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -7
, Y = 65, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -6
, Y = 66, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -5
, Y = 67, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -4
, Y = 68, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -3
, Y = 69, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -2
, Y = 70, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, -1
, Y = 71, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0
, Y = 72, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 1
, Y = 73, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 2
, Y = 74, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 3
, Y = 75, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 4
, Y = 76, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 5
, Y = 77, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 6
, Y = 78, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 7
, Y = 79, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 8
, Y = 80, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 9
, Y = 81, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 10
, Y = 82, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 11
, Y = 83, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 12
, Y = 84, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 13
, Y = 85, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 14
, Y = 86, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 15
, Y = 87, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 16
, Y = 88, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 17
, Y = 89, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 18
, Y = 90, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 19
, Y = 91, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 20
, Y = 92, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 21
, Y = 93, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 22
, Y = 94, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 23
, Y = 95, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 24
, Y = 96, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 25
, Y = 97, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 26
, Y = 98, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 27
, Y = 99, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 28
, Y = 100, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 29
, Y = 101, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 30
, Y = 102, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 31
, Y = 103, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 32
, Y = 104, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 33
, Y = 105, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 34
, Y = 106, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 35
, Y = 107, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 36
, Y = 108, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 37
, Y = 109, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 38
, Y = 110, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 39
, Y = 111, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 40
, Y = 112, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 41
, Y = 113, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 42
, Y = 114, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 43
, Y = 115, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 44
, Y = 116, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 45
, Y = 117, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 46
, Y = 118, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 47
, Y = 119, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 48
, Y = 120, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 49
, Y = 121, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 50
, Y = 122, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 51
, Y = 123, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 52
, Y = 124, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 53
, Y = 125, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 54
, Y = 126, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 55
, Y = 127, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 56
, Y = 128, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 57
, Y = 129, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 58
, Y = 130, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 59
, Y = 131, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 60
, Y = 132, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 61
, Y = 133, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 62
, Y = 134, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 63
, Y = 135, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 64
, Y = 136, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 65
, Y = 137, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 66
, Y = 138, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 67
, Y = 139, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 68
, Y = 140, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 69
, Y = 141, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 70
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='testrig.rer_retract_stop.spline'
SPLINE/5
, X = 0, 2, 4, 6, 8, 10, 20, 30, 40, 50
, Y = 0, 200, 400, 600, 800, 1000, 2500, 4500, 7500, 12500
, LINEAR_EXTRAPOLATE
!
!           adams_view_name='testrig.rer_retract_stop.damping_spline'
SPLINE/6
, X = -50000, -20000, 0, 20000, 50000
, Y = 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='testrig.rel_retract_stop.spline'
SPLINE/7
, X = 0, 2, 4, 6, 8, 10, 20, 30, 40, 50
, Y = 0, 200, 400, 600, 800, 1000, 2500, 4500, 7500, 12500
, LINEAR_EXTRAPOLATE
!
!           adams_view_name='testrig.rel_retract_stop.damping_spline'
SPLINE/8
, X = -50000, -20000, 0, 20000, 50000
, Y = 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.tx_spline'
SPLINE/9
, X = -400, -200, 0, 200, 400
, Y = -4.0E+05, -2.0E+05, 0, 2.0E+05, 4.0E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.ty_spline'
SPLINE/12
, X = -400, -200, 0, 200, 400
, Y = -4.1E+05, -2.1E+05, 0, 2.1E+05, 4.1E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.tz_spline'
SPLINE/15
, X = -410, -200, 0, 200, 410
, Y = -4.4E+05, -2.2E+05, 0, 2.2E+05, 4.4E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.rx_spline'
SPLINE/18
, X = -0.0872664626, -0.034906585, -0.0174532925, 0, 0.0174532925, 0.034906585
, 0.0872664626
, Y = -21000, -13000, -6000, 0, 6000, 13000, 21000
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.ry_spline'
SPLINE/21
, X = -0.1221730476, -0.0872664626, -0.034906585, 0, 0.034906585, 0.0872664626
, 0.1221730476
, Y = -2.6E+05, -1.7E+05, -90000, 0, 90000, 1.7E+05, 2.6E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgr_subframe_front.rz_spline'
SPLINE/24
, X = -0.872664626, -0.436332313, -0.3490658504, -0.2617993878, -0.1745329252
, -0.0872664626, 0, 0.0872664626, 0.1745329252, 0.2617993878, 0.3490658504
, 0.436332313, 0.872664626
, Y = -35500, -14000, -10000, -6000, -3750, -1900, 0, 1900, 3750, 6000, 10000
, 14000, 35500
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.tx_spline'
SPLINE/27
, X = -400, -200, 0, 200, 400
, Y = -4.0E+05, -2.0E+05, 0, 2.0E+05, 4.0E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.ty_spline'
SPLINE/30
, X = -400, -200, 0, 200, 400
, Y = -4.1E+05, -2.1E+05, 0, 2.1E+05, 4.1E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.tz_spline'
SPLINE/33
, X = -410, -200, 0, 200, 410
, Y = -4.4E+05, -2.2E+05, 0, 2.2E+05, 4.4E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.rx_spline'
SPLINE/36
, X = -0.0872664626, -0.034906585, -0.0174532925, 0, 0.0174532925, 0.034906585
, 0.0872664626
, Y = -21000, -13000, -6000, 0, 6000, 13000, 21000
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.ry_spline'
SPLINE/39
, X = -0.1221730476, -0.0872664626, -0.034906585, 0, 0.034906585, 0.0872664626
, 0.1221730476
, Y = -2.6E+05, -1.7E+05, -90000, 0, 90000, 1.7E+05, 2.6E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgl_subframe_rear.rz_spline'
SPLINE/42
, X = -0.872664626, -0.436332313, -0.3490658504, -0.2617993878, -0.1745329252
, -0.0872664626, 0, 0.0872664626, 0.1745329252, 0.2617993878, 0.3490658504
, 0.436332313, 0.872664626
, Y = -35500, -14000, -10000, -6000, -3750, -1900, 0, 1900, 3750, 6000, 10000
, 14000, 35500
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.tx_spline'
SPLINE/45
, X = -400, -200, 0, 200, 400
, Y = -4.0E+05, -2.0E+05, 0, 2.0E+05, 4.0E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.ty_spline'
SPLINE/48
, X = -400, -200, 0, 200, 400
, Y = -4.1E+05, -2.1E+05, 0, 2.1E+05, 4.1E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.tz_spline'
SPLINE/51
, X = -410, -200, 0, 200, 410
, Y = -4.4E+05, -2.2E+05, 0, 2.2E+05, 4.4E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.rx_spline'
SPLINE/54
, X = -0.0872664626, -0.034906585, -0.0174532925, 0, 0.0174532925, 0.034906585
, 0.0872664626
, Y = -21000, -13000, -6000, 0, 6000, 13000, 21000
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.ry_spline'
SPLINE/57
, X = -0.1221730476, -0.0872664626, -0.034906585, 0, 0.034906585, 0.0872664626
, 0.1221730476
, Y = -2.6E+05, -1.7E+05, -90000, 0, 90000, 1.7E+05, 2.6E+05
, LINEAR_EXTRAPOLATE
!
!             adams_view_name='FRT_SUSP.bgr_subframe_rear.rz_spline'
SPLINE/60
, X = -0.872664626, -0.436332313, -0.3490658504, -0.2617993878, -0.1745329252
, -0.0872664626, 0, 0.0872664626, 0.1745329252, 0.2617993878, 0.3490658504
, 0.436332313, 0.872664626
, Y = -35500, -14000, -10000, -6000, -3750, -1900, 0, 1900, 3750, 6000, 10000
, 14000, 35500
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='FRT_SUSP.nsl_ride_spring.spline'
SPLINE/279
, X = -150, -139.6552, -129.3103, -118.9655, -108.6207, -98.2759, -87.931
, -77.5862, -67.2414, -56.8966, -46.5517, -36.2069, -25.8621, -15.5172, -5.1724
, 5.1724, 15.5172, 25.8621, 36.2069, 46.5517, 56.8966, 67.2414, 77.5862, 87.931
, 98.2759, 108.6207, 118.9655, 129.3103, 139.6552, 150
, Y = -5100, -4748.2759, -4396.5517, -4044.8276, -3693.1034, -3341.3793
, -2989.6552, -2637.931, -2286.2069, -1934.4828, -1582.7586, -1231.0345
, -879.3103, -527.5862, -175.8621, 175.8621, 527.5862, 879.3103, 1231.0345
, 1582.7586, 1934.4828, 2286.2069, 2637.931, 2989.6552, 3341.3793, 3693.1034
, 4044.8276, 4396.5517, 4748.2759, 5100
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='FRT_SUSP.nsr_ride_spring.spline'
SPLINE/280
, X = -150, -139.6552, -129.3103, -118.9655, -108.6207, -98.2759, -87.931
, -77.5862, -67.2414, -56.8966, -46.5517, -36.2069, -25.8621, -15.5172, -5.1724
, 5.1724, 15.5172, 25.8621, 36.2069, 46.5517, 56.8966, 67.2414, 77.5862, 87.931
, 98.2759, 108.6207, 118.9655, 129.3103, 139.6552, 150
, Y = -5100, -4748.2759, -4396.5517, -4044.8276, -3693.1034, -3341.3793
, -2989.6552, -2637.931, -2286.2069, -1934.4828, -1582.7586, -1231.0345
, -879.3103, -527.5862, -175.8621, 175.8621, 527.5862, 879.3103, 1231.0345
, 1582.7586, 1934.4828, 2286.2069, 2637.931, 2989.6552, 3341.3793, 3693.1034
, 4044.8276, 4396.5517, 4748.2759, 5100
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='FRT_SUSP.dal_ride_damper.spline'
SPLINE/281
, X = -2725.356, -300, -200, -100, -75, -50, -25, -10, 0, 10, 25, 50, 75, 100
, 200, 300, 2725.356
, Y = 11401.42, 1700, 1300, 500, 350, 200, 100, 50, 0, -50, -100, -200, -350
, -500, -1200, -1600, -11301.42
, LINEAR_EXTRAPOLATE
!
!           adams_view_name='FRT_SUSP.dal_ride_damper.preload_spline'
SPLINE/282
, X = -50000, -20000, 0, 20000, 50000
, Y = 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='FRT_SUSP.dar_ride_damper.spline'
SPLINE/283
, X = -2725.356, -300, -200, -100, -75, -50, -25, -10, 0, 10, 25, 50, 75, 100
, 200, 300, 2725.356
, Y = 11401.42, 1700, 1300, 500, 350, 200, 100, 50, 0, -50, -100, -200, -350
, -500, -1200, -1600, -11301.42
, LINEAR_EXTRAPOLATE
!
!           adams_view_name='FRT_SUSP.dar_ride_damper.preload_spline'
SPLINE/284
, X = -50000, -20000, 0, 20000, 50000
, Y = 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.tx_spline'
SPLINE/285
, X = -400, -200, 0, 200, 400
, Y = -4.0E+05, -2.0E+05, 0, 2.0E+05, 4.0E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.ty_spline'
SPLINE/288
, X = -400, -200, 0, 200, 400
, Y = -4.1E+05, -2.1E+05, 0, 2.1E+05, 4.1E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.tz_spline'
SPLINE/291
, X = -410, -200, 0, 200, 410
, Y = -4.4E+05, -2.2E+05, 0, 2.2E+05, 4.4E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.rx_spline'
SPLINE/294
, X = -0.0872664626, -0.034906585, -0.0174532925, 0, 0.0174532925, 0.034906585
, 0.0872664626
, Y = -21000, -13000, -6000, 0, 6000, 13000, 21000
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.ry_spline'
SPLINE/297
, X = -0.1221730476, -0.0872664626, -0.034906585, 0, 0.034906585, 0.0872664626
, 0.1221730476
, Y = -2.6E+05, -1.7E+05, -90000, 0, 90000, 1.7E+05, 2.6E+05
, LINEAR_EXTRAPOLATE
!
!            adams_view_name='FRT_SUSP.bgl_subframe_front.rz_spline'
SPLINE/300
, X = -0.872664626, -0.436332313, -0.3490658504, -0.2617993878, -0.1745329252
, -0.0872664626, 0, 0.0872664626, 0.1745329252, 0.2617993878, 0.3490658504
, 0.436332313, 0.872664626
, Y = -35500, -14000, -10000, -6000, -3750, -1900, 0, 1900, 3750, 6000, 10000
, 14000, 35500
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='FRT_SUSP.bul_jounce_stop.spline'
SPLINE/339
, X = 0, 2, 4, 6, 8, 10, 20, 30, 40, 50
, Y = 0, 200, 400, 600, 800, 1000, 2500, 4500, 7500, 12500
, LINEAR_EXTRAPOLATE
!
!           adams_view_name='FRT_SUSP.bul_jounce_stop.damping_spline'
SPLINE/340
, X = -50000, -20000, 0, 20000, 50000
, Y = 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!               adams_view_name='FRT_SUSP.bur_jounce_stop.spline'
SPLINE/341
, X = 0, 2, 4, 6, 8, 10, 20, 30, 40, 50
, Y = 0, 200, 400, 600, 800, 1000, 2500, 4500, 7500, 12500
, LINEAR_EXTRAPOLATE
!
!           adams_view_name='FRT_SUSP.bur_jounce_stop.damping_spline'
SPLINE/342
, X = -50000, -20000, 0, 20000, 50000
, Y = 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!Example of a steering assist spline
!            adams_view_name='MDI_FRONT_STEERING.gss_steering_assist'
SPLINE/343
, X = -3, -2.2, -1.8, -1.5, -1, -0.5, 0, 0.5, 1, 1.5, 1.8, 2.2, 3
, Y = -4, -4, -3.6, -3, -2, -1, 0, 1, 2, 3, 3.6, 4, 4
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.tx_spline'
SPLINE/344
, X = -3.5, -3, -2.5, -2, -1.75, -1.5, -1, -0.5, 0, 0.5, 1, 1.5, 1.75, 2, 2.5, 3
, 3.5
, Y = -25000, -20000, -15000, -10000, -8300, -7000, -4500, -2200, 0, 2200, 4500
, 7000, 8300, 10000, 15000, 20000, 25000
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.ty_spline'
SPLINE/347
, X = -3.5, -3, -2.5, -2, -1.75, -1.5, -1, -0.5, 0, 0.5, 1, 1.5, 1.75, 2, 2.5, 3
, 3.5
, Y = -25000, -20000, -15000, -10000, -8300, -7000, -4500, -2200, 0, 2200, 4500
, 7000, 8300, 10000, 15000, 20000, 25000
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.tz_spline'
SPLINE/350
, X = -4, -3.5, -3, -2.5, -2, -1.5, -1, -0.5, 0, 0.5, 1, 1.5, 2, 2.5, 3, 3.5, 4
, Y = -5200, -4100, -3000, -2100, -1600, -1200, -800, -400, 0, 400, 800, 1200
, 1600, 2100, 3000, 4100, 5200
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.rx_spline'
SPLINE/353
, X = -0.5235987756, -0.3490658504, -0.1745329252, 0, 0.1745329252, 0.3490658504
, 0.5235987756
, Y = -7.8E+05, -5.2E+05, -2.6E+05, 0, 2.6E+05, 5.2E+05, 7.8E+05
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.ry_spline'
SPLINE/356
, X = -0.5235987756, -0.3490658504, -0.1745329252, 0, 0.1745329252, 0.3490658504
, 0.5235987756
, Y = -7.8E+05, -5.2E+05, -2.6E+05, 0, 2.6E+05, 5.2E+05, 7.8E+05
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.rz_spline'
SPLINE/359
, X = -0.5235987756, -0.4188790205, -0.3141592654, -0.2094395102, -0.1047197551
, 0, 0.1047197551, 0.2094395102, 0.3141592654, 0.4188790205, 0.5235987756
, Y = -1.5E+06, -1.2E+06, -9.0E+05, -6.0E+05, -3.0E+05, 0, 3.0E+05, 6.0E+05
, 9.0E+05, 1.2E+06, 1.5E+06
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.tx_spline'
SPLINE/362
, X = -3.5, -3, -2.5, -2, -1.75, -1.5, -1, -0.5, 0, 0.5, 1, 1.5, 1.75, 2, 2.5, 3
, 3.5
, Y = -25000, -20000, -15000, -10000, -8300, -7000, -4500, -2200, 0, 2200, 4500
, 7000, 8300, 10000, 15000, 20000, 25000
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.ty_spline'
SPLINE/365
, X = -3.5, -3, -2.5, -2, -1.75, -1.5, -1, -0.5, 0, 0.5, 1, 1.5, 1.75, 2, 2.5, 3
, 3.5
, Y = -25000, -20000, -15000, -10000, -8300, -7000, -4500, -2200, 0, 2200, 4500
, 7000, 8300, 10000, 15000, 20000, 25000
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.tz_spline'
SPLINE/368
, X = -4, -3.5, -3, -2.5, -2, -1.5, -1, -0.5, 0, 0.5, 1, 1.5, 2, 2.5, 3, 3.5, 4
, Y = -5200, -4100, -3000, -2100, -1600, -1200, -800, -400, 0, 400, 800, 1200
, 1600, 2100, 3000, 4100, 5200
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.rx_spline'
SPLINE/371
, X = -0.5235987756, -0.3490658504, -0.1745329252, 0, 0.1745329252, 0.3490658504
, 0.5235987756
, Y = -7.8E+05, -5.2E+05, -2.6E+05, 0, 2.6E+05, 5.2E+05, 7.8E+05
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.ry_spline'
SPLINE/374
, X = -0.5235987756, -0.3490658504, -0.1745329252, 0, 0.1745329252, 0.3490658504
, 0.5235987756
, Y = -7.8E+05, -5.2E+05, -2.6E+05, 0, 2.6E+05, 5.2E+05, 7.8E+05
, LINEAR_EXTRAPOLATE
!
!    adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.rz_spline'
SPLINE/377
, X = -0.5235987756, -0.4188790205, -0.3141592654, -0.2094395102, -0.1047197551
, 0, 0.1047197551, 0.2094395102, 0.3141592654, 0.4188790205, 0.5235987756
, Y = -1.5E+06, -1.2E+06, -9.0E+05, -6.0E+05, -3.0E+05, 0, 3.0E+05, 6.0E+05
, 9.0E+05, 1.2E+06, 1.5E+06
, LINEAR_EXTRAPOLATE
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.tx_spline'
SPLINE/380
, X = -20, -18, -16, -14, -12, -10, -8, -6, -4, -2, 0, 2, 4, 6, 8, 10, 12, 14
, 16, 18, 20
, Y = 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.ty_spline'
SPLINE/383
, X = -20, -18, -16, -14, -12, -10, -8, -6, -4, -2, 0, 2, 4, 6, 8, 10, 12, 14
, 16, 18, 20
, Y = 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.tz_spline'
SPLINE/386
, X = -20, -18, -16, -14, -12, -10, -8, -6, -4, -2, 0, 2, 4, 6, 8, 10, 12, 14
, 16, 18, 20
, Y = 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.rx_spline'
SPLINE/389
, X = -0.3490658504, -0.3141592654, -0.2792526803, -0.2443460953, -0.2094395102
, -0.1745329252, -0.1396263402, -0.1047197551, -0.0698131701, -0.034906585, 0
, 0.034906585, 0.0698131701, 0.1047197551, 0.1396263402, 0.1745329252
, 0.2094395102, 0.2443460953, 0.2792526803, 0.3141592654, 0.3490658504
, Y = 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.ry_spline'
SPLINE/392
, X = -0.3490658504, -0.3141592654, -0.2792526803, -0.2443460953, -0.2094395102
, -0.1745329252, -0.1396263402, -0.1047197551, -0.0698131701, -0.034906585, 0
, 0.034906585, 0.0698131701, 0.1047197551, 0.1396263402, 0.1745329252
, 0.2094395102, 0.2443460953, 0.2792526803, 0.3141592654, 0.3490658504
, Y = 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0, 0
, LINEAR_EXTRAPOLATE
!
!         adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.rz_spline'
SPLINE/395
, X = -0.3490658504, -0.3141592654, -0.2792526803, -0.2443460953, -0.2094395102
, -0.1745329252, -0.1396263402, -0.1047197551, -0.0698131701, -0.034906585, 0
, 0.034906585, 0.0698131701, 0.1047197551, 0.1396263402, 0.1745329252
, 0.2094395102, 0.2443460953, 0.2792526803, 0.3141592654, 0.3490658504
, Y = -4.0E+05, -3.6E+05, -3.2E+05, -2.8E+05, -2.4E+05, -2.0E+05, -1.6E+05
, -1.2E+05, -80000, -40000, 0, 40000, 80000, 1.2E+05, 1.6E+05, 2.0E+05, 2.4E+05
, 2.8E+05, 3.2E+05, 3.6E+05, 4.0E+05
, LINEAR_EXTRAPOLATE
!
!                   adams_view_name='grarev_lca_case_MATRIX_1'
!                   adams_view_units='length'
MATRIX/1
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 4.9790902759, -0.2383542847, 0.3896758384
, 1.8402028913, -0.6182124758, 40.2645187063
, -3.1388873847, -0.3798581912, 39.8748428679
, 0, 0, 0
!
!                   adams_view_name='grarev_lca_case_MATRIX_2'
!                   adams_view_units='length'
MATRIX/2
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 4.9790902759, 0.2383542847, 0.3896758384
, 1.8402028913, 0.6182124758, 40.2645187063
, -3.1388873847, 0.3798581912, 39.8748428679
, 0, 0, 0
!
!                      adams_view_name='i_graphic_MATRIX_3'
!                      adams_view_units='length'
MATRIX/3
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -29.4, -14
, 0, -29.4, 10
, 0, 0, 20
, 0, 0, 0
!
!                      adams_view_name='i_graphic_MATRIX_4'
!                      adams_view_units='length'
MATRIX/4
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -29.4, -14
, 0, -29.4, 10
, 0, 0, 20
, 0, 0, 0
!
!                      adams_view_name='i_graphic_MATRIX_5'
!                      adams_view_units='length'
MATRIX/5
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -29.4, -14
, 0, -29.4, 10
, 0, 0, 20
, 0, 0, 0
!
!                      adams_view_name='i_graphic_MATRIX_6'
!                      adams_view_units='length'
MATRIX/6
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0.712821546, -23.8822253391, -22.1244479772
, -0.5091582472, -31.0409022172, 0.7504314922
, -1.0183164943, -5.9655640651, 19.0623995578
, 0, 0, 0
!
!                      adams_view_name='i_graphic_MATRIX_7'
!                      adams_view_units='length'
MATRIX/7
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0.712821546, -32.2340150302, -4.5629114037
, -0.5091582472, -25.0753381521, 18.3119680657
, -1.0183164943, 5.9655640651, 19.0623995578
, 0, 0, 0
!
!                      adams_view_name='i_graphic_MATRIX_8'
!                      adams_view_units='length'
MATRIX/8
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 17.4314245794, 4.4255349924, 21.7441964018
, -35.9668000172, 4.4255349924, 29.783450716
, -49.4428005524, 0, 7.4437539946
, 0, 0, 0
!
!                      adams_view_name='i_graphic_MATRIX_9'
!                      adams_view_units='length'
MATRIX/9
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 10.2565437299, 4.4255349924, -25.9126986388
, -43.1416808667, 4.4255349924, -17.8734443246
, -49.4428005524, 0, 7.4437539946
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_10'
!                     adams_view_units='length'
MATRIX/10
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, -10.2565437299, 4.4255349924, 25.9126986388
, 43.1416808667, 4.4255349924, 17.8734443246
, 49.4428005524, 0, -7.4437539946
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_11'
!                     adams_view_units='length'
MATRIX/11
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, -17.4314245794, 4.4255349924, -21.7441964018
, 35.9668000172, 4.4255349924, -29.783450716
, 49.4428005524, 0, -7.4437539946
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_12'
!                     adams_view_units='length'
MATRIX/12
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, -13.931961517, -27.6463895186, -10.0964149514
, 49.757005418, -29.5285868488, -4.0820301986
, 59.7084065016, -1.7645599971, 5.6384857058
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_13'
!                     adams_view_units='length'
MATRIX/13
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, -13.931961517, -28.4698508506, 7.4651216221
, 49.757005418, -26.5876535204, 13.4795063749
, 59.7084065016, 1.7645599971, 5.6384857058
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_14'
!                     adams_view_units='length'
MATRIX/14
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 12.0342558266, -0.2326631421, 25.5220013824
, -41.7992095222, -0.2326631421, 21.2843123258
, -49.8458012489, 0, -3.9237861635
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_15'
!                     adams_view_units='length'
MATRIX/15
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 15.8793928728, -0.2326631421, -23.3246811308
, -37.954072476, -0.2326631421, -27.5623701874
, -49.8458012489, 0, -3.9237861635
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_16'
!                     adams_view_units='length'
MATRIX/16
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 12.0342558266, -0.2326631421, 25.5220013824
, -41.7992095222, -0.2326631421, 21.2843123258
, -49.8458012489, 0, -3.9237861635
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_17'
!                     adams_view_units='length'
MATRIX/17
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 15.8793928728, -0.2326631421, -23.3246811308
, -37.954072476, -0.2326631421, -27.5623701874
, -49.8458012489, 0, -3.9237861635
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_18'
!                     adams_view_units='length'
MATRIX/18
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -29.4, -14
, 0, -29.4, 10
, 0, 0, 20
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_19'
!                     adams_view_units='length'
MATRIX/19
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -29.4, -14
, 0, -29.4, 10
, 0, 0, 20
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_20'
!                     adams_view_units='length'
MATRIX/20
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -29.4, -14
, 0, -29.4, 10
, 0, 0, 20
, 0, 0, 0
!
!                 adams_view_name='steering_wheel_rim_MATRIX_21'
!                 adams_view_units='length'
MATRIX/21
, FULL = RORDER
, ROWS = 26
, COLUMNS = 3
, VALUES = 0, 0, 0
, -0.1208321718, -3.4816584203, 0.4229126011
, -0.4757363572, -6.7445514374, 1.6650772502
, -1.0424126212, -9.583659483, 3.6484441742
, -1.78525461, -11.820590957, 6.2483911348
, -2.6575868293, -13.3147912281, 9.3015539025
, -3.6045974378, -13.972374198, 12.616091032
, -4.5667822759, -13.7520215102, 15.9837379654
, -5.4836837316, -12.6675787345, 19.1928930605
, -6.2976895144, -10.7871853989, 22.0419133002
, -6.9576526472, -8.2289935321, 24.351784265
, -7.4221052191, -5.1537437376, 25.9773682669
, -7.6618639671, -1.7546652699, 26.8165238847
, -7.6618639671, 1.7546652699, 26.8165238847
, -7.4221052191, 5.1537437376, 25.9773682669
, -6.9576526472, 8.2289935321, 24.351784265
, -6.2976895144, 10.7871853989, 22.0419133002
, -5.4836837316, 12.6675787345, 19.1928930605
, -4.5667822759, 13.7520215102, 15.9837379654
, -3.6045974378, 13.972374198, 12.616091032
, -2.6575868293, 13.3147912281, 9.3015539025
, -1.78525461, 11.820590957, 6.2483911348
, -1.0424126212, 9.583659483, 3.6484441742
, -0.4757363572, 6.7445514374, 1.6650772502
, -0.1208321718, 3.4816584203, 0.4229126011
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_22'
!                     adams_view_units='length'
MATRIX/22
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, 19.6, 14
, 0, 19.6, -15
, 0, 0, -25
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_23'
!                     adams_view_units='length'
MATRIX/23
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -19.6, -14
, 0, -19.6, 15
, 0, 0, 25
, 0, 0, 0
!
!                     adams_view_name='i_graphic_MATRIX_24'
!                     adams_view_units='length'
MATRIX/24
, FULL = RORDER
, ROWS = 5
, COLUMNS = 3
, VALUES = 0, 0, 0
, 0, -19.6, -14
, 0, -19.6, 15
, 0, 0, 25
, 0, 0, 0
!
!                 adams_view_name='testrig.left_vertical_input'
VARIABLE/2
, FUNCTION = AKISPL(1,time,2)
!
!                 adams_view_name='testrig.right_vertical_input'
VARIABLE/3
, FUNCTION = AKISPL(2,time,2)
!
!                 adams_view_name='testrig.tire_fx_braking_left'
VARIABLE/4
, FUNCTION = 0.0
!
!                adams_view_name='testrig.tire_fx_traction_left'
VARIABLE/5
, FUNCTION = 0.0
!
!                adams_view_name='testrig.tire_fy_cornering_left'
VARIABLE/6
, FUNCTION = 0.0
!
!               adams_view_name='testrig.tire_tx_overturning_left'
VARIABLE/7
, FUNCTION = 0.0
!
!                 adams_view_name='testrig.tire_ty_rolling_left'
VARIABLE/8
, FUNCTION = 0.0
!
!              adams_view_name='testrig.tire_ty_damage_force_left'
VARIABLE/9
, FUNCTION = 0.0
!
!              adams_view_name='testrig.tire_ty_damage_radius_left'
VARIABLE/10
, FUNCTION = 0.0
!
!                adams_view_name='testrig.tire_tz_aligning_left'
VARIABLE/11
, FUNCTION = 0.0
!
!                adams_view_name='testrig.tire_fx_braking_right'
VARIABLE/12
, FUNCTION = 0.0
!
!                adams_view_name='testrig.tire_fx_traction_right'
VARIABLE/13
, FUNCTION = 0.0
!
!               adams_view_name='testrig.tire_fy_cornering_right'
VARIABLE/14
, FUNCTION = 0.0
!
!              adams_view_name='testrig.tire_tx_overturning_right'
VARIABLE/15
, FUNCTION = 0.0
!
!                adams_view_name='testrig.tire_ty_rolling_right'
VARIABLE/16
, FUNCTION = 0.0
!
!              adams_view_name='testrig.tire_ty_damage_force_right'
VARIABLE/17
, FUNCTION = 0.0
!
!             adams_view_name='testrig.tire_ty_damage_radius_right'
VARIABLE/18
, FUNCTION = 0.0
!
!                adams_view_name='testrig.tire_tz_aligning_right'
VARIABLE/19
, FUNCTION = 0.0
!
!            adams_view_name='testrig.jml_bearing_lock.var_register'
VARIABLE/20
, FUNCTION = USER(913, 13, 0)\
, ROUTINE = abgFDM::var913
!
!            adams_view_name='testrig.jmr_bearing_lock.var_register'
VARIABLE/21
, FUNCTION = USER(913, 15, 0)\
, ROUTINE = abgFDM::var913
!
!             adams_view_name='testrig.jfl_jack_force.var_register'
VARIABLE/22
, FUNCTION = USER(913, 17, 0)\
, ROUTINE = abgFDM::var913
!
!             adams_view_name='testrig.jfr_jack_force.var_register'
VARIABLE/23
, FUNCTION = USER(913, 19, 0)\
, ROUTINE = abgFDM::var913
!
!              adams_view_name='testrig.ffs_roll_angle.raw_channel'
VARIABLE/24
, FUNCTION = -1.0*AX(111, 46)*RTOD
!
!            adams_view_name='testrig.ffs_roll_angle.offset_channel'
VARIABLE/25
, FUNCTION = varval(24) + (ARYVAL(21,1)*ARYVAL(21,2))
!
!         adams_view_name='testrig.ffs_table_center_height.raw_channel'
VARIABLE/26
, FUNCTION = 0.5*(DZ(99, 46, 46)+DZ(111, 46, 46))
!
!        adams_view_name='testrig.ffs_table_center_height.offset_channel'
VARIABLE/27
, FUNCTION = varval(26) + (ARYVAL(22,1)*ARYVAL(22,2))
!
!         adams_view_name='testrig.ffl_wheel_center_height.raw_channel'
VARIABLE/28
, FUNCTION = DZ(74, 48, 46)
!
!        adams_view_name='testrig.ffl_wheel_center_height.offset_channel'
VARIABLE/29
, FUNCTION = varval(28) + (ARYVAL(23,1)*ARYVAL(23,2))
!
!         adams_view_name='testrig.ffr_wheel_center_height.raw_channel'
VARIABLE/30
, FUNCTION = DZ(81, 49, 46)
!
!        adams_view_name='testrig.ffr_wheel_center_height.offset_channel'
VARIABLE/31
, FUNCTION = varval(30) + (ARYVAL(24,1)*ARYVAL(24,2))
!
!         adams_view_name='testrig.ffl_contact_patch_height.raw_channel'
VARIABLE/32
, FUNCTION = USER(917,1,98,46,75,329.815)\
, ROUTINE = acarSDM::var917
!
!       adams_view_name='testrig.ffl_contact_patch_height.offset_channel'
VARIABLE/33
, FUNCTION = varval(32) + (ARYVAL(25,1)*ARYVAL(25,2))
!
!         adams_view_name='testrig.ffr_contact_patch_height.raw_channel'
VARIABLE/34
, FUNCTION = USER(917,1,110,46,82,329.815)\
, ROUTINE = acarSDM::var917
!
!       adams_view_name='testrig.ffr_contact_patch_height.offset_channel'
VARIABLE/35
, FUNCTION = varval(34) + (ARYVAL(26,1)*ARYVAL(26,2))
!
!         adams_view_name='testrig.ffs_total_vertical_force.raw_channel'
VARIABLE/36
, FUNCTION = USER(917,3,1,2,98,110)\
, ROUTINE = acarSDM::var917
!
!       adams_view_name='testrig.ffs_total_vertical_force.offset_channel'
VARIABLE/37
, FUNCTION = varval(36) + (ARYVAL(27,1)*ARYVAL(27,2))
!
!         adams_view_name='testrig.ffl_wheel_vertical_force.raw_channel'
VARIABLE/38
, FUNCTION = USER(917,2,1,98)\
, ROUTINE = acarSDM::var917
!
!       adams_view_name='testrig.ffl_wheel_vertical_force.offset_channel'
VARIABLE/39
, FUNCTION = varval(38) + (ARYVAL(28,1)*ARYVAL(28,2))
!
!         adams_view_name='testrig.ffr_wheel_vertical_force.raw_channel'
VARIABLE/40
, FUNCTION = USER(917,2,2,110)\
, ROUTINE = acarSDM::var917
!
!       adams_view_name='testrig.ffr_wheel_vertical_force.offset_channel'
VARIABLE/41
, FUNCTION = varval(40) + (ARYVAL(29,1)*ARYVAL(29,2))
!
!           adams_view_name='testrig.jfs_steering_input.var_register'
VARIABLE/46
, FUNCTION = USER(913, 38, 0)\
, ROUTINE = abgFDM::var913
!
!     adams_view_name='testrig.ffs_steering_input_displacement.raw_channel'
VARIABLE/47
, FUNCTION = DZ(140, 60, 60)
!
!    adams_view_name='testrig.ffs_steering_input_displacement.offset_channel'
VARIABLE/48
, FUNCTION = varval(47) + (ARYVAL(40,1)*ARYVAL(40,2))
!
!      adams_view_name='testrig.ffs_steering_part_displacement.raw_channel'
VARIABLE/49
, FUNCTION = DZ(143, 61, 61)
!
!    adams_view_name='testrig.ffs_steering_part_displacement.offset_channel'
VARIABLE/50
, FUNCTION = varval(49) + (ARYVAL(41,1)*ARYVAL(41,2))
!
!          adams_view_name='testrig.outside_tire_ty_damage_force_left'
VARIABLE/56
, FUNCTION = 0.0
!
!               adams_view_name='testrig.vehicle_parameters_ARRAY'
ARRAY/2
, IC
, SIZE = 8
, NUMBERS = 17455.837, 300, 2905, 1, 0.55, 1, 329.815, 200
!
!              adams_view_name='testrig.leaf_adjustment_multiplier'
ARRAY/3
, IC
, SIZE = 1
, NUMBERS = 0
!
!               adams_view_name='testrig.testrig_parameters_ARRAY'
ARRAY/4
, IC
, SIZE = 10
, NUMBERS = 142, 111, 46, 74, 81, 1, 1, 0, 2, 99
!
!             adams_view_name='testrig.characteristics_input_ARRAY'
ARRAY/5
, IC
, SIZE = 3
, NUMBERS = 59, 2, 4
!
!                adams_view_name='testrig.loadcase_function_left'
ARRAY/7
, IC
, SIZE = 8
, NUMBERS = 4, 5, 6, 7, 8, 9, 10, 11
!
!               adams_view_name='testrig.loadcase_function_right'
ARRAY/8
, IC
, SIZE = 8
, NUMBERS = 12, 13, 14, 15, 16, 17, 18, 19
!
!                   adams_view_name='testrig.left_user_array'
ARRAY/9
, IC
, SIZE = 4
, NUMBERS = 2, 0, 7, 1
!
!                   adams_view_name='testrig.right_user_array'
ARRAY/10
, IC
, SIZE = 4
, NUMBERS = 2, 1, 8, 1
!
!Input array for tire gfosub
!                adams_view_name='testrig.til_wheel.input_array'
ARRAY/11
, IC
, SIZE = 15
, NUMBERS = 5, 6, 0, 3, 5, 8, 6, 7, 329.815, 0, 0, 0, 9, 0, 200
!
!Input array for tire gfosub
!                adams_view_name='testrig.tir_wheel.input_array'
ARRAY/12
, IC
, SIZE = 15
, NUMBERS = 7, 8, 1, 3, 9, 12, 10, 11, 329.815, 0, 0, 0, 10, 0, 200
!
!a1 : actuator type (0=joint_force,1=joint_motion,2=point_point,3=point_torque,4=variable)
!a2 : symmetry type (0=single, 1=left, 2=right)
!a3 : freedom type (0=translational, 1=rotational)
!a4 : limits array id
!a5 : application string id
!a6 : identifier string id
!a7 : minor_role string id
!a8 : unit string id
!a9 : request id
!a10: motion id
!            adams_view_name='testrig.jml_bearing_lock.arr_elements'
ARRAY/13
, IC
, SIZE = 10
, NUMBERS = 1, 1, 1, 14, 13, 14, 3, 15, 71, 3
!
!a1  : dis_min
!a2  : dis_max
!a3  : vel_min
!a4  : vel_max
!a5  : acc_min
!a6  : acc_max
!a7  : frc_min
!a8  : frc_max
!             adams_view_name='testrig.jml_bearing_lock.arr_limits'
ARRAY/14
, IC
, SIZE = 8
, NUMBERS = -90, 90, -100, 100, -100, 100, -100, 100
!
!a1 : actuator type (0=joint_force,1=joint_motion,2=point_point,3=point_torque,4=variable)
!a2 : symmetry type (0=single, 1=left, 2=right)
!a3 : freedom type (0=translational, 1=rotational)
!a4 : limits array id
!a5 : application string id
!a6 : identifier string id
!a7 : minor_role string id
!a8 : unit string id
!a9 : request id
!a10: motion id
!            adams_view_name='testrig.jmr_bearing_lock.arr_elements'
ARRAY/15
, IC
, SIZE = 10
, NUMBERS = 1, 2, 1, 16, 16, 17, 3, 18, 72, 4
!
!a1  : dis_min
!a2  : dis_max
!a3  : vel_min
!a4  : vel_max
!a5  : acc_min
!a6  : acc_max
!a7  : frc_min
!a8  : frc_max
!             adams_view_name='testrig.jmr_bearing_lock.arr_limits'
ARRAY/16
, IC
, SIZE = 8
, NUMBERS = -90, 90, -100, 100, -100, 100, -100, 100
!
!a1 : actuator type (0=joint_force,1=joint_motion,2=point_point,3=point_torque,4=variable)
!a2 : symmetry type (0=single, 1=left, 2=right)
!a3 : freedom type (0=translational, 1=rotational)
!a4 : limits array id
!a5 : application string id
!a6 : identifier string id
!a7 : minor_role string id
!a8 : unit string id
!a9 : request id
!a10: sforce-i id
!a11: sforce-j id
!             adams_view_name='testrig.jfl_jack_force.arr_elements'
ARRAY/17
, IC
, SIZE = 11
, NUMBERS = 0, 1, 0, 18, 19, 20, 3, 21, 73, 1, 2
!
!a1  : dis_min
!a2  : dis_max
!a3  : vel_min
!a4  : vel_max
!a5  : acc_min
!a6  : acc_max
!a7  : frc_min
!a8  : frc_max
!              adams_view_name='testrig.jfl_jack_force.arr_limits'
ARRAY/18
, IC
, SIZE = 8
, NUMBERS = -250, 250, -10000, 10000, -10000, 10000, -20000, 40000
!
!a1 : actuator type (0=joint_force,1=joint_motion,2=point_point,3=point_torque,4=variable)
!a2 : symmetry type (0=single, 1=left, 2=right)
!a3 : freedom type (0=translational, 1=rotational)
!a4 : limits array id
!a5 : application string id
!a6 : identifier string id
!a7 : minor_role string id
!a8 : unit string id
!a9 : request id
!a10: sforce-i id
!a11: sforce-j id
!             adams_view_name='testrig.jfr_jack_force.arr_elements'
ARRAY/19
, IC
, SIZE = 11
, NUMBERS = 0, 2, 0, 20, 22, 23, 3, 24, 74, 3, 4
!
!a1  : dis_min
!a2  : dis_max
!a3  : vel_min
!a4  : vel_max
!a5  : acc_min
!a6  : acc_max
!a7  : frc_min
!a8  : frc_max
!              adams_view_name='testrig.jfr_jack_force.arr_limits'
ARRAY/20
, IC
, SIZE = 8
, NUMBERS = -250, 250, -10000, 10000, -10000, 10000, -20000, 40000
!
!             adams_view_name='testrig.ffs_roll_angle.offset_array'
ARRAY/21
, IC
, SIZE = 2
, NUMBERS = 0, 0
!
!         adams_view_name='testrig.ffs_table_center_height.offset_array'
ARRAY/22
, IC
, SIZE = 2
, NUMBERS = 0, 0
!
!         adams_view_name='testrig.ffl_wheel_center_height.offset_array'
ARRAY/23
, IC
, SIZE = 2
, NUMBERS = 0, 0
!
!         adams_view_name='testrig.ffr_wheel_center_height.offset_array'
ARRAY/24
, IC
, SIZE = 2
, NUMBERS = 0, 0
!
!        adams_view_name='testrig.ffl_contact_patch_height.offset_array'
ARRAY/25
, IC
, SIZE = 2
, NUMBERS = 0, 1
!
!        adams_view_name='testrig.ffr_contact_patch_height.offset_array'
ARRAY/26
, IC
, SIZE = 2
, NUMBERS = 0, 1
!
!        adams_view_name='testrig.ffs_total_vertical_force.offset_array'
ARRAY/27
, IC
, SIZE = 2
, NUMBERS = 0, 0
!
!        adams_view_name='testrig.ffl_wheel_vertical_force.offset_array'
ARRAY/28
, IC
, SIZE = 2
, NUMBERS = 0, 0
!
!        adams_view_name='testrig.ffr_wheel_vertical_force.offset_array'
ARRAY/29
, IC
, SIZE = 2
, NUMBERS = 0, 0
!
!a1 : actuator type (0=joint_force,1=joint_motion,2=point_point,3=point_torque,4=variable)
!a2 : symmetry type (0=single, 1=left, 2=right)
!a3 : freedom type (0=translational, 1=rotational)
!a4 : limits array id
!a5 : application string id
!a6 : identifier string id
!a7 : minor_role string id
!a8 : unit string id
!a9 : request id
!a10: sforce-i id
!a11: sforce-j id
!           adams_view_name='testrig.jfs_steering_input.arr_elements'
ARRAY/38
, IC
, SIZE = 11
, NUMBERS = 0, 0, 0, 39, 37, 38, 3, 39, 81, 11, 12
!
!a1  : dis_min
!a2  : dis_max
!a3  : vel_min
!a4  : vel_max
!a5  : acc_min
!a6  : acc_max
!a7  : frc_min
!a8  : frc_max
!            adams_view_name='testrig.jfs_steering_input.arr_limits'
ARRAY/39
, IC
, SIZE = 8
, NUMBERS = 0, 0, 0, 0, 0, 0, 0, 0
!
!     adams_view_name='testrig.ffs_steering_input_displacement.offset_array'
ARRAY/40
, IC
, SIZE = 2
, NUMBERS = 0, 1
!
!     adams_view_name='testrig.ffs_steering_part_displacement.offset_array'
ARRAY/41
, IC
, SIZE = 2
, NUMBERS = 0, 1
!
!STEER AXIS CALCULATION METHOD=: geometric
!             adams_view_name='FRT_SUSP.suspension_parameters_ARRAY'
ARRAY/59
, IC
, SIZE = 6
, NUMBERS = 1, 233, 401, 240, 413, 1
!
!          adams_view_name='FRT_SUSP.bgr_subframe_front.tx_data_array'
ARRAY/60
, IC
, SIZE = 11
, NUMBERS = 2, 9, 1, 1, 0.1, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgr_subframe_front.ty_data_array'
ARRAY/61
, IC
, SIZE = 11
, NUMBERS = 2, 12, 1, 1, 0.2, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgr_subframe_front.tz_data_array'
ARRAY/62
, IC
, SIZE = 11
, NUMBERS = 2, 15, 1, 1, 0.15, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgr_subframe_front.rx_data_array'
ARRAY/63
, IC
, SIZE = 11
, NUMBERS = 2, 18, 1, 1, 85.94366927, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgr_subframe_front.ry_data_array'
ARRAY/64
, IC
, SIZE = 11
, NUMBERS = 2, 21, 1, 1, 91.67324722, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgr_subframe_front.rz_data_array'
ARRAY/65
, IC
, SIZE = 11
, NUMBERS = 2, 24, 1, 1, 88.80845825, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.tx_data_array'
ARRAY/84
, IC
, SIZE = 11
, NUMBERS = 2, 27, 1, 1, 0.1, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.ty_data_array'
ARRAY/85
, IC
, SIZE = 11
, NUMBERS = 2, 30, 1, 1, 0.2, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.tz_data_array'
ARRAY/86
, IC
, SIZE = 11
, NUMBERS = 2, 33, 1, 1, 0.15, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.rx_data_array'
ARRAY/87
, IC
, SIZE = 11
, NUMBERS = 2, 36, 1, 1, 85.94366927, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.ry_data_array'
ARRAY/88
, IC
, SIZE = 11
, NUMBERS = 2, 39, 1, 1, 91.67324722, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.rz_data_array'
ARRAY/89
, IC
, SIZE = 11
, NUMBERS = 2, 42, 1, 1, 88.80845825, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.tx_data_array'
ARRAY/108
, IC
, SIZE = 11
, NUMBERS = 2, 45, 1, 1, 0.1, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.ty_data_array'
ARRAY/109
, IC
, SIZE = 11
, NUMBERS = 2, 48, 1, 1, 0.2, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.tz_data_array'
ARRAY/110
, IC
, SIZE = 11
, NUMBERS = 2, 51, 1, 1, 0.15, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.rx_data_array'
ARRAY/111
, IC
, SIZE = 11
, NUMBERS = 2, 54, 1, 1, 85.94366927, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.ry_data_array'
ARRAY/112
, IC
, SIZE = 11
, NUMBERS = 2, 57, 1, 1, 91.67324722, 1, 0, 0, 1, 0, 1
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.rz_data_array'
ARRAY/113
, IC
, SIZE = 11
, NUMBERS = 2, 60, 1, 1, 88.80845825, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgl_subframe_front.tx_data_array'
ARRAY/420
, IC
, SIZE = 11
, NUMBERS = 2, 285, 1, 1, 0.1, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgl_subframe_front.ty_data_array'
ARRAY/421
, IC
, SIZE = 11
, NUMBERS = 2, 288, 1, 1, 0.2, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgl_subframe_front.tz_data_array'
ARRAY/422
, IC
, SIZE = 11
, NUMBERS = 2, 291, 1, 1, 0.15, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgl_subframe_front.rx_data_array'
ARRAY/423
, IC
, SIZE = 11
, NUMBERS = 2, 294, 1, 1, 85.94366927, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgl_subframe_front.ry_data_array'
ARRAY/424
, IC
, SIZE = 11
, NUMBERS = 2, 297, 1, 1, 91.67324722, 1, 0, 0, 1, 0, 1
!
!          adams_view_name='FRT_SUSP.bgl_subframe_front.rz_data_array'
ARRAY/425
, IC
, SIZE = 11
, NUMBERS = 2, 300, 1, 1, 88.80845825, 1, 0, 0, 1, 0, 1
!
!Array for adjustable forces
!a1 : lock
!a2 : motion id
!a3 : sforce id
!a4 : i_marker id
!a5 : j_marker id
!a6 : alignment flag
!a7+: pattern
!              adams_view_name='FRT_SUSP.afl_camber_adjuster.array'
ARRAY/492
, IC
, SIZE = 9
, NUMBERS = 1, 9, 17, 270, 230, 0, 0, 1, 1
!
!Array for adjustable forces
!a1 : lock
!a2 : motion id
!a3 : sforce id
!a4 : i_marker id
!a5 : j_marker id
!a6 : alignment flag
!a7+: pattern
!              adams_view_name='FRT_SUSP.afr_camber_adjuster.array'
ARRAY/493
, IC
, SIZE = 9
, NUMBERS = 1, 10, 18, 289, 237, 0, 0, 1, 1
!
!Array for adjustable forces
!a1 : lock
!a2 : motion id
!a3 : sforce id
!a4 : i_marker id
!a5 : j_marker id
!a6 : alignment flag
!a7+: pattern
!               adams_view_name='FRT_SUSP.afl_toe_adjuster.array'
ARRAY/494
, IC
, SIZE = 9
, NUMBERS = 1, 11, 19, 245, 259, 0, 1, 0, 1
!
!Array for adjustable forces
!a1 : lock
!a2 : motion id
!a3 : sforce id
!a4 : i_marker id
!a5 : j_marker id
!a6 : alignment flag
!a7+: pattern
!               adams_view_name='FRT_SUSP.afr_toe_adjuster.array'
ARRAY/495
, IC
, SIZE = 9
, NUMBERS = 1, 12, 20, 252, 267, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.tx_data_array'
ARRAY/496
, IC
, SIZE = 11
, NUMBERS = 2, 344, 1, 1, 10, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.ty_data_array'
ARRAY/497
, IC
, SIZE = 11
, NUMBERS = 2, 347, 1, 1, 10, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.tz_data_array'
ARRAY/498
, IC
, SIZE = 11
, NUMBERS = 2, 350, 1, 1, 10, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.rx_data_array'
ARRAY/499
, IC
, SIZE = 11
, NUMBERS = 2, 353, 1, 1, 14896.90267, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.ry_data_array'
ARRAY/500
, IC
, SIZE = 11
, NUMBERS = 2, 356, 1, 1, 14896.90267, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.rz_data_array'
ARRAY/501
, IC
, SIZE = 11
, NUMBERS = 2, 359, 1, 1, 28647.88976, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.tx_data_array'
ARRAY/520
, IC
, SIZE = 11
, NUMBERS = 2, 362, 1, 1, 10, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.ty_data_array'
ARRAY/521
, IC
, SIZE = 11
, NUMBERS = 2, 365, 1, 1, 10, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.tz_data_array'
ARRAY/522
, IC
, SIZE = 11
, NUMBERS = 2, 368, 1, 1, 10, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.rx_data_array'
ARRAY/523
, IC
, SIZE = 11
, NUMBERS = 2, 371, 1, 1, 14896.90267, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.ry_data_array'
ARRAY/524
, IC
, SIZE = 11
, NUMBERS = 2, 374, 1, 1, 14896.90267, 1, 0, 0, 1, 0, 1
!
!  adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.rz_data_array'
ARRAY/525
, IC
, SIZE = 11
, NUMBERS = 2, 377, 1, 1, 28647.88976, 1, 0, 0, 1, 0, 1
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.tx_data_array'
ARRAY/544
, IC
, SIZE = 11
, NUMBERS = 2, 380, 1, 1, 0.1, 1, 0, 0, 1, 0, 1
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.ty_data_array'
ARRAY/545
, IC
, SIZE = 11
, NUMBERS = 2, 383, 1, 1, 0.2, 1, 0, 0, 1, 0, 1
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.tz_data_array'
ARRAY/546
, IC
, SIZE = 11
, NUMBERS = 2, 386, 1, 1, 0.15, 1, 0, 0, 1, 0, 1
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.rx_data_array'
ARRAY/547
, IC
, SIZE = 11
, NUMBERS = 2, 389, 1, 1, 0, 1, 0, 0, 1, 0, 1
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.ry_data_array'
ARRAY/548
, IC
, SIZE = 11
, NUMBERS = 2, 392, 1, 1, 0, 1, 0, 0, 1, 0, 1
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.rz_data_array'
ARRAY/549
, IC
, SIZE = 11
, NUMBERS = 2, 395, 1, 1, 8594.366927, 1, 0, 0, 1, 0, 1
!
!                   adams_view_name='grarev_lca_case_CURVE_1'
CURVE/1
, CLOSED
, MATRIX = 1
, CURVE_POINTS
, ORDER = 2
!
!                   adams_view_name='grarev_lca_case_CURVE_2'
CURVE/2
, CLOSED
, MATRIX = 2
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_3'
CURVE/3
, CLOSED
, MATRIX = 3
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_4'
CURVE/4
, CLOSED
, MATRIX = 4
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_5'
CURVE/5
, CLOSED
, MATRIX = 5
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_6'
CURVE/6
, CLOSED
, MATRIX = 6
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_7'
CURVE/7
, CLOSED
, MATRIX = 7
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_8'
CURVE/8
, CLOSED
, MATRIX = 8
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_9'
CURVE/9
, CLOSED
, MATRIX = 9
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_10'
CURVE/10
, CLOSED
, MATRIX = 10
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_11'
CURVE/11
, CLOSED
, MATRIX = 11
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_12'
CURVE/12
, CLOSED
, MATRIX = 12
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_13'
CURVE/13
, CLOSED
, MATRIX = 13
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_14'
CURVE/14
, CLOSED
, MATRIX = 14
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_15'
CURVE/15
, CLOSED
, MATRIX = 15
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_16'
CURVE/16
, CLOSED
, MATRIX = 16
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_17'
CURVE/17
, CLOSED
, MATRIX = 17
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_18'
CURVE/18
, CLOSED
, MATRIX = 18
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_19'
CURVE/19
, CLOSED
, MATRIX = 19
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_20'
CURVE/20
, CLOSED
, MATRIX = 20
, CURVE_POINTS
, ORDER = 2
!
!                 adams_view_name='steering_wheel_rim_CURVE_21'
CURVE/21
, CLOSED
, MATRIX = 21
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_22'
CURVE/22
, CLOSED
, MATRIX = 22
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_23'
CURVE/23
, CLOSED
, MATRIX = 23
, CURVE_POINTS
, ORDER = 2
!
!                      adams_view_name='i_graphic_CURVE_24'
CURVE/24
, CLOSED
, MATRIX = 24
, CURVE_POINTS
, ORDER = 2
!
!--------------------------------- EQUATIONS -----------------------------------
!
!               adams_view_name='testrig.left_vertical_controller'
DIFF/2
, IC = 0
, FUNCTION = USER(903, 1, 0, 1, 2, 29, -20000, 40000, -250, 250, 1, 1, 1)\
, ROUTINE = acarSDM::dif903
!
!              adams_view_name='testrig.right_vertical_controller'
DIFF/3
, IC = 0
, FUNCTION = USER(903, 1, 0, 3, 3, 31, -20000, 40000, -250, 250, 1, 1, 1)\
, ROUTINE = acarSDM::dif903
!
!                 adams_view_name='testrig.controller_steering'
DIFF/4
, IC = 0
, FUNCTION = USER(903, 1, 0, 22, 49, 47, 0, 0, 0, 0, 1, 1, 1)\
, ROUTINE = acarSDM::dif903
!
!                    adams_view_name='testrig.til_wheel.dif1'
DIFF/5
, IC = 0
, FUNCTION = USER(900, 1, 11)\
, ROUTINE = abgTire::dif900
!
!                    adams_view_name='testrig.til_wheel.dif2'
DIFF/6
, IC = 0
, FUNCTION = USER(900, 1, 11)\
, ROUTINE = abgTire::dif900
!
!                    adams_view_name='testrig.tir_wheel.dif1'
DIFF/7
, IC = 0
, FUNCTION = USER(900, 2, 12)\
, ROUTINE = abgTire::dif900
!
!                    adams_view_name='testrig.tir_wheel.dif2'
DIFF/8
, IC = 0
, FUNCTION = USER(900, 2, 12)\
, ROUTINE = abgTire::dif900
!
!----------------------------------- OUTPUT ------------------------------------
!
!                 adams_view_name='testrig.steering_rack_input'
REQUEST/2
, TITLE = steering_rack_input
, COMMENT = Steering rack input (mode=length)
, CUNITS = "no_units", "length", "force", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "rack_input", "rack_input_force", "", "", "", "", ""
, RESULTS_NAME = steering_rack_input
, F2 = DZ(140, 60, 60)\
, F3 = FZ(140, 60, 60)
!
!                     adams_view_name='testrig.wheel_travel'
REQUEST/3
, TITLE = wheel_travel
, COMMENT = Wheel Center Vertical Travel
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "vertical_left", "vertical_right", "", "", "", "", ""
, RESULTS_NAME = wheel_travel
, F2 = DZ(74, 48, 46)\
, F3 = DZ(81, 49, 46)
!
!                  adams_view_name='testrig.anti_dive_braking'
REQUEST/4
, TITLE = anti_dive_braking
, COMMENT = Anti-Dive Braking (front)
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Percent Anti-Dive (%)", "Percent Anti-Dive (%)", "", "", "", ""
, ""
, RESULTS_NAME = anti_dive_braking
, FUNCTION = USER(900, 1, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.dive_braking'
REQUEST/5
, TITLE = dive_braking
, COMMENT = Dive Braking (front)
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Dive Braking (mm/g)", "Dive Braking (mm/g)", "", "", "", "", ""
, RESULTS_NAME = dive_braking
, FUNCTION = USER(900, 2, 5)\
, ROUTINE = acarSDM::req900
!
!                adams_view_name='testrig.anti_lift_acceleration'
REQUEST/6
, TITLE = anti_lift_acceleration
, COMMENT = Anti-Lift Acceleration (front)
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Percent Anti-Lift (%)", "Percent Anti-Lift (%)", "", "", "", ""
, ""
, RESULTS_NAME = anti_lift_acceleration
, FUNCTION = USER(900, 3, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.lift_acceleration'
REQUEST/7
, TITLE = lift_acceleration
, COMMENT = Lift Acceleration (front)
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Lift Acceleration (mm/g)", "Lift Acceleration (mm/g)", "", ""
, "", "", ""
, RESULTS_NAME = lift_acceleration
, FUNCTION = USER(900, 4, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.anti_lift_braking'
REQUEST/8
, TITLE = anti_lift_braking
, COMMENT = Anti-Lift Braking (rear)
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Percent Anti-Lift (%)", "Percent Anti-Lift (%)", "", "", "", ""
, ""
, RESULTS_NAME = anti_lift_braking
, FUNCTION = USER(900, 1, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.lift_braking'
REQUEST/9
, TITLE = lift_braking
, COMMENT = Lift Braking (rear)
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Lift Braking (mm/g)", "Lift Braking (mm/g)", "", "", "", "", ""
, RESULTS_NAME = lift_braking
, FUNCTION = USER(900, 2, 5)\
, ROUTINE = acarSDM::req900
!
!               adams_view_name='testrig.anti_squat_acceleration'
REQUEST/10
, TITLE = anti_squat_acceleration
, COMMENT = Anti-Squat Acceleration (rear)
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Percent Anti-Squat (%)", "Percent Anti-Squat (%)", "", "", ""
, "", ""
, RESULTS_NAME = anti_squat_acceleration
, FUNCTION = USER(900, 3, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.squat_acceleration'
REQUEST/11
, TITLE = squat_acceleration
, COMMENT = Squat Acceleration (rear)
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, CLABELS = "", "Squat Acceleration (mm/g)", "Squat Acceleration (mm/g)", "", ""
, "", "", ""
, RESULTS_NAME = squat_acceleration
, FUNCTION = USER(900, 4, 5)\
, ROUTINE = acarSDM::req900
!
!                adams_view_name='testrig.alt_camber_compliance'
REQUEST/12
, TITLE = alt_camber_compliance
, COMMENT = Aligning torque camber compliance
, CUNITS = "no_units", "angle/force/length", "angle/force/length", "no_units"
, "no_units", "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = alt_camber_compliance
, FUNCTION = USER(900, 5, 5)\
, ROUTINE = acarSDM::req900
!
!                 adams_view_name='testrig.alt_steer_compliance'
REQUEST/13
, TITLE = alt_steer_compliance
, COMMENT = Aligning torque steer compliance
, CUNITS = "no_units", "angle/force/length", "angle/force/length", "no_units"
, "no_units", "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = alt_steer_compliance
, FUNCTION = USER(900, 6, 5)\
, ROUTINE = acarSDM::req900
!
!           adams_view_name='testrig.fore_aft_wheel_center_stiffness'
REQUEST/14
, TITLE = fore_aft_wheel_center_stiffness
, COMMENT = Fore-aft wheel center stiffness
, CUNITS = "no_units", "stiffness", "stiffness", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = fore_aft_wheel_center_stiffness
, FUNCTION = USER(900, 7, 5)\
, ROUTINE = acarSDM::req900
!
!               adams_view_name='testrig.fr_view_swing_arm_angle'
REQUEST/15
, TITLE = fr_view_swing_arm_angle
, COMMENT = Front view swing arm angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = fr_view_swing_arm_angle
, FUNCTION = USER(900, 8, 5)\
, ROUTINE = acarSDM::req900
!
!               adams_view_name='testrig.fr_view_swing_arm_length'
REQUEST/16
, TITLE = fr_view_swing_arm_length
, COMMENT = Front view swing arm length
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = fr_view_swing_arm_length
, FUNCTION = USER(900, 9, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.caster_angle'
REQUEST/17
, TITLE = caster_angle
, COMMENT = Caster angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = caster_angle
, FUNCTION = USER(900, 10, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.kingpin_incl_angle'
REQUEST/18
, TITLE = kingpin_incl_angle
, COMMENT = Kingpin inclination angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = kingpin_incl_angle
, FUNCTION = USER(900, 11, 5)\
, ROUTINE = acarSDM::req900
!
!              adams_view_name='testrig.lat_force_defl_compliance'
REQUEST/19
, TITLE = lat_force_defl_compliance
, COMMENT = Lateral force deflection compliance
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = lat_force_defl_compliance
, FUNCTION = USER(900, 12, 5)\
, ROUTINE = acarSDM::req900
!
!              adams_view_name='testrig.lat_force_steer_compliance'
REQUEST/20
, TITLE = lat_force_steer_compliance
, COMMENT = Lateral force steer compliance
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = lat_force_steer_compliance
, FUNCTION = USER(900, 13, 5)\
, ROUTINE = acarSDM::req900
!
!             adams_view_name='testrig.lat_force_camber_compliance'
REQUEST/21
, TITLE = lat_force_camber_compliance
, COMMENT = Lateral force camber compliance
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = lat_force_camber_compliance
, FUNCTION = USER(900, 14, 5)\
, ROUTINE = acarSDM::req900
!
!               adams_view_name='testrig.roll_camber_coefficient'
REQUEST/22
, TITLE = roll_camber_coefficient
, COMMENT = Roll camber coefficient
, CUNITS = "no_units", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = roll_camber_coefficient
, FUNCTION = USER(900, 15, 5)\
, ROUTINE = acarSDM::req900
!
!               adams_view_name='testrig.roll_caster_coefficient'
REQUEST/23
, TITLE = roll_caster_coefficient
, COMMENT = Roll caster coefficient
, CUNITS = "no_units", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = roll_caster_coefficient
, FUNCTION = USER(900, 16, 5)\
, ROUTINE = acarSDM::req900
!
!                      adams_view_name='testrig.roll_steer'
REQUEST/24
, TITLE = roll_steer
, COMMENT = Roll steer
, CUNITS = "no_units", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = roll_steer
, FUNCTION = USER(900, 17, 5)\
, ROUTINE = acarSDM::req900
!
!                    adams_view_name='testrig.roll_center_1'
REQUEST/25
, TITLE = roll_center_location
, COMMENT = Roll center position
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "lateral_from_half_track", "vertical", "", "", "", "", ""
, RESULTS_NAME = roll_center_location
, FUNCTION = USER(900, 18, 5)\
, ROUTINE = acarSDM::req900
!
!                      adams_view_name='testrig.wheel_rate'
REQUEST/26
, TITLE = wheel_rate
, COMMENT = Wheel Rate
, CUNITS = "no_units", "stiffness", "stiffness", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = wheel_rate
, FUNCTION = USER(900, 19, 5)\
, ROUTINE = acarSDM::req900
!
!                      adams_view_name='testrig.ride_rate'
REQUEST/27
, TITLE = ride_rate
, COMMENT = Ride rate
, CUNITS = "no_units", "stiffness", "stiffness", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = ride_rate
, FUNCTION = USER(900, 20, 5)\
, ROUTINE = acarSDM::req900
!
!                    adams_view_name='testrig.susp_roll_rate'
REQUEST/28
, TITLE = susp_roll_rate
, COMMENT = Suspension roll rate
, CUNITS = "no_units", "torsion_stiffness", "no_units", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "suspension_roll_rate", "", "", "", "", "", ""
, RESULTS_NAME = susp_roll_rate
, FUNCTION = USER(900, 21, 5)\
, ROUTINE = acarSDM::req900
!
!                   adams_view_name='testrig.total_roll_rate'
REQUEST/29
, TITLE = total_roll_rate
, COMMENT = Total roll rate
, CUNITS = "no_units", "torsion_stiffness", "no_units", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "total_roll_rate", "", "", "", "", "", ""
, RESULTS_NAME = total_roll_rate
, FUNCTION = USER(900, 22, 5)\
, ROUTINE = acarSDM::req900
!
!                      adams_view_name='testrig.ride_steer'
REQUEST/30
, TITLE = ride_steer
, COMMENT = Ride steer
, CUNITS = "no_units", "angle/length", "angle/length", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = ride_steer
, FUNCTION = USER(900, 23, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.scrub_radius'
REQUEST/31
, TITLE = scrub_radius
, COMMENT = Scrub radius
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = scrub_radius
, FUNCTION = USER(900, 24, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.caster_moment_arm'
REQUEST/32
, TITLE = caster_moment_arm
, COMMENT = Caster moment arm
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = caster_moment_arm
, FUNCTION = USER(900, 25, 5)\
, ROUTINE = acarSDM::req900
!
!                   adams_view_name='testrig.side_view_angle'
REQUEST/33
, TITLE = side_view_angle
, COMMENT = Wheel_carrier side view rotation angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = side_view_angle
, F2 = AZ(450, 62)\
, F3 = AZ(463, 62)
!
!              adams_view_name='testrig.side_view_swing_arm_angle'
REQUEST/34
, TITLE = side_view_swing_arm_angle
, COMMENT = Side view swing arm angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = side_view_swing_arm_angle
, FUNCTION = USER(900, 26, 5)\
, ROUTINE = acarSDM::req900
!
!              adams_view_name='testrig.side_view_swing_arm_length'
REQUEST/35
, TITLE = side_view_swing_arm_length
, COMMENT = Side view swing arm length
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = side_view_swing_arm_length
, FUNCTION = USER(900, 27, 5)\
, ROUTINE = acarSDM::req900
!
!                      adams_view_name='testrig.toe_angle'
REQUEST/36
, TITLE = toe_angle
, COMMENT = Toe angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = toe_angle
, FUNCTION = USER(900, 28, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.camber_angle'
REQUEST/37
, TITLE = camber_angle
, COMMENT = Camber Angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = camber_angle
, FUNCTION = USER(900, 29, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.inclination_angle'
REQUEST/38
, TITLE = inclination_angle
, COMMENT = Inclination Angle (relative to the road)
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = inclination_angle
, FUNCTION = USER(900, 39, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.steer_angle'
REQUEST/39
, TITLE = steer_angle
, COMMENT = Steer Angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = steer_angle
, FUNCTION = USER(900, 31, 5)\
, ROUTINE = acarSDM::req900
!
!                    adams_view_name='testrig.ackerman_angle'
REQUEST/40
, TITLE = ackerman_angle
, COMMENT = Ackerman angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = ackerman_angle
, FUNCTION = USER(900, 32, 5)\
, ROUTINE = acarSDM::req900
!
!                       adams_view_name='testrig.ackerman'
REQUEST/41
, TITLE = ackerman
, COMMENT = Ackerman
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = ackerman
, FUNCTION = USER(900, 33, 5)\
, ROUTINE = acarSDM::req900
!
!                   adams_view_name='testrig.percent_ackerman'
REQUEST/42
, TITLE = percent_ackerman
, COMMENT = Percent Ackerman
, CUNITS = "no_units", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = percent_ackerman
, FUNCTION = USER(900, 34, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.ideal_steer_angle'
REQUEST/43
, TITLE = ideal_steer_angle
, COMMENT = Ideal Steer Angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = ideal_steer_angle
, FUNCTION = USER(900, 35, 5)\
, ROUTINE = acarSDM::req900
!
!                    adams_view_name='testrig.ackerman_error'
REQUEST/44
, TITLE = ackerman_error
, COMMENT = Ackerman Error
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = ackerman_error
, FUNCTION = USER(900, 36, 5)\
, ROUTINE = acarSDM::req900
!
!                adams_view_name='testrig.outside_turn_diameter'
REQUEST/45
, TITLE = outside_turn_diameter
, COMMENT = Outside Turn Diameter
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = outside_turn_diameter
, FUNCTION = USER(900, 37, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.turn_radius'
REQUEST/46
, TITLE = turn_radius
, COMMENT = Turn Radius
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = turn_radius
, FUNCTION = USER(900, 38, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.steer_axis_offset'
REQUEST/47
, TITLE = steer_axis_offset
, COMMENT = Steer Axis Offset
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "off_left", "off_right", "", "", "", "", ""
, RESULTS_NAME = steer_axis_offset
, FUNCTION = USER(900, 44, 5)\
, ROUTINE = acarSDM::req900
!
!            adams_view_name='testrig.steer_axis_offset_longitudinal'
REQUEST/48
, TITLE = steer_axis_offset
, COMMENT = Steer Axis Offset - Longitudinal
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "lon_left", "lon_right", "", "", "", "", ""
, RESULTS_NAME = steer_axis_offset
, FUNCTION = USER(900, 45, 5)\
, ROUTINE = acarSDM::req900
!
!              adams_view_name='testrig.steer_axis_offset_lateral'
REQUEST/49
, TITLE = steer_axis_offset
, COMMENT = Steer Axis Offset - Lateral
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "lat_left", "lat_right", "", "", "", "", ""
, RESULTS_NAME = steer_axis_offset
, FUNCTION = USER(900, 46, 5)\
, ROUTINE = acarSDM::req900
!
!                     adams_view_name='testrig.total_track'
REQUEST/50
, TITLE = total_track
, COMMENT = Total Track
, CUNITS = "no_units", "length", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "track", "", "", "", "", "", ""
, RESULTS_NAME = total_track
, FUNCTION = USER(900, 47, 5)\
, ROUTINE = acarSDM::req900
!
!                  adams_view_name='testrig.wheel_travel_base'
REQUEST/51
, TITLE = wheel_travel_base
, COMMENT = Wheel Center Longitudinal Travel
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "base_left", "base_right", "", "", "", "", ""
, RESULTS_NAME = wheel_travel_base
, F2 = DX(74, 48, 46)\
, F3 = DX(81, 49, 46)
!
!                  adams_view_name='testrig.wheel_travel_track'
REQUEST/52
, TITLE = wheel_travel_track
, COMMENT = Wheel Center Lateral Travel
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "track_left", "track_right", "", "", "", "", ""
, RESULTS_NAME = wheel_travel_track
, F2 = DY(74, 48, 46)\
, F3 = DY(81, 49, 46)
!
!               adams_view_name='testrig.left_tire_contact_point'
REQUEST/53
, TITLE = left_tire_contact_point
, COMMENT = Left Tire Contact Patch Travel
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "base_change_left", "track_change_left", "", "", "", "", ""
, RESULTS_NAME = left_tire_contact_point
, FUNCTION = USER(902, 10, 1)\
, ROUTINE = abgTire::req902
!
!               adams_view_name='testrig.right_tire_contact_point'
REQUEST/54
, TITLE = right_tire_contact_point
, COMMENT = Right Tire Contact Patch Travel
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "base_change_right", "track_change_right", "", "", "", "", ""
, RESULTS_NAME = right_tire_contact_point
, FUNCTION = USER(902, 10, 2)\
, ROUTINE = abgTire::req902
!
!           adams_view_name='testrig.left_tire_contact_point_position'
REQUEST/55
, TITLE = left_tire_contact_point_position
, COMMENT = Left Tire Contact Patch Position
, CUNITS = "no_units", "length", "length", "length", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "x_left", "y_left", "z_left", "", "", "", ""
, RESULTS_NAME = left_tire_contact_point
, FUNCTION = USER(902, 19, 1)\
, ROUTINE = abgTire::req902
!
!          adams_view_name='testrig.right_tire_contact_point_position'
REQUEST/56
, TITLE = right_tire_contact_point_position
, COMMENT = Right Tire Contact Patch Position
, CUNITS = "no_units", "length", "length", "length", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "x_right", "y_right", "z_right", "", "", "", ""
, RESULTS_NAME = right_tire_contact_point
, FUNCTION = USER(902, 19, 2)\
, ROUTINE = abgTire::req902
!
!                      adams_view_name='testrig.roll_angle'
REQUEST/57
, TITLE = roll_angle
, COMMENT = Suspension Roll Angle
, CUNITS = "no_units", "angle", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "at_wheel_centers", "at_contact_patches", "", "", "", "", ""
, RESULTS_NAME = roll_angle
, F2 = ATAN(DZ(74, 81, 46)/
,ABS(DY(74, 81, 46)))\
, F3 = ATAN(DZ(90,103, 46)/
,ABS(DY(90,103, 46)))
!
!                 adams_view_name='testrig.left_wheelenv_output'
REQUEST/58
, TITLE = wheelenv_output
, COMMENT = Wheel Envelope Left Spindle Coordinates
, CUNITS = "no_units", "length", "length", "length", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "wheel_ctr_x_left", "wheel_ctr_y_left", "wheel_ctr_z_left", ""
, "wheel_axis_x_left", "wheel_axis_y_left", "wheel_axis_z_left"
, RESULTS_NAME = wheelenv_output
, FUNCTION = USER(901, 1, 74, 81, 1000)\
, ROUTINE = acarSDM::req901
!
!                adams_view_name='testrig.right_wheelenv_output'
REQUEST/59
, TITLE = wheelenv_output
, COMMENT = Wheel Envelope Right Spindle Coordinates
, CUNITS = "no_units", "length", "length", "length", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "wheel_ctr_x_right", "wheel_ctr_y_right", "wheel_ctr_z_right", ""
, "wheel_axis_x_right", "wheel_axis_y_right", "wheel_axis_z_right"
, RESULTS_NAME = wheelenv_output
, FUNCTION = USER(901, 2, 74, 81, 1000)\
, ROUTINE = acarSDM::req901
!
!                    adams_view_name='testrig.roll_center_2'
REQUEST/60
, TITLE = roll_center_location
, COMMENT = Roll Center Lateral Position Relative To Contact Patches
, CUNITS = "no_units", "length", "length", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "lateral_to_left_patch", "lateral_to_right_patch", "", "", "", ""
, ""
, RESULTS_NAME = roll_center_location
, FUNCTION = USER(900, 43, 5)\
, ROUTINE = acarSDM::req900
!
!               adams_view_name='testrig.wheel_load_longitudinal'
REQUEST/61
, TITLE = wheel_load_longitudinal
, COMMENT = Longitudinal Wheel Load
, CUNITS = "no_units", "force", "force", "no_units", "no_units", "force"
, "force", "no_units"
, CNAMES = "", "braking_left", "braking_right", "", "", "driving_left"
, "driving_right", ""
, RESULTS_NAME = wheel_load_longitudinal
, F2 = AKISPL(11,time,2)\
, F3 = AKISPL(12,time,2)\
, F6 = AKISPL(13,time,2)\
, F7 = AKISPL(14,time,2)
!
!                  adams_view_name='testrig.wheel_load_lateral'
REQUEST/62
, TITLE = wheel_load_lateral
, COMMENT = Lateral Wheel Load
, CUNITS = "no_units", "force", "force", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "lateral_left", "lateral_right", "", "", "", "", ""
, RESULTS_NAME = wheel_load_lateral
, F2 = AKISPL(3,time,2)\
, F3 = AKISPL(4,time,2)
!
!              adams_view_name='testrig.wheel_load_vertical_force'
REQUEST/63
, TITLE = wheel_load_vertical_force
, COMMENT = Vertical Wheel Load (mode=force)
, CUNITS = "no_units", "force", "force", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "vertical_left_force", "vertical_right_force", "", "", "", "", ""
, RESULTS_NAME = wheel_load_vertical_force
, F2 = AKISPL(1,time,2)\
, F3 = AKISPL(2,time,2)
!
!                 adams_view_name='testrig.jack_vertical_force'
REQUEST/64
, TITLE = jack_vertical_force
, COMMENT = Vertical Input at Jack
, CUNITS = "no_units", "force", "force", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "left", "right", "", "", "", "", ""
, RESULTS_NAME = jack_vertical_force
, F2 = SFORCE(1, 0, 4, 46)\
, F3 = SFORCE(3, 0, 4, 46)
!
!                   adams_view_name='testrig.wheel_load_align'
REQUEST/65
, TITLE = wheel_load_align
, COMMENT = Vertical Wheel Torque
, CUNITS = "no_units", "torque", "torque", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "algn_torque_left", "algn_torque_right", "", "", "", "", ""
, RESULTS_NAME = wheel_load_align
, F2 = AKISPL(9,time,2)\
, F3 = AKISPL(10,time,2)
!
!                   adams_view_name='testrig.kingpin_location'
REQUEST/66
, TITLE = kingpin_location
, COMMENT = Kingpin axis point location relative to global reference frame
, CUNITS = "no_units", "length", "length", "length", "no_units", "length"
, "length", "length"
, CNAMES = "", "left_X", "left_Y", "left_Z", "", "right_X", "right_Y", "right_Z"
, RESULTS_NAME = kingpin_location
, FUNCTION = USER(900, 50, 5)\
, ROUTINE = acarSDM::req900
!
!             adams_view_name='testrig.til_wheel.hub_forces_request'
REQUEST/67
, CUNITS = "no_units", "force", "force", "force", "no_units", "torque", "torque"
, "torque"
, CNAMES = "", "longitudinal", "lateral", "normal", "", "overturning_moment"
, "rotational_torque", "aligning_torque"
, RESULTS_NAME = left_hub_forces
, FUNCTION = USER(902, 6, 1)\
, ROUTINE = abgTire::req902
!
!               adams_view_name='testrig.til_wheel.forces_request'
REQUEST/68
, CUNITS = "no_units", "force", "force", "force", "no_units", "torque", "torque"
, "torque"
, CNAMES = "", "longitudinal", "lateral", "normal", "", "overturning_moment"
, "rotational_torque", "aligning_torque"
, RESULTS_NAME = left_tire_forces
, FUNCTION = USER(902, 3, 1)\
, ROUTINE = abgTire::req902
!
!             adams_view_name='testrig.tir_wheel.hub_forces_request'
REQUEST/69
, CUNITS = "no_units", "force", "force", "force", "no_units", "torque", "torque"
, "torque"
, CNAMES = "", "longitudinal", "lateral", "normal", "", "overturning_moment"
, "rotational_torque", "aligning_torque"
, RESULTS_NAME = right_hub_forces
, FUNCTION = USER(902, 6, 2)\
, ROUTINE = abgTire::req902
!
!               adams_view_name='testrig.tir_wheel.forces_request'
REQUEST/70
, CUNITS = "no_units", "force", "force", "force", "no_units", "torque", "torque"
, "torque"
, CNAMES = "", "longitudinal", "lateral", "normal", "", "overturning_moment"
, "rotational_torque", "aligning_torque"
, RESULTS_NAME = right_tire_forces
, FUNCTION = USER(902, 3, 2)\
, ROUTINE = abgTire::req902
!
!               adams_view_name='testrig.jml_bearing_lock.request'
REQUEST/71
, CUNITS = "no_units", "angle", "angular_velocity", "torque", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "displacement", "velocity", "torque", "", "", "", ""
, RESULTS_NAME = jml_bearing_lock_data
, FUNCTION = USER(909, 80, 451, 1, 0, 13, 1.0E-07)\
, ROUTINE = abgFDM::req909
!
!               adams_view_name='testrig.jmr_bearing_lock.request'
REQUEST/72
, CUNITS = "no_units", "angle", "angular_velocity", "torque", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "displacement", "velocity", "torque", "", "", "", ""
, RESULTS_NAME = jmr_bearing_lock_data
, FUNCTION = USER(909, 87, 464, 1, 0, 15, 1.0E-07)\
, ROUTINE = abgFDM::req909
!
!                adams_view_name='testrig.jfl_jack_force.request'
REQUEST/73
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "displacement", "velocity", "force", "", "", "", ""
, RESULTS_NAME = jfl_jack_force_data
, FUNCTION = USER(909, 120, 4, 0, 1, 17, 1.0E-07)\
, ROUTINE = abgFDM::req909
!
!                adams_view_name='testrig.jfr_jack_force.request'
REQUEST/74
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "displacement", "velocity", "force", "", "", "", ""
, RESULTS_NAME = jfr_jack_force_data
, FUNCTION = USER(909, 130, 9, 0, 1, 19, 1.0E-07)\
, ROUTINE = abgFDM::req909
!
!               adams_view_name='testrig.rer_retract_stop.request'
REQUEST/75
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "length"
, "no_units", "no_units"
, CNAMES = "", "displacement", "velocity", "force", "", "clearance", "", ""
, RESULTS_NAME = rer_retract_stop_data
, FUNCTION = USER(904, 133, 10, 0, 1.0E-07, 520)\
, ROUTINE = abgFDM::req904
!
!               adams_view_name='testrig.rel_retract_stop.request'
REQUEST/76
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "length"
, "no_units", "no_units"
, CNAMES = "", "displacement", "velocity", "force", "", "clearance", "", ""
, RESULTS_NAME = rel_retract_stop_data
, FUNCTION = USER(904, 123, 5, 0, 1.0E-07, 520)\
, ROUTINE = abgFDM::req904
!
!              adams_view_name='testrig.jfs_steering_input.request'
REQUEST/81
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "displacement", "velocity", "force", "", "", "", ""
, RESULTS_NAME = jfs_steering_input_data
, FUNCTION = USER(909, 141, 144, 0, 1, 38, 1.0E-07)\
, ROUTINE = abgFDM::req909
!
!                     adams_view_name='FRT_SUSP.toe_camber'
REQUEST/92
, COMMENT = Computes the toe and camber of a front or rear suspension
, CUNITS = "no_units", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units", "no_units"
, CNAMES = "", "toe_left_front", "", "camber_left_front", "", "toe_right_front"
, "", "camber_right_front"
, RESULTS_NAME = suspension_kinematics
, FUNCTION = USER(1101, 0, 321, 320, 0, 340, 339, 2, 1, 191)\
, ROUTINE = apresolver::reqsub
!
!           adams_view_name='FRT_SUSP.bgr_subframe_front.disp_request'
REQUEST/93
, CUNITS = "length", "length", "length", "length", "angle", "angle", "angle"
, "angle"
, CNAMES = "dm_front", "dx_front", "dy_front", "dz_front", "amag_front"
, "ax_front", "ay_front", "az_front"
, RESULTS_NAME = bgr_subframe_front_disp
, FUNCTION = USER(905, 1, 348, 17, 2, 17, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgr_subframe_front.velo_request'
REQUEST/94
, CUNITS = "velocity", "velocity", "velocity", "velocity", "angular_velocity"
, "angular_velocity", "angular_velocity", "angular_velocity"
, CNAMES = "vm_front", "vx_front", "vy_front", "vz_front", "wm_front"
, "wx_front", "wy_front", "wz_front"
, RESULTS_NAME = bgr_subframe_front_velo
, FUNCTION = USER(905, 2, 348, 17, 2, 17, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!          adams_view_name='FRT_SUSP.bgr_subframe_front.force_request'
REQUEST/95
, CUNITS = "force", "force", "force", "force", "torque", "torque", "torque"
, "torque"
, CNAMES = "fm_front", "fx_front", "fy_front", "fz_front", "tm_front"
, "tx_front", "ty_front", "tz_front"
, RESULTS_NAME = bgr_subframe_front_force
, FUNCTION = USER(905, 3, 348, 17, 2, 17, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.disp_request'
REQUEST/96
, CUNITS = "length", "length", "length", "length", "angle", "angle", "angle"
, "angle"
, CNAMES = "dm_front", "dx_front", "dy_front", "dz_front", "amag_front"
, "ax_front", "ay_front", "az_front"
, RESULTS_NAME = bgl_subframe_rear_disp
, FUNCTION = USER(905, 1, 349, 18, 3, 18, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.velo_request'
REQUEST/97
, CUNITS = "velocity", "velocity", "velocity", "velocity", "angular_velocity"
, "angular_velocity", "angular_velocity", "angular_velocity"
, CNAMES = "vm_front", "vx_front", "vy_front", "vz_front", "wm_front"
, "wx_front", "wy_front", "wz_front"
, RESULTS_NAME = bgl_subframe_rear_velo
, FUNCTION = USER(905, 2, 349, 18, 3, 18, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgl_subframe_rear.force_request'
REQUEST/98
, CUNITS = "force", "force", "force", "force", "torque", "torque", "torque"
, "torque"
, CNAMES = "fm_front", "fx_front", "fy_front", "fz_front", "tm_front"
, "tx_front", "ty_front", "tz_front"
, RESULTS_NAME = bgl_subframe_rear_force
, FUNCTION = USER(905, 3, 349, 18, 3, 18, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.disp_request'
REQUEST/99
, CUNITS = "length", "length", "length", "length", "angle", "angle", "angle"
, "angle"
, CNAMES = "dm_front", "dx_front", "dy_front", "dz_front", "amag_front"
, "ax_front", "ay_front", "az_front"
, RESULTS_NAME = bgr_subframe_rear_disp
, FUNCTION = USER(905, 1, 350, 19, 4, 19, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.velo_request'
REQUEST/100
, CUNITS = "velocity", "velocity", "velocity", "velocity", "angular_velocity"
, "angular_velocity", "angular_velocity", "angular_velocity"
, CNAMES = "vm_front", "vx_front", "vy_front", "vz_front", "wm_front"
, "wx_front", "wy_front", "wz_front"
, RESULTS_NAME = bgr_subframe_rear_velo
, FUNCTION = USER(905, 2, 350, 19, 4, 19, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgr_subframe_rear.force_request'
REQUEST/101
, CUNITS = "force", "force", "force", "force", "torque", "torque", "torque"
, "torque"
, CNAMES = "fm_front", "fx_front", "fy_front", "fz_front", "tm_front"
, "tx_front", "ty_front", "tz_front"
, RESULTS_NAME = bgr_subframe_rear_force
, FUNCTION = USER(905, 3, 350, 19, 4, 19, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!               adams_view_name='FRT_SUSP.nsl_ride_spring.request'
REQUEST/138
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "displacement_front", "velocity_front", "force_front", "", "", ""
, ""
, RESULTS_NAME = nsl_ride_spring_data
, FUNCTION = USER(904, 26, 426, 0, 1.0E-07)\
, ROUTINE = abgFDM::req904
!
!               adams_view_name='FRT_SUSP.nsr_ride_spring.request'
REQUEST/139
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "displacement_front", "velocity_front", "force_front", "", "", ""
, ""
, RESULTS_NAME = nsr_ride_spring_data
, FUNCTION = USER(904, 30, 435, 0, 1.0E-07)\
, ROUTINE = abgFDM::req904
!
!               adams_view_name='FRT_SUSP.dal_ride_damper.request'
REQUEST/140
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "displacement_front", "velocity_front", "force_front", "", "", ""
, ""
, RESULTS_NAME = dal_ride_damper_data
, FUNCTION = USER(904, 380, 425, 0, 1.0E-07)\
, ROUTINE = abgFDM::req904
!
!               adams_view_name='FRT_SUSP.dar_ride_damper.request'
REQUEST/141
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "displacement_front", "velocity_front", "force_front", "", "", ""
, ""
, RESULTS_NAME = dar_ride_damper_data
, FUNCTION = USER(904, 388, 434, 0, 1.0E-07)\
, ROUTINE = abgFDM::req904
!
!           adams_view_name='FRT_SUSP.bgl_subframe_front.disp_request'
REQUEST/142
, CUNITS = "length", "length", "length", "length", "angle", "angle", "angle"
, "angle"
, CNAMES = "dm_front", "dx_front", "dy_front", "dz_front", "amag_front"
, "ax_front", "ay_front", "az_front"
, RESULTS_NAME = bgl_subframe_front_disp
, FUNCTION = USER(905, 1, 347, 16, 17, 16, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!           adams_view_name='FRT_SUSP.bgl_subframe_front.velo_request'
REQUEST/143
, CUNITS = "velocity", "velocity", "velocity", "velocity", "angular_velocity"
, "angular_velocity", "angular_velocity", "angular_velocity"
, CNAMES = "vm_front", "vx_front", "vy_front", "vz_front", "wm_front"
, "wx_front", "wy_front", "wz_front"
, RESULTS_NAME = bgl_subframe_front_velo
, FUNCTION = USER(905, 2, 347, 16, 17, 16, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!          adams_view_name='FRT_SUSP.bgl_subframe_front.force_request'
REQUEST/144
, CUNITS = "force", "force", "force", "force", "torque", "torque", "torque"
, "torque"
, CNAMES = "fm_front", "fx_front", "fy_front", "fz_front", "tm_front"
, "tx_front", "ty_front", "tz_front"
, RESULTS_NAME = bgl_subframe_front_force
, FUNCTION = USER(905, 3, 347, 16, 17, 16, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!             adams_view_name='FRT_SUSP.afl_camber_adjuster.request'
REQUEST/151
, CUNITS = "no_units", "length", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "dm_front", "", "", "", "", "", ""
, RESULTS_NAME = afl_camber_adjuster_motion_lock
, F2 = (DM(270,230))
!
!             adams_view_name='FRT_SUSP.afr_camber_adjuster.request'
REQUEST/152
, CUNITS = "no_units", "length", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "dm_front", "", "", "", "", "", ""
, RESULTS_NAME = afr_camber_adjuster_motion_lock
, F2 = (DM(289,237))
!
!              adams_view_name='FRT_SUSP.afl_toe_adjuster.request'
REQUEST/153
, CUNITS = "no_units", "length", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "dm_front", "", "", "", "", "", ""
, RESULTS_NAME = afl_toe_adjuster_motion_lock
, F2 = (DM(245,259))
!
!              adams_view_name='FRT_SUSP.afr_toe_adjuster.request'
REQUEST/154
, CUNITS = "no_units", "length", "no_units", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "dm_front", "", "", "", "", "", ""
, RESULTS_NAME = afr_toe_adjuster_motion_lock
, F2 = (DM(252,267))
!
!               adams_view_name='FRT_SUSP.bul_jounce_stop.request'
REQUEST/155
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "length"
, "no_units", "no_units"
, CNAMES = "", "displacement_front", "velocity_front", "force_front", ""
, "clearance_front", "", ""
, RESULTS_NAME = bul_jounce_stop_data
, FUNCTION = USER(904, 379, 422, 0, 1.0E-07, -671.7250653)\
, ROUTINE = abgFDM::req904
!
!               adams_view_name='FRT_SUSP.bur_jounce_stop.request'
REQUEST/156
, CUNITS = "no_units", "length", "velocity", "force", "no_units", "length"
, "no_units", "no_units"
, CNAMES = "", "displacement_front", "velocity_front", "force_front", ""
, "clearance_front", "", ""
, RESULTS_NAME = bur_jounce_stop_data
, FUNCTION = USER(904, 387, 431, 0, 1.0E-07, -671.7250653)\
, ROUTINE = abgFDM::req904
!
!           adams_view_name='MDI_FRONT_STEERING.steering_wheel_angle'
REQUEST/157
, CUNITS = "no_units", "no_units", "no_units", "no_units", "no_units", "angle"
, "no_units", "no_units"
, CNAMES = "", "", "", "", "", "angle_front", "", ""
, RESULTS_NAME = steering_displacements
, F6 = AZ(520,42)
!
!      adams_view_name='MDI_FRONT_STEERING.pinion_rotational_displacement'
REQUEST/158
, CUNITS = "no_units", "no_units", "angle", "no_units", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "", "pinion_displacement_front", "", "", "", "", ""
, RESULTS_NAME = steering_displacements
, F3 = AZ(525,532)
!
!                adams_view_name='MDI_FRONT_STEERING.rack_travel'
REQUEST/159
, CUNITS = "no_units", "no_units", "no_units", "length", "no_units", "no_units"
, "no_units", "no_units"
, CNAMES = "", "", "", "rack_displacement_front", "", "", "", ""
, RESULTS_NAME = steering_displacements
, F4 = DZ(513,531,531)
!
!              adams_view_name='MDI_FRONT_STEERING.steering_assist'
REQUEST/160
, CUNITS = "no_units", "no_units", "no_units", "force", "no_units", "angle"
, "torque", "torque"
, CNAMES = "", "", "", "force_front", "", "angle_front"
, "torsion_bar_torque_front", "pinion_torque_front"
, RESULTS_NAME = steering_assist
, F4 = FZ(515,540,515)\
, F6 = AZ(508,526)\
, F7 = TZ(508,526,526)\
, F8 = TZ(532,525,525)
!
!   adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.disp_request'
REQUEST/161
, CUNITS = "length", "length", "length", "length", "angle", "angle", "angle"
, "angle"
, CNAMES = "dm_front", "dx_front", "dy_front", "dz_front", "amag_front"
, "ax_front", "ay_front", "az_front"
, RESULTS_NAME = bkl_rack_housing_bushing_disp
, FUNCTION = USER(905, 1, 535, 558, 20, 558, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!   adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.velo_request'
REQUEST/162
, CUNITS = "velocity", "velocity", "velocity", "velocity", "angular_velocity"
, "angular_velocity", "angular_velocity", "angular_velocity"
, CNAMES = "vm_front", "vx_front", "vy_front", "vz_front", "wm_front"
, "wx_front", "wy_front", "wz_front"
, RESULTS_NAME = bkl_rack_housing_bushing_velo
, FUNCTION = USER(905, 2, 535, 558, 20, 558, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!  adams_view_name='MDI_FRONT_STEERING.bkl_rack_housing_bushing.force_request'
REQUEST/163
, CUNITS = "force", "force", "force", "force", "torque", "torque", "torque"
, "torque"
, CNAMES = "fm_front", "fx_front", "fy_front", "fz_front", "tm_front"
, "tx_front", "ty_front", "tz_front"
, RESULTS_NAME = bkl_rack_housing_bushing_force
, FUNCTION = USER(905, 3, 535, 558, 20, 558, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!   adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.disp_request'
REQUEST/164
, CUNITS = "length", "length", "length", "length", "angle", "angle", "angle"
, "angle"
, CNAMES = "dm_front", "dx_front", "dy_front", "dz_front", "amag_front"
, "ax_front", "ay_front", "az_front"
, RESULTS_NAME = bkr_rack_housing_bushing_disp
, FUNCTION = USER(905, 1, 536, 559, 21, 559, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!   adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.velo_request'
REQUEST/165
, CUNITS = "velocity", "velocity", "velocity", "velocity", "angular_velocity"
, "angular_velocity", "angular_velocity", "angular_velocity"
, CNAMES = "vm_front", "vx_front", "vy_front", "vz_front", "wm_front"
, "wx_front", "wy_front", "wz_front"
, RESULTS_NAME = bkr_rack_housing_bushing_velo
, FUNCTION = USER(905, 2, 536, 559, 21, 559, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!  adams_view_name='MDI_FRONT_STEERING.bkr_rack_housing_bushing.force_request'
REQUEST/166
, CUNITS = "force", "force", "force", "force", "torque", "torque", "torque"
, "torque"
, CNAMES = "fm_front", "fx_front", "fy_front", "fz_front", "tm_front"
, "tx_front", "ty_front", "tz_front"
, RESULTS_NAME = bkr_rack_housing_bushing_force
, FUNCTION = USER(905, 3, 536, 559, 21, 559, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.disp_request'
REQUEST/167
, CUNITS = "length", "length", "length", "length", "angle", "angle", "angle"
, "angle"
, CNAMES = "dm_front", "dx_front", "dy_front", "dz_front", "amag_front"
, "ax_front", "ay_front", "az_front"
, RESULTS_NAME = bgs_torsion_bar_disp
, FUNCTION = USER(905, 1, 508, 526, 22, 526, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.velo_request'
REQUEST/168
, CUNITS = "velocity", "velocity", "velocity", "velocity", "angular_velocity"
, "angular_velocity", "angular_velocity", "angular_velocity"
, CNAMES = "vm_front", "vx_front", "vy_front", "vz_front", "wm_front"
, "wx_front", "wy_front", "wz_front"
, RESULTS_NAME = bgs_torsion_bar_velo
, FUNCTION = USER(905, 2, 508, 526, 22, 526, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!       adams_view_name='MDI_FRONT_STEERING.bgs_torsion_bar.force_request'
REQUEST/169
, CUNITS = "force", "force", "force", "force", "torque", "torque", "torque"
, "torque"
, CNAMES = "fm_front", "fx_front", "fy_front", "fz_front", "tm_front"
, "tx_front", "ty_front", "tz_front"
, RESULTS_NAME = bgs_torsion_bar_force
, FUNCTION = USER(905, 3, 508, 526, 22, 526, 1.0E-07)\
, ROUTINE = abgFDM::req905
!
!----------------------------- EXECUTION CONTROL -------------------------------
!
!Caches actuator states
!               adams_view_name='testrig.jml_bearing_lock.monitor'
SENSOR/1
, VALUE = 1
, GE
, ERROR = 0.01
, RETURN
, FUNCTION = USER(20)\
, ROUTINE = abgFDM::ActuatorMonitor
!
!Caches actuator states
!               adams_view_name='testrig.jmr_bearing_lock.monitor'
SENSOR/2
, VALUE = 1
, GE
, ERROR = 0.01
, RETURN
, FUNCTION = USER(21)\
, ROUTINE = abgFDM::ActuatorMonitor
!
!Caches actuator states
!                adams_view_name='testrig.jfl_jack_force.monitor'
SENSOR/3
, VALUE = 1
, GE
, ERROR = 0.01
, RETURN
, FUNCTION = USER(22)\
, ROUTINE = abgFDM::ActuatorMonitor
!
!Caches actuator states
!                adams_view_name='testrig.jfr_jack_force.monitor'
SENSOR/4
, VALUE = 1
, GE
, ERROR = 0.01
, RETURN
, FUNCTION = USER(23)\
, ROUTINE = abgFDM::ActuatorMonitor
!
!Caches actuator states
!              adams_view_name='testrig.jfs_steering_input.monitor'
SENSOR/9
, VALUE = 1
, GE
, ERROR = 0.01
, RETURN
, FUNCTION = USER(46)\
, ROUTINE = abgFDM::ActuatorMonitor
!
!------------------------- GRAVITATIONAL ACCELERATION --------------------------
!
ACCGRAV/
, KGRAV = -9806.65
!
!----------------------------- ANALYSIS SETTINGS -------------------------------
!
INTEGRATOR/
, GSTIFF
, ERROR = 0.01
, CORRECTOR = MODIFIED
!
OUTPUT/
, NOPRINT
!
RESULTS/
, FORMATTED
, FRICTION_SUMMARY
, XRF
, NODE_INCIDENTS
!
END
