IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Číslo projektu"
Time stamp: "2020-05-06T22:09:44"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200206_0915(x64) - Exporter 20.2.11.3 - Alternativní uživatelské rozhraní 20.2.11.3"
Application: "Autodesk Revit 2020 (CSY)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (CSY)"

People and organizations
  Person "petr.simanek88" of Organization (no name given)
  Owner history of Person "petr.simanek88" of Organization (no name given) | application "Autodesk Revit 2020 (CSY)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (CSY)" | change NOCHANGE | created 1588793234 (2020-05-06T19:27:14Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Číslo projektu" | long name "Název projektu" | phase "Stav projektu"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "UP" | long name "UP" | object type "Podlaží:8mm Head" | elevation 536.75
        contains 518 elements
          1 x IFCSLAB | type IFCSLABTYPE "Zakl.Pas_500x1000mm" | object type "Základový pas1:Zakl.Pas_500x1000mm" | FLOOR | names: "Základový pas1:Zakl.Pas_500x1000mm:383028" | material: "C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Zakl.Deska_250mm" | object type "Podlaha:Zakl.Deska_250mm" | FLOOR | names: "Podlaha:Zakl.Deska_250mm:383031" | material: layers "Podlaha:Zakl.Deska_250mm" ("C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" 0.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Základní stěna:ŽB.Stěna_200mm" | object type "Základní stěna:ŽB.Stěna_200mm" | names: "Základní stěna:ŽB.Stěna_200mm:383038", "Základní stěna:ŽB.Stěna_200mm:383039", "Základní stěna:ŽB.Stěna_200mm:383040" (+1 more) | material: layers "Základní stěna:ŽB.Stěna_200mm" ("C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "Základová deska:Podkl.beton_100mm" | object type "Základová deska:Podkl.beton_100mm" | BASESLAB | names: "Základová deska:Podkl.beton_100mm:383058" | material: layers "Základová deska:Podkl.beton_100mm" ("Beton prostý C12/15" 0.1) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Základová deska:Podkl.beton_100mm" | object type "Základová deska:Podkl.beton_100mm" | BASESLAB | names: "Základová deska:Podkl.beton_100mm:383081" | material: layers "Základová deska:Podkl.beton_100mm" ("Beton prostý C12/15" 0.1) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Dobetonávka 3.5%" | object type "Dobetonávka 3.5%1:Dobetonávka 3.5%" | FLOOR | names: "Dobetonávka 3.5%1:Dobetonávka 3.5%:383824" | material: "FLOORCRETE C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Spojná šachta" | object type "Spojná šachta:Spojná šachta" | names: "Spojná šachta:Spojná šachta:383865" | material: "C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Základová deska:Podkl.beton_100mm" | object type "Základová deska:Podkl.beton_100mm" | BASESLAB | names: "Základová deska:Podkl.beton_100mm:383898" | material: layers "Základová deska:Podkl.beton_100mm" ("Beton prostý C12/15" 0.1) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          504 x IFCREINFORCINGBAR | object type "Tyč výztuže:Structural Rebar 1" | names: "Tyč výztuže:Structural Rebar 1 : Tvar M_T1:384136: 1", "Tyč výztuže:Structural Rebar 1 : Tvar M_T1:384136: 2", "Tyč výztuže:Structural Rebar 1 : Tvar M_T1:384136: 3" (+501 more) | property sets: Pset_QuantityTakeOff, Pset_ReinforcingBarBendingsISOCD3766Common
          1 x IFCSITE | object type "Kačírek 1:Kačírek 1" | names: "Kačírek 1:Kačírek 1:384459" | material: "Štěrkopísek hutněný na Edef 0,45 MPa"
          1 x IFCSITE | object type "Kačírek2:Kačírek" | names: "Kačírek2:Kačírek:384499" | material: "Kačírek"
          1 x IFCSITE | object type "Kačírek3:Kačírek" | names: "Kačírek3:Kačírek:384531" | material: "Štěrkopísek hutněný na Edef 0,45 MPa"
      IFCBUILDINGSTOREY "Srovnávací hladina" | long name "Srovnávací hladina" | object type "Podlaží:8mm záhlaví" | elevation 538.
        contains 210 elements
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska_200mm" | object type "Podlaha:Deska_200mm" | FLOOR | names: "Podlaha:Deska_200mm:383043" | material: layers "Podlaha:Deska_200mm" ("FLOORCRETE C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Základní stěna:ŽB.Stěna_300mm" | object type "Základní stěna:ŽB.Stěna_300mm" | names: "Základní stěna:ŽB.Stěna_300mm:383092", "Základní stěna:ŽB.Stěna_300mm:383094", "Základní stěna:ŽB.Stěna_300mm:383096" (+1 more) | material: layers "Základní stěna:ŽB.Stěna_300mm" ("C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Základní stěna:Poro.Stěna_300mm" | object type "Základní stěna:Poro.Stěna_300mm" | names: "Základní stěna:Poro.Stěna_300mm:383104", "Základní stěna:Poro.Stěna_300mm:383105", "Základní stěna:Poro.Stěna_300mm:383106" (+3 more) | material: layers "Základní stěna:Poro.Stěna_300mm" ("POROTHERM 30 P+D" 0.3) | property sets: Pset_ConcreteElementGeneral, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1600x750mm" | object type "NBS_Okno-jeden panel:1600x750mm" | names: "NBS_Okno-jeden panel:1600x750mm:383116" | material: materials ("Polyamid 6,6 s 25 % skelných vláken", "Křemenné sklo") | property sets: Pset_DoorWindowGlazingType, Pset_ElementShading, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWINDOW | type IFCWINDOWSTYLE "1600x750mm" | object type "NBS_Okno-jeden panel:1600x750mm" | names: "NBS_Okno-jeden panel:1600x750mm:383117" | material: materials ("Polyamid 6,6 s 25 % skelných vláken", "Křemenné sklo") | property sets: Pset_DoorWindowGlazingType, Pset_ElementShading, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Porotherm KP 7 - 200 (zdivo tl.300 mm var.2)" | object type "Sestava prekladu Porotherm KP 7:Porotherm KP 7 - 200 (zdivo tl.300 mm var.2)" | names: "Sestava prekladu Porotherm KP 7:Porotherm KP 7 - 200 (zdivo tl.300 mm var.2):383118" | material: "XPS" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          2 x IFCBEAM | type IFCBEAMTYPE "PTH KP 7 - 200" | object type "Porotherm KP 7:PTH KP 7 - 200" | names: "Porotherm KP 7:PTH KP 7 - 200:383119", "Porotherm KP 7:PTH KP 7 - 200:383120" | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
          1 x IFCBEAM | type IFCBEAMTYPE "PTH KP 7 - 200" | object type "Porotherm KP 7:PTH KP 7 - 200" | names: "Porotherm KP 7:PTH KP 7 - 200:383121" | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Porotherm KP 7 - 200 (zdivo tl.300 mm var.2)" | object type "Sestava prekladu Porotherm KP 7:Porotherm KP 7 - 200 (zdivo tl.300 mm var.2)" | names: "Sestava prekladu Porotherm KP 7:Porotherm KP 7 - 200 (zdivo tl.300 mm var.2):383122", "Sestava prekladu Porotherm KP 7:Porotherm KP 7 - 200 (zdivo tl.300 mm var.2):383152" | material: "XPS" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
          4 x IFCBEAM | type IFCBEAMTYPE "PTH KP 7 - 200" | object type "Porotherm KP 7:PTH KP 7 - 200" | names: "Porotherm KP 7:PTH KP 7 - 200:383123", "Porotherm KP 7:PTH KP 7 - 200:383124", "Porotherm KP 7:PTH KP 7 - 200:383153" (+1 more) | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
          2 x IFCBEAM | type IFCBEAMTYPE "PTH KP 7 - 200" | object type "Porotherm KP 7:PTH KP 7 - 200" | names: "Porotherm KP 7:PTH KP 7 - 200:383125", "Porotherm KP 7:PTH KP 7 - 200:383155" | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
          1 x IFCDOOR | type IFCDOORSTYLE "1600x2100mm" | object type "Dveře, průchod, nerovnoměrné, hladké:1600x2100mm" | names: "Dveře, průchod, nerovnoměrné, hladké:1600x2100mm:383151" | material: materials ("Hliník1", "Kov, nátěr, šedý", "Polyamid 6,6 s 25 % skelných vláken") | property sets: Pset_DoorCommon, Pset_QuantityTakeOff
          8 x IFCBEAM | type IFCBEAMTYPE "I160" | object type "I:I160" | names: "I:I160:383189", "I:I160:383191", "I:I160:383193" (+5 more) | material: "Structural Steel - S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:383206" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCBEAM | type IFCBEAMTYPE "U200" | object type "U:U200" | names: "U:U200:383211", "U:U200:383213" | material: "Structural Steel - S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "160x180mm" | object type "M_Lepená konstrukce, dřevo sosny dlouhojehlé:160x180mm" | names: "M_Lepená konstrukce, dřevo sosny dlouhojehlé:160x180mm:383612", "M_Lepená konstrukce, dřevo sosny dlouhojehlé:160x180mm:383614" | material: "Dřevo 500 kg/m3" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          22 x IFCBEAM | type IFCBEAMTYPE "100x160mm" | object type "M_Lepená konstrukce, západní druhy:100x160mm" | names: "M_Lepená konstrukce, západní druhy:100x160mm:383616", "M_Lepená konstrukce, západní druhy:100x160mm:383618", "M_Lepená konstrukce, západní druhy:100x160mm:383624" (+19 more) | material: "Dřevo 500 kg/m3" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          14 x IFCBEAM | type IFCBEAMTYPE "80x160mm" | object type "M_Lepená konstrukce, západní druhy:80x160mm" | names: "M_Lepená konstrukce, západní druhy:80x160mm:383620", "M_Lepená konstrukce, západní druhy:80x160mm:383622", "M_Lepená konstrukce, západní druhy:80x160mm:383628" (+11 more) | material: "Dřevo 500 kg/m3" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCROOF | object type "Základní střecha:Wood Rafter 184mm - Asphalt Shingles" | names: "Základní střecha:Wood Rafter 184mm - Asphalt Shingles:383722" | parts: 2 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:383749" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:383758" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:383767" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:383776" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:383785" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "MDGTRAP" | object type "Window-Fixed-Marvin-Direct_Glaze_Trapezoid-Modern:MDGTRAP" | names: "Window-Fixed-Marvin-Direct_Glaze_Trapezoid-Modern:MDGTRAP:383797", "Window-Fixed-Marvin-Direct_Glaze_Trapezoid-Modern:MDGTRAP:383798" | material: materials ("Polyamid 6,6 s 25 % skelných vláken", "Křemenné sklo") | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_WindowCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:383802" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska_200mm" | object type "Podlaha:Deska_200mm" | FLOOR | names: "Podlaha:Deska_200mm:383827" | material: layers "Podlaha:Deska_200mm" ("FLOORCRETE C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          14 x IFCBEAM | type IFCBEAMTYPE "L75x50x8" | object type "Unequal L:L75x50x8" | names: "Unequal L:L75x50x8:383916", "Unequal L:L75x50x8:383918", "Unequal L:L75x50x8:383920" (+11 more) | material: "Ocel S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          16 x IFCBEAM | type IFCBEAMTYPE "U160" | object type "U:U160" | names: "U:U160:383924", "U:U160:383926", "U:U160:383928" (+13 more) | material: "Ocel S235" | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Svařovaný podstavec" | object type "Svařovaný podstavec6:Svařovaný podstavec" | names: "Svařovaný podstavec6:Svařovaný podstavec:384074" | material: "Ocel S235" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Svařovaný podstavec" | object type "Svařovaný podstavec7:Svařovaný podstavec" | names: "Svařovaný podstavec7:Svařovaný podstavec:384105" | material: "Ocel S235" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Schody" | object type "Schody:Schody" | names: "Schody:Schody:384123" | material: materials ("Steel, 43-355", "Dřevo 500 kg/m3") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | object type "Podlaha:Deska.Krov_60mm" | FLOOR | names: "Podlaha:Deska.Krov_60mm:384126" | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Základová deska:Podsyp" | object type "Základová deska:Podsyp" | BASESLAB | names: "Základová deska:Podsyp:384377" | material: layers "Základová deska:Podsyp" ("Štěrkopísek hutněný na Edef 0,45 MPa" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          8 x IFCROOF | object type "Základní střecha:Orsik 200mm" | names: "Základní střecha:Orsik 200mm:384651", "Základní střecha:Orsik 200mm:384661", "Základní střecha:Orsik 200mm:384671" (+5 more) | parts: 16 IFCSLAB | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "2300x600x2100" | object type "Rozvaděč panel:2300x600x2100" | names: "Rozvaděč panel:2300x600x2100:417509" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "3.9 LPS - 0.8 Meter Head" | object type "Turbína:3.9 LPS - 0.8 Meter Head" | names: "Turbína:3.9 LPS - 0.8 Meter Head:417510", "Turbína:3.9 LPS - 0.8 Meter Head:417511" | material: materials ("Steel", "Aluminum, Anodized Blue") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Three Phase - 480" | object type "Asynchroní generátor:Three Phase - 480" | names: "Asynchroní generátor:Three Phase - 480:417512", "Asynchroní generátor:Three Phase - 480:417513" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Kabelová lávka s tvarovkami:Channel Cable Tray" | object type "Kabelová lávka s tvarovkami:Channel Cable Tray" | names: "Kabelová lávka s tvarovkami:Channel Cable Tray:417515", "Kabelová lávka s tvarovkami:Channel Cable Tray:417516", "Kabelová lávka s tvarovkami:Channel Cable Tray:417518" | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "300mm Radius" | object type "M_Channel Horizontal Tee:300mm Radius" | names: "M_Channel Horizontal Tee:300mm Radius:417517" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          15 x IFCFLOWSEGMENT | type IFCCABLECARRIERSEGMENTTYPE "Elektroinstalační trubka s tvarovkami:Rigid Nonmetallic Conduit (RNC Sch 80)" | object type "Elektroinstalační trubka s tvarovkami:Rigid Nonmetallic Conduit (RNC Sch 80)" | names: "Elektroinstalační trubka s tvarovkami:Rigid Nonmetallic Conduit (RNC Sch 80):417519", "Elektroinstalační trubka s tvarovkami:Rigid Nonmetallic Conduit (RNC Sch 80):417523", "Elektroinstalační trubka s tvarovkami:Rigid Nonmetallic Conduit (RNC Sch 80):417527" (+12 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          11 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Standard" | object type "M_Conduit Elbow - without Fittings - RNC:Standard" | names: "M_Conduit Elbow - without Fittings - RNC:Standard:417521", "M_Conduit Elbow - without Fittings - RNC:Standard:417525", "M_Conduit Elbow - without Fittings - RNC:Standard:417531" (+8 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Reducer - Flanged - CS - Class 150:Standard" | names: "M_Reducer - Flanged - CS - Class 150:Standard:417543" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          21 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "Typy trubek:Default" | object type "Typy trubek:Default" | names: "Typy trubek:Default:417545", "Typy trubek:Default:417549", "Typy trubek:Default:417554" (+18 more) | property sets: Pset_DistributionFlowElementCommon, Pset_FlowSegmentDuctSegment, Pset_FlowSegmentPipeSegment, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "Tvarovka:Standard" | names: "Tvarovka:Standard:417547", "Tvarovka:Standard:417551" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Elbow - Flanged - CS - Class 150:Standard" | names: "M_Elbow - Flanged - CS - Class 150:Standard:417558", "M_Elbow - Flanged - CS - Class 150:Standard:417586", "M_Elbow - Flanged - CS - Class 150:Standard:417600" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Reducer - Flanged - CS - Class 150:Standard" | names: "M_Reducer - Flanged - CS - Class 150:Standard:417560" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Elbow - Flanged - CS - Class 150:Standard" | names: "M_Elbow - Flanged - CS - Class 150:Standard:417566", "M_Elbow - Flanged - CS - Class 150:Standard:417596" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Elbow - Flanged - CS - Class 150:Standard" | names: "M_Elbow - Flanged - CS - Class 150:Standard:417574" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Reducer - Flanged - CS - Class 150:Standard" | names: "M_Reducer - Flanged - CS - Class 150:Standard:417576" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Elbow - Flanged - CS - Class 150:Standard" | names: "M_Elbow - Flanged - CS - Class 150:Standard:417582", "M_Elbow - Flanged - CS - Class 150:Standard:417610" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Reducer - Flanged - CS - Class 150:Standard" | names: "M_Reducer - Flanged - CS - Class 150:Standard:417608" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Elbow - Flanged - CS - Class 150:Standard" | names: "M_Elbow - Flanged - CS - Class 150:Standard:417612" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Elbow - Flanged - CS - Class 150:Standard" | names: "M_Elbow - Flanged - CS - Class 150:Standard:417614" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Elbow - Flanged - CS - Class 150:Standard" | names: "M_Elbow - Flanged - CS - Class 150:Standard:417632" | property sets: Pset_DistributionFlowElementCommon, Pset_PipeConnectionFlanged, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Standard" | object type "M_Cap - Threaded - MI - Class 150:Standard" | names: "M_Cap - Threaded - MI - Class 150:Standard:417634" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          4 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Standard" | object type "M_Conduit Reducer Bushing - PVC:Standard" | names: "M_Conduit Reducer Bushing - PVC:Standard:417636", "M_Conduit Reducer Bushing - PVC:Standard:417637", "M_Conduit Reducer Bushing - PVC:Standard:417638" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          1 x IFCFLOWFITTING | type IFCCABLECARRIERFITTINGTYPE "Standard" | object type "M_Conduit Elbow - without Fittings - RMC:Standard" | names: "M_Conduit Elbow - without Fittings - RMC:Standard:417654" | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff
          2 x IFCRAILING | object type "Zábradlí:900mm Pipe" | names: "Zábradlí:900mm Pipe:383733", "Zábradlí:900mm Pipe:384167" | property sets: Pset_QuantityTakeOff, Pset_RailingCommon

Types
  IFCSLABTYPE "Zakl.Pas_500x1000mm" | FLOOR | 1 occurrence | material: "C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Podlaha:Zakl.Deska_250mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Zakl.Deska_250mm" ("C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" 0.25) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Základní stěna:ŽB.Stěna_200mm" | STANDARD | 4 occurrences | material: layers "Základní stěna:ŽB.Stěna_200mm" ("C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCSLABTYPE "Základová deska:Podkl.beton_100mm" | BASESLAB | 1 occurrence | material: layers "Základová deska:Podkl.beton_100mm" ("Beton prostý C12/15" 0.1) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Základová deska:Podkl.beton_100mm" | BASESLAB | 1 occurrence | material: layers "Základová deska:Podkl.beton_100mm" ("Beton prostý C12/15" 0.1) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Dobetonávka 3.5%" | FLOOR | 1 occurrence | material: "FLOORCRETE C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "Spojná šachta" | 1 occurrence | material: "C 25/30 - XC4, XA2, XD2, XM1, XF3 (F.1.2) - Cl 0,2 - Dmax22 - S4" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Základová deska:Podkl.beton_100mm" | BASESLAB | 1 occurrence | material: layers "Základová deska:Podkl.beton_100mm" ("Beton prostý C12/15" 0.1) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Podlaha:Deska_200mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska_200mm" ("FLOORCRETE C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWALLTYPE "Základní stěna:ŽB.Stěna_300mm" | STANDARD | 4 occurrences | material: layers "Základní stěna:ŽB.Stěna_300mm" ("C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Základní stěna:Poro.Stěna_300mm" | STANDARD | 6 occurrences | material: layers "Základní stěna:Poro.Stěna_300mm" ("POROTHERM 30 P+D" 0.3) | property sets: Pset_ConcreteElementGeneral, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWINDOWSTYLE "1600x750mm" | PLASTIC | SINGLE_PANEL | 1 occurrence | material: materials ("Polyamid 6,6 s 25 % skelných vláken", "Křemenné sklo") | property sets: NBS_Okno-jeden panel:1600x750mm:383116
  IFCWINDOWSTYLE "1600x750mm" | PLASTIC | SINGLE_PANEL | 1 occurrence | material: materials ("Polyamid 6,6 s 25 % skelných vláken", "Křemenné sklo") | property sets: NBS_Okno-jeden panel:1600x750mm:383117
  IFCBUILDINGELEMENTPROXYTYPE "Porotherm KP 7 - 200 (zdivo tl.300 mm var.2)" | 1 occurrence | material: "XPS" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBEAMTYPE "PTH KP 7 - 200" | BEAM | 2 occurrences | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
  IFCBEAMTYPE "PTH KP 7 - 200" | BEAM | 1 occurrence | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Porotherm KP 7 - 200 (zdivo tl.300 mm var.2)" | 2 occurrences | material: "XPS" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBEAMTYPE "PTH KP 7 - 200" | BEAM | 4 occurrences | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
  IFCBEAMTYPE "PTH KP 7 - 200" | BEAM | 2 occurrences | material: materials ("BT Beton C20/25", "BT Cihelná tvárnice") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_PrecastConcreteElementGeneral, Pset_QuantityTakeOff
  IFCDOORSTYLE "1600x2100mm" | 1 occurrence | material: materials ("Hliník1", "Kov, nátěr, šedý", "Polyamid 6,6 s 25 % skelných vláken") | property sets: Dveře, průchod, nerovnoměrné, hladké:1600x2100mm:383151
  IFCBEAMTYPE "I160" | BEAM | 8 occurrences | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBEAMTYPE "U200" | BEAM | 2 occurrences | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "160x180mm" | BEAM | 2 occurrences | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "100x160mm" | BEAM | 22 occurrences | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "80x160mm" | BEAM | 14 occurrences | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCWINDOWSTYLE "MDGTRAP" | 2 occurrences | material: materials ("Polyamid 6,6 s 25 % skelných vláken", "Křemenné sklo") | property sets: Window-Fixed-Marvin-Direct_Glaze_Trapezoid-Modern:MDGTRAP:383797
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Podlaha:Deska_200mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska_200mm" ("FLOORCRETE C 25/30 - XC2 - Cl 0,2 - Dmax22 - S4" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBEAMTYPE "L75x50x8" | BEAM | 14 occurrences | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCBEAMTYPE "U160" | BEAM | 16 occurrences | property sets: Pset_BeamCommon, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfBeam
  IFCBUILDINGELEMENTPROXYTYPE "Svařovaný podstavec" | 1 occurrence | material: "Ocel S235" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Svařovaný podstavec" | 1 occurrence | material: "Ocel S235" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Schody" | 1 occurrence | material: materials ("Steel, 43-355", "Dřevo 500 kg/m3") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCSLABTYPE "Podlaha:Deska.Krov_60mm" | FLOOR | 1 occurrence | material: layers "Podlaha:Deska.Krov_60mm" ("Dřevo 500 kg/m3" 0.06) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCSLABTYPE "Základová deska:Podsyp" | BASESLAB | 1 occurrence | material: layers "Základová deska:Podsyp" ("Štěrkopísek hutněný na Edef 0,45 MPa" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "2300x600x2100" | 1 occurrence | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "3.9 LPS - 0.8 Meter Head" | 2 occurrences | material: materials ("Steel", "Aluminum, Anodized Blue") | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Three Phase - 480" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
  IFCCABLECARRIERSEGMENTTYPE "Kabelová lávka s tvarovkami:Channel Cable Tray" | 3 occurrences
  IFCCABLECARRIERFITTINGTYPE "300mm Radius" | 1 occurrence
  IFCCABLECARRIERSEGMENTTYPE "Elektroinstalační trubka s tvarovkami:Rigid Nonmetallic Conduit (RNC Sch 80)" | 15 occurrences
  IFCCABLECARRIERFITTINGTYPE "Standard" | 11 occurrences
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPESEGMENTTYPE "Typy trubek:Default" | 21 occurrences
  IFCPIPEFITTINGTYPE "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | 4 occurrences
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | 2 occurrences
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCPIPEFITTINGTYPE "Standard" | 1 occurrence
  IFCCABLECARRIERFITTINGTYPE "Standard" | 4 occurrences
  IFCCABLECARRIERFITTINGTYPE "Standard" | 1 occurrence

Property sets
  Pset_QuantityTakeOff | properties | on 504 objects (504 IFCREINFORCINGBAR)
    Reference = "Structural Rebar 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 35 objects (35 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 24 objects (16 IFCSLAB, 8 IFCROOF)
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 22 objects (22 IFCBEAM) | on 1 type object
    Reference = "100x160mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 21 objects (21 IFCFLOWSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 16 objects (16 IFCBEAM) | on 1 type object
    Reference = "U160" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 15 objects (15 IFCFLOWSEGMENT)
    Reference = "Rigid Nonmetallic Conduit (RNC Sch 80)" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 14 objects (14 IFCBEAM) | on 1 type object
    Reference = "80x160mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 29 more contents on 105 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 16 objects (16 IFCSLAB)
    Reference = "Orsik 200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 8 objects (8 IFCSLAB) | on 8 type objects
    Reference = "Deska.Krov_60mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 3 objects (3 IFCSLAB) | on 3 type objects
    Reference = "Podkl.beton_100mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB) | on 2 type objects
    Reference = "Deska_200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 2 objects (2 IFCSLAB)
    Reference = "Wood Rafter 184mm - Asphalt Shingles" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Zakl.Pas_500x1000mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Zakl.Deska_250mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Reference = "Dobetonávka 3.5%" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab: 1 more content on 1 objects not shown
  Pset_SlabCommon | properties | on 10 objects (10 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 38.9600000000042 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.189308296608546 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Deska.Krov_60mm" (IFCIDENTIFIER)
    ThermalTransmittance = 2.16666666666667 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 38.9600000000026 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.189308296608546 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Podkl.beton_100mm" (IFCIDENTIFIER)
    ThermalTransmittance = 17. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Deska_200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 6.8 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 38.9600000000042 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Wood Rafter 184mm - Asphalt Shingles" (IFCIDENTIFIER)
    ThermalTransmittance = 5.41505208691598 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Zakl.Pas_500x1000mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Zakl.Deska_250mm" (IFCIDENTIFIER)
    ThermalTransmittance = 5.72 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon: 9 more contents on 2 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 6 objects (6 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Poro.Stěna_300mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "ŽB.Stěna_200mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 4 objects (4 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "ŽB.Stěna_300mm" (IFCLABEL)
  Pset_WallCommon | properties | on 6 objects (6 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating (no value)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Poro.Stěna_300mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.833333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 4 objects (4 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ŽB.Stěna_300mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.53333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 3 objects (3 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ŽB.Stěna_200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 7.15 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ŽB.Stěna_200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 7.15 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ŽB.Stěna_200mm" (IFCIDENTIFIER)
    ThermalTransmittance = 7.15 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ŽB.Stěna_300mm" (IFCIDENTIFIER)
    ThermalTransmittance = 4.53333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    FireRating (no value)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Poro.Stěna_300mm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.833333333333333 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_OpeningElementCommon | properties | on 6 objects (6 IFCOPENINGELEMENT)
    Reference = "Poro.Stěna_300mm" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 5 objects (5 IFCOPENINGELEMENT)
    Reference = "ŽB.Stěna_300mm" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 2 objects (2 IFCOPENINGELEMENT)
    Reference = "Deska_200mm" (IFCIDENTIFIER)
  Pset_ConcreteElementGeneral | properties | on 9 objects (9 IFCBEAM) | on 4 type objects
    FireRating = "R 60 DP1" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 6 objects (6 IFCWALLSTANDARDCASE) | on 1 type object
    FireRating (no value)
  Pset_ManufacturerTypeInformation | properties | on 15 objects (6 IFCOPENINGELEMENT, 6 IFCWALLSTANDARDCASE, 3 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Manufacturer = "Wienerberger" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 9 objects (9 IFCBEAM) | on 4 type objects
    ArticleNumber (no value)
    Manufacturer = "Wienerberger" (IFCLABEL)
    ModelLabel (no value)
    ModelReference (no value)
    ProductionYear (no value)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCWINDOW)
    Manufacturer = "deceuninck.ltd@deceuninck.com" (IFCLABEL)
    ModelReference = "Fully Reversible Window FRW1" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCWINDOW)
    Manufacturer = "Marvin Windows and Doors" (IFCLABEL)
  Pset_DoorWindowGlazingType | properties | on 2 objects (2 IFCWINDOW)
    BeamRadiationTransmittance = 0. (IFCPOSITIVERATIOMEASURE)
    FillGas = "Argon" (IFCLABEL)
    GlassLayers = 2. (IFCCOUNTMEASURE)
    GlassThickness1 = 0.00400000000608 (IFCPOSITIVELENGTHMEASURE) [METRE]
    GlassThickness2 = 0.00400000000608 (IFCPOSITIVELENGTHMEASURE) [METRE]
    IsCoated = TRUE (IFCBOOLEAN)
    IsLaminated = FALSE (IFCBOOLEAN)
    IsTempered = FALSE (IFCBOOLEAN)
    IsWired = FALSE (IFCBOOLEAN)
    Reflectivity = 0. (IFCPOSITIVERATIOMEASURE)
    SolarHeatGainTransmittance = 0. (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittanceSummer = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    ThermalTransmittanceWinter = 0. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Translucency = 0. (IFCPOSITIVERATIOMEASURE)
  Pset_ElementShading | properties | on 2 objects (2 IFCWINDOW)
    Color = "n/a" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 9 objects (9 IFCBEAM) | on 4 type objects
    BarCode (no value)
    BatchReference (no value)
    SerialNumber (no value)
  Pset_ManufacturerOccurrence | properties | on 2 objects (2 IFCWINDOW)
    BarCode = "n/a" (IFCIDENTIFIER)
    SerialNumber = "n/a" (IFCIDENTIFIER)
  Pset_ProductRequirements | properties | on 2 objects (2 IFCWINDOW)
    Category = "Pr_30_59_98_92:Unplasticized polyvinylchloride (PVC-U) window units" (IFCLABEL)
    Name = "PVCUWindowUnits_FullyReversibleWindow_FRW1-1000x1000mm-DoubleGlazed_DeceuninckLtd" (IFCLABEL)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    AcousticRating = "32-43 dB" (IFCLABEL)
    FireRating = "n/a" (IFCLABEL)
    GlazingAreaFraction = 0. (IFCPOSITIVERATIOMEASURE)
    Infiltration = 0.02 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCIDENTIFIER)
    SecurityRating = "PAS 24" (IFCLABEL)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0.96 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "MDGTRAP" (IFCIDENTIFIER)
    ThermalTransmittance = 6.2426 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Porotherm KP 7 - 200 (zdivo tl.300 mm var.2)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "Svařovaný podstavec" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "3.9 LPS - 0.8 Meter Head" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Three Phase - 480" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Spojná šachta" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "Schody" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "2300x600x2100" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 14 objects (14 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "80x160mm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.15548640054056 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 11 objects (11 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "100x160mm" (IFCIDENTIFIER)
    Slope = 38.9565582806457 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4.3722992806985 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 11 objects (11 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "100x160mm" (IFCIDENTIFIER)
    Slope = 38.9565582806456 (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4.37229928069851 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 9 objects (9 IFCBEAM)
    FireRating = "R 60 DP1" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "PTH KP 7 - 200" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.6 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "I160" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5.6 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "U160" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 0.77 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 5 objects (5 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "L75x50x8" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 0.6768 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "L75x50x8" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 0.752 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_BeamCommon: 17 more contents on 19 objects not shown
  Pset_PrecastConcreteElementGeneral | properties | on 9 objects (9 IFCBEAM) | on 4 type objects
    SerialNumber (no value)
  Pset_ReinforcementBarPitchOfBeam | properties | on 22 objects (22 IFCBEAM) | on 1 type object
    Reference = "100x160mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 16 objects (16 IFCBEAM) | on 1 type object
    Reference = "U160" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 14 objects (14 IFCBEAM) | on 1 type object
    Reference = "80x160mm" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 14 objects (14 IFCBEAM) | on 1 type object
    Reference = "L75x50x8" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 9 objects (9 IFCBEAM) | on 4 type objects
    Reference = "PTH KP 7 - 200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 8 objects (8 IFCBEAM) | on 1 type object
    Reference = "I160" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM) | on 1 type object
    Reference = "U200" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 2 objects (2 IFCBEAM) | on 1 type object
    Reference = "160x180mm" (IFCLABEL)
  Pset_Warranty | properties | on 9 objects (9 IFCBEAM) | on 4 type objects
    Exclusions (no value)
    IsExtendedWarranty = TRUE (IFCBOOLEAN)
    WarrantyContent (no value)
    WarrantyIdentifier (no value)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1600x2100mm" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 64.9400000000017 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Wood Rafter 184mm - Asphalt Shingles" (IFCIDENTIFIER)
    TotalArea = 83.5149725524995 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.18750000000031 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    TotalArea = 5.38526251252867 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.1875000000002 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    TotalArea = 5.38526251252841 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.18750000000031 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    TotalArea = 5.38526251252848 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.1875000000001 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    TotalArea = 5.38526251252832 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.18750000000005 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    TotalArea = 5.3852625125282 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.18749999999991 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    TotalArea = 5.38526251252812 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 4.18750000000029 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Orsik 200mm" (IFCIDENTIFIER)
    TotalArea = 5.38526251252848 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_RoofCommon: 1 more content on 1 objects not shown
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 53 objects (53 IFCREINFORCINGBAR)
    ISOCD3766BendingEndHook = 135. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    ISOCD3766BendingStartHook = 135. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    ISOCD3766ShapeCode = "M_T1" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.025 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_a = 0.0956858347057703 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 0.8 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_c = 0.450000000000096 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_d = 0.8 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_e = 0.450000000000096 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 42 objects (42 IFCREINFORCINGBAR)
    ISOCD3766BendingEndHook = 135. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    ISOCD3766BendingStartHook = 135. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    ISOCD3766ShapeCode = "M_T1" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.025 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_a = 0.0956858347057703 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 0.800000000000001 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_c = 0.449999999999958 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_d = 0.8 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_e = 0.449999999999957 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 38 objects (38 IFCREINFORCINGBAR)
    ISOCD3766ShapeCode = "M_00" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.04 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 1. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 37 objects (37 IFCREINFORCINGBAR)
    ISOCD3766ShapeCode = "M_00" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.04 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 2.63229440155605 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 35 objects (35 IFCREINFORCINGBAR)
    ISOCD3766ShapeCode = "M_00" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.04 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 2.64444565585347 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 34 objects (34 IFCREINFORCINGBAR)
    ISOCD3766ShapeCode = "M_00" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.04 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 2.26729750300485 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 33 objects (33 IFCREINFORCINGBAR)
    ISOCD3766ShapeCode = "M_00" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.04 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 2.25356136172147 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common | properties | on 30 objects (30 IFCREINFORCINGBAR)
    ISOCD3766ShapeCode = "M_00" (IFCLABEL)
    ISOCD3766ShapeParameter_R = 0.04 (IFCPOSITIVELENGTHMEASURE) [METRE]
    ISOCD3766ShapeParameter_b = 4.95000000000019 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_ReinforcingBarBendingsISOCD3766Common: 37 more contents on 202 objects not shown
  Pset_DistributionFlowElementCommon | properties | on 35 objects (35 IFCFLOWFITTING)
    Reference = "Standard" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 21 objects (21 IFCFLOWSEGMENT)
    Reference = "Default" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 15 objects (15 IFCFLOWSEGMENT)
    Reference = "Rigid Nonmetallic Conduit (RNC Sch 80)" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Reference = "Channel Cable Tray" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "300mm Radius" (IFCIDENTIFIER)
  Pset_FlowSegmentDuctSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 0.149999999999931 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 0.721001196802416 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 0.799665196802412 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 3.09663922640134 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 0.632101196802393 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 1.55318154361921 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 1.6786814257128 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 0.721001196802346 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment: 27 more contents on 27 objects not shown
  Pset_FlowSegmentPipeSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 0.149999999999931 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 0.721001196802416 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 0.799665196802412 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 3.09663922640134 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 0.632101196802393 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 1.55318154361921 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 1.6786814257128 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 0.721001196802346 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment: 27 more contents on 27 objects not shown
  Pset_PipeConnectionFlanged | properties | on 11 objects (11 IFCFLOWFITTING)
    FlangeThickness = 0.027 (IFCLENGTHMEASURE) [METRE]
  Pset_PipeConnectionFlanged | properties | on 2 objects (2 IFCFLOWFITTING)
    FlangeDiameter = 0.775 (IFCLENGTHMEASURE) [METRE]
    FlangeThickness = 0.0635 (IFCLENGTHMEASURE) [METRE]
  Pset_PipeConnectionFlanged | properties | on 1 object (1 IFCFLOWFITTING)
    FlangeThickness = 0.0413 (IFCLENGTHMEASURE) [METRE]
  Pset_RailingCommon | properties | on 2 objects (2 IFCRAILING)
    Height = 0.9 (IFCPOSITIVELENGTHMEASURE) [METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "900mm Pipe" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 2 (IFCINTEGER)
  NBS_Okno-jeden panel:1600x750mm:383116 | predefined | on 1 type object
  NBS_Okno-jeden panel:1600x750mm:383117 | predefined | on 1 type object
  Dveře, průchod, nerovnoměrné, hladké:1600x2100mm:383151 | predefined | on 2 type objects
  Window-Fixed-Marvin-Direct_Glaze_Trapezoid-Modern:MDGTRAP:383797 | predefined | on 1 type object

Other addresses and roles
  2 x postal address: "Zde zadejte adresu"