IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2016-11-22T17:27:03"
Author: "Daniel Šabart"
Author: "daniel.sabart@seznam.cz"
Organization: "ČVUT v Praze"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Authorization: "student"
Application: "Autodesk Revit 2017 (CSY)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (CSY)"

People and organizations
  Person "sabardan@fsv.cvut.cz" (telecom address: e-mail "daniel.sabart@seznam.cz") of Organization (no name given)
  Owner history of Person "sabardan@fsv.cvut.cz" (telecom address: e-mail "daniel.sabart@seznam.cz") of Organization (no name given) | application "Autodesk Revit 2017 (CSY)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (CSY)" | change NOCHANGE | created 1477340442 (2016-10-24T20:20:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Projekt A" | phase "Stav projektu"
  IFCSITE "Default" | latitude 50° 5′ 59.994506″ | longitude 14° 29′ 59.999999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Zde zadejte adresu", "Praha", "Česká republika"
      IFCBUILDINGSTOREY "Podlaží 2" | long name "Podlaží 2" | elevation 2800.
        contains 16 elements
          16 x IFCBEAM | object type "UB univerzální nosníky:UB305x165x40:61397" | names: "UB univerzální nosníky:UB305x165x40:389427", "UB univerzální nosníky:UB305x165x40:389430", "UB univerzální nosníky:UB305x165x40:389433" (+13 more) | material: "Kov, ocel 43-275" | property sets: Pset_BeamCommon

Property sets
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_BeamCommon | properties | on 16 objects (16 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "UB305x165x40" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 5551. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)